13	003
	Prefabricated concrete column
14	003
	Concrete
3	003
	-reinforcement: refer to working drawings
	rubble masonry: tied to the reinforced concrete backup wall with non-corrosive ties
	pointing kept back of face
1	004
	-with 3/8" mortar joints
10	004
	-story height studs
	2x4 sole plate and double top plate
	subfloor extends to outer edge of frame
	brick veneer with 3/8" weathered mortar joints
11	004
	-common brick column
2	004
	-with 3/8" weathered mortar joints
21	004
	-laid flat in 1/3" mortar bed
	with 3/8" mortar joints
22	004
	-laid on edge in 1/3" mortar bed
	with 3/8" mortar joints
4	004
	-block with 3/8" mortar joints in running bond
5	004
	-brick with 3/8" mortar joints
6	004
	-brick with 3/8" mortar joints
	3 coat plaster, 5/8" thick total
	metal ties every 6th course
	face brick with weathered mortar joints
7	004
	-brick with 3/8" mortar joints
	steel reinforcement: refer to working drawings and reinforcement notes
8	004
	-brick with 3/8" mortar joints
	3 coat plaster, 5/8" thick total
	metal ties every 6th course
9	004
	-story height studs
	2x4 sole plate and double top plate
	subfloor extends to outer edge of frame
16	005
	* Steel floor deck *
15	006
	* Wood joist flat roof *
	white gravel surface
	5 ply roofing
	joists 16" o.c.
	4x10 double header at edges
17	006
	* Wood joist floor *
	joists 16" o.c.
	4x10 double header at edges
12	009
	Gypsum Firecode Veneer
18	009
	* Asphalt shingle+concrete plank roof *
19	009
	* Tile+wood joist and rafters *
	joists 16" o.c.
23	009
	-4 1/4"x4 1/4" glazed tiles, 5/16" thick
	laid with thin set mortar
	plywood subfloor protected with water proofing
24	009
	-9"x9" quarry tiles, 1/2" thick
	laid with thin set mortar
	plywood subfloor protected with water proofing
25	009
	-4x4" square + octogonal tiles, 1/2" thick
	laid with thin set mortar
	plywood subfloor protected with water proofing
26	009
	-hexagonal tiles, 4" edges, 1/2" thick
	laid with thin set mortar
	plywood subfloor protected with water proofing
27	009
	-nailed to plywood subfloor
28	009
	-applied to plywood subfloor with blind nailing
