013	0100
	AWNING	
	
014	0100
	FIXED	
	
015	0100
	CASEMENT	
	
016	0100
	REVERSIBLE	
	
017	0100
	PROJECTED	
	
018	0100
	SLIDING	
	
019	0100
	SINGLE HUNG	
	
020	0100
	DOUBLE HUNG	
	
021	0100
	SECURITY	
	
022	0100
	COMBINATION	
	
023	0100
	JALOUSIE	
	
024	0100
	PIVOTED	
	
025	0200
	FLUSH	
	
026	0200
	VISION	
	
027	0200
	GLASS	
	
028	0200
	NARROW LITE	
	
029	0200
	GLASS/LOUVERED	
	
030	0200
	DECORATIVE	
	
031	0200
	DUTCH	
	
032	0200
	WIRED GLASS	
	
033	0200
	GARAGE	
	
009	0300
	PAINT	
	
011	0300
	STAINED	
	
012	0300
	ANODIZED	
	
005	0400
	STEEL	
	
006	0400
	ALU	
	
007	0400
	VINYL	
	
008	0400
	WOOD	
	
001	0500
	DBL.	
	
002	0500
	SINGLE	
	
003	0500
	TRIPLE	
	
004	0500
	SECURITY	
	
010	0500
	WIRED GLASS	
	
01000	E-WF.01
	Prepare plans to include foundation plans, floor plans, elevations and sections, as required. Includes on site inspection and measurement by designer.	
	
01006	E-WF.01
	Design service including the preparations of the plans and specifications for a one story home.   Plans include site, foundation, floor, elevations and sections as required. Contractor and the owner will participate in a pre-construction conference to approve existing conditions, make product selections and approve the plans. The designer will supervise the work during construction and be responsible for the approval of payments to the contractor.	
	
01007	E-WF.01
	Design service including the preparations of the plans and specifications for a two story home.   Plans include site, foundation, floor, elevations and sections as required. Contractor and the owner will participate in a pre-construction conference to approve existing conditions, make product selections and approve the plans. The designer will supervise the work during construction and be responsible for the approval of payments to the contractor.	
	
01008	E-WF.01
	Design service including the preparations of the plans and specifications for a two and one half story home.   Plans include site, foundation, floor, elevations and sections as required. Contractor and the owner will participate in a pre-construction conference to approve existing conditions, make product selections and approve the plans. The designer will supervise the work during construction and be responsible for the approval of payments to the contractor.	
	
01009	E-WF.01
	The contractor will provide the building permit contingent upon plan compliance with the local building official.  Set up costs.	
	
01010	E-WF.01
	The contractor will provide the building permit contingent upon plan compliance with the local building official.  Cost based on job size.	
	
01850	E-WF.01
	Design service including the preparations of the plans and specifications. Plans include site, foundation, floor, elevations and sections as required. Contractor and the owner will participate in a pre-construction conference to approve existing conditions, make product selections and approve the plans.	
	
02011	E-WF.01
	Preparation of survey by engineer before construction for the location of house corners and the property boundaries.	
	
04004	E-WF.01
	Percolation test to determine if a septic system permit will be issued by the building officials.	
	
04100	E-WF.02
	Unless otherwise noted within this proposal the following conditions prevail for this proposal.  The building permit will be obtained, but the permit fee and any other required fees such as tap or impact fees will be billed to owner.  All surveys desired or required will be billed at cost to owner.  Plans or architectural services are the responsibility of the owner unless included in this proposal.  The owner certifies the site to be an acceptable building location and free of any environmental hazards.  Contractor will install temporary electrical service.  Batter boards for house location will be installed by the contractor from the house location survey.   Trench for concrete footings will be at least 36" below grade.  Footing grade stakes will be placed in footing trench and concrete will be poured to that grade.  Pour 2500# (5sack) concrete mix into footings and backfill after footing has setup.  Pour continuously, take American Concrete Institute ( ACI) recommended weather precautions as needed.  Footing depth as required by building official.  Site clean up and rubbish removal is the responsibility of the contractor.	
	
04110	E-WF.02
	Put full basement under living area with concrete foundation walls.  Set up pre-built 2' x 8' sectional forms in existing excavation.  Pour concrete foundation wall 6 inches thick. Includes cutouts for beams, vents, windows etc. Fill the forms with 2500 # concrete mix poured by chute from transit mix truck. Clean and strip forms. Pour continuously, take ACI recommended weather precautions as needed.  This takes into consideration that the basic shell includes costs for the footers.  Excavation to desired grade to be added to this proposal.	
	
04111	E-WF.02
	Put full basement under living area with block foundation walls.  Block walls laid on footing. Lay up walls plumb and true with courses level.  Lay in bond pattern with metal ladder type reinforcing every other course.  Cutouts inserted as required for beams, windows and doorways. Top course to be 4" solid cap blocks.  Blocks to be 8x8x16.  All joints to be tooled and steel angles installed as needed.  Bucks as required are to be tied into wall and shall be plumb and true.  Wall to be only up to 8 feet above footing with scaffolding as required.   Take ACI recommended weather precautions as needed.  This takes into consideration that the basic shell includes costs for the footers.   Excavation to desired grade to be added to this proposal.	
	
04113	E-WF.02
	Slab at first floor grade under living area abutting continuous concrete footings and foundation wall.  Pour 4" concrete floor over compacted gravel base with vapor barrier.   Back fill from excavation spoils and rough grade.  Slab will also be 2500# concrete with 6x6x10 wire mesh reinforcement with spread footers as required.  Pour continuously, take ACI recommended weather precautions as needed.  Trowel to a smooth finish.	
	
04114	E-WF.02
	Wood floor system to be installed on continuous masonry foundation footers and wall.  The system may be either structural lumber or engineered wood with plywood subfloor.  All structural lumber will be used to full length permissible under applicable building code. Joists to be nailed 16" oc.  Floor trusses or engineered lumber will be nailed 24" oc and installed according to manufacturers specifications.  Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Floor system will be fastened to a bolted mud sill with bridging at least every 8'. Solid perimeter banding with headers and hangers as required.	
	
04120	E-WF.02
	Construct an interior/exterior bearing wall of 2x4's eight feet high nailed 16" OC with a sole plate and two cap plates.  Headers as required may be solid or laminated and sized to code.  Anchor bolts, beam(s)and steel support column(s) as required. Mudsill to be approved treated lumber.  Floor joists to be sized and placed as required by building official.  Subfloor to be 5/8" plywood nailed and glued.   Exterior walls will be sheathed with plywood corners and foil faced insulation board for the balance of the walls.  Roof framing to be trusses 24" OC with 1/2 " CDX plywood with a 18" overhang.  Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
05400	E-WF.02
	Build a one story ranch shell on continuous masonry foundation under living area according to general specifications.   Roofing to be 240# fiberglass shingles over 15# felt with aluminum flashing.  Gutters and downspouts to be aluminum with all exterior wood trim to be tight knot pine, fir or spruce.  Soffits maybe ACX plywood.  Siding to be 1/2"x8" beveled cedar. Included are two solid core exterior doors with hardware and lock sets.  A builder grade insulated wood double hung window will be installed for every 120 sq. ft of living area.  Basic charge for shell living space, any ells, wings, garage, basement, and floor systems are to be added to this item.  Exterior improvements, such as stoops, decks, driveways, aprons, sitework and landscaping, as required by owner, are shown if they are part of the proposal.  ITEMS NOT SHOWN IN THIS DOCUMENT ARE NOT INCLUDED.	
	
05401	E-WF.02
	Square footage charge associated with the living area for a one story ranch type shell, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
05402	E-WF.02
	Square footage charge associated with the living area for a one story ranch type shell with wing, to be added to the basic shell.  Wing to be gable style with full valley roof tie in to basic shell.  A builder grade insulated wood double hung window will be installed for every 120 sq. ft of living area.  On footing and slab unless a basement is shown later in this document.	
	
05403	E-WF.02
	Square footage associated with the garage area for a single story ranch type shell.  Garage to be built on continuous masonry foundation with 6" concrete slab floor.  Slab will be 2500# concrete with 6x6x10 wire mesh reinforcement with spread footers as required.  Pour continuously, take ACI recommended weather precautions as needed.  Trowel to a smooth finish.  One builder grade wood double hung insulated for every 130 sq. ft of garage area.  Additional trim and finish items may be added to the basic garage shell.	
	
05410	E-WF.02
	Build a one story Santa Fe style shell on continuous masonry foundation under living area according to general specifications.  Form and pour a concrete slab. Roofing to be concrete roofing tiles over 30lb felt with aluminum flashing.  Gutters and downspouts to be aluminum with all exterior wood trim to be tight pine, fir or spruce.  Soffits maybe ACX plywood.  Siding to be stucco mesh and 3 coats of stucco on exterior walls. Included are two solid core exterior doors with hardware and lock sets.  Insulated builder grade sliding windows will be installed for ever 100 SF of living area. Basic charge for shell, living space, ells or wings, garage, and basement, if any are to be added to this item.  Exterior improvements, such as stoops, decks, driveways, aprons, site work and landscaping, as required by owner, are shown if they are part of the proposal.  ITEMS NOT SHOWN IN THIS DOCUMENT ARE NOT INCLUDED.	
	
05411	E-WF.02
	Square footage associated with the living area for the single story Santa Fe style shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
05412	E-WF.02
	Square footage charge associated with the living area for a one story Santa Fe type shell with wing, to be added to the basic shell.  Wing to be gable style with full valley roof tie in to basic shell.  A builder grade insulated wood double hung window will be installed for every 120 sq. ft of living area.  	
	
05413	E-WF.02
	Square footage associated with the garage area for a single story Santa Fe type shell.  Garage to be built on continuous masonry foundation with 6" concrete slab floor.  Slab will be 2500# concrete with 6x6x10 wire mesh reinforcement with spread footers as required.  Pour continuously, take ACI recommended weather precautions as needed.  Trowel to a smooth Finish.  One builder grade wood double hung insulated for every 130 sq. ft of garage area.  Additional trim and finish items may be added to the basic garage shell.	
	
05420	E-WF.02
	Build a two story Santa Fe style shell on continuous masonry foundation under living area according to general specifications.  Form and pour a concrete slab. Roofing to be concrete roofing tiles over 30lb felt with aluminum flashing.  Gutters and downspouts to be aluminum with all exterior wood trim to be tight pine, fir or spruce.  Soffits maybe ACX plywood.  Siding to be stucco mesh and 3 coats of stucco on exterior walls. Included are two solid core exterior doors with hardware and lock sets.  Insulated builder grade sliding windows will be installed for ever 100 SF of living area. Basic charge for shell, living space, ells or wings, garage, and basement, if any are to be added to this item.  Exterior improvements, such as stoops, decks, driveways, aprons, site work and landscaping, as required by owner, are shown if they are part of the proposal.  ITEMS NOT SHOWN IN THIS DOCUMENT ARE NOT INCLUDED.	
	
05421	E-WF.02
	Square footage associated with the living area for the two story Santa Fe type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
05422	E-WF.02
	Square footage charge associated with the living area for a  Santa Fe type shell with wing, to be added to the basic shell.  Wing to be gable style with full valley roof tie in to basic shell.  A builder grade insulated wood double hung window will be installed for every 120 sq. ft of living area.  	
	
05423	E-WF.02
	Square footage associated with the garage area for the two story Santa Fe type shell that is described above to be added to the basic shell.  Additional trim and finish items may be added to the basic garage shell.	
	
05450	E-WF.02
	Build a one story Provincial  shell on continuous masonry foundation under living area according to general specifications.  Roofing to be 240# fiberglass shingles over 15# felt with aluminum flashing.  Gutters and downspouts to be aluminum with all exterior wood trim to be tight knot pine, fir or spruce.  Soffits maybe ACX plywood.  Siding to be 1/2"x8" beveled cedar. Included are two solid core exterior doors with hardware and locksets.  A builder grade wood double hung insulated window will be installed for every 120 SF of living area as well as two for the garage.   Basic charge for shell, living space, ells or wings, garage, and basement, if any are to be added to this item.  Exterior improvements, such as stoops, decks, driveways, aprons, sitework and landscaping, as required by owner, are shown if they are part of the proposal.  ITEMS NOT SHOWN IN THIS DOCUMENT ARE NOT INCLUDED.	
	
05451	E-WF.02
	Square footage associated with the living area for the single story provincial type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
05452	E-WF.02
	Square footage associated with the living area for the single story Provincial type shell with a wing, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.   Wing to be a hip style roof with full valley roof tie in to basic shell.  A builder grade insulated wood double hung window will be installed for every 120 sq. ft of living area.  On footing and slab unless a basement is shown later in this document.	
	
05453	E-WF.02
	Square footage associated with the garage area for the single story provincial type shell garage.  One builder grade wood double hung insulated for every 130 sq. ft of garage area.   Additional trim and finish items may be added to the basic garage shell.	
	
06500	E-WF.02
	Build a one and a half story Salt Box shell on continuous masonry foundation under living area according to general specifications.   Roof framing includes shed dormer in rear. Roofing to be 240# fiberglass shingles over 15# felt with aluminum flashing.  Gutters and downspouts to be aluminum with all exterior wood trim to be tight knot pine, fir or spruce.   Siding to be 1/2"x8" beveled cedar. Included are two solid core exterior doors with hardware and locksets.  A builder grade wood double hung window will be installed for ever 100 SF of living area as well as two for the garage.   Basic charge for shell, living space, ells or wings, garage, and basement, if any are to be added to this item.  Exterior improvements, such as stoops, decks, driveways, aprons, site work and landscaping, as required by owner, are shown if they are part of the proposal.  ITEMS NOT SHOWN IN THIS DOCUMENT ARE NOT INCLUDED.	
	
06501	E-WF.02
	Square footage associated with the living area for the one and a 1/2 story Salt Box type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
06502	E-WF.02
	Square footage associated with the living area for an additional one story wing on a Salt Box type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
06503	E-WF.02
	Square footage associated with the garage area for the one and half story Salt Box type shell that is described above to be added to the basic shell.  Additional trim and finish items may be added to the basic garage shell.	
	
07460	E-WF.02
	Build a two story provincial shape shell on continuous masonry foundation under living area according to general specifications.   Roofing to be 240# fiberglass shingles over 15# felt with aluminum flashing.  Gutters and downspouts to be aluminum with all exterior wood trim to be tight knot pine, fir or spruce.  Soffits maybe ACX plywood.  Siding to be 1/2"x8" beveled cedar. Included are two solid core exterior doors with hardware and locksets.  A builder grade wood double hung window will be installed for ever 100 SF of living area as well as two for the garage.     Basic charge for shell, living space, ells or wings, garage, and basement, if any are to be added to this item.  Exterior improvements, such as stoops, decks, driveways, aprons, site work and landscaping, as required by owner, are shown if they are part of the proposal.  ITEMS NOT SHOWN IN THIS DOCUMENT ARE NOT INCLUDED.	
	
07461	E-WF.02
	Square footage associated with the living area for the two story provincial type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
07462	E-WF.02
	Square footage associated with the living area for an additional two story wing on a Provincial type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
07463	E-WF.02
	Square footage associated with the garage area for the two story Provincial type shell that is described above to be added to the basic shell.  Additional trim and finish items may be added to the basic garage shell.	
	
07500	E-WF.02
	Build a two story colonial shell on continuous masonry foundation under living area according to general specifications.  Roofing to be 240# fiberglass shingles over 15# felt with aluminum flashing.  Gutters and downspouts to be aluminum with all exterior wood trim to be tight knot pine, fir or spruce.  Soffits maybe ACX plywood.  Siding to be 1/2"x8" beveled cedar. Included are two solid core exterior doors with hardware and locksets.  A builder grade wood double hung window will be installed for ever 100 SF of living area as well as two for the garage.   Basic charge for shell, living space, ells or wings, garage, and basement, if any are to be added to this item.  Exterior improvements, such as stoops, decks, driveways, aprons, site work and landscaping, as required by owner, are shown if they are part of the proposal.  ITEMS NOT SHOWN IN THIS DOCUMENT ARE NOT INCLUDED.	
	
07501	E-WF.02
	Square footage associated with the living area for the two story Colonial type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
07502	E-WF.02
	Square footage associated with the living area for an additional one story wing on a Colonial type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
07503	E-WF.02
	Square footage associated with the garage area for the two story Colonial type shell that is described above to be added to the basic shell.  Additional trim and finish items may be added to the basic garage shell.	
	
07600	E-WF.02
	Build a two story plantation style shell on a continuous masonry foundation according to general specifications.   Roofing to be 240# fiberglass shingles over 15# felt with aluminum flashing.  Gutters and downspouts to be aluminum with all exterior wood trim to be tight knot pine.  Portico posts & headers covered with pine. Soffits maybe ACX plywood.  Siding to be 1/2"x8" beveled cedar.  Included are two solid core exterior doors with hardware and lock sets.  A builder grade wood double hung window will be installed for ever 100 SF of living area as well as two for the garage.   Basic charge for shell, living space, ells or wings, garage, and basement, if any are to be added to this item.  Exterior improvements, such as stoops, decks, driveways, aprons, site work and landscaping, as required by owner, are shown if they are part of the proposal.  ITEMS NOT SHOWN IN THIS DOCUMENT ARE NOT INCLUDED.	
	
07601	E-WF.02
	Square footage associated with the living area for the two story plantation style shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
07602	E-WF.02
	Square footage associated with the living area for an additional two story wing on a plantation style shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
07603	E-WF.02
	Square footage associated with the garage area for the one story plantation style shell that is described above to be added to the basic shell.  Additional trim and finish items may be added to the basic garage shell.	
	
10202	E-WF.02
	Square footage associated with the living area for an additional two story wing on a Victorian type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
10510	E-WF.02
	Build a two and a half story colonial shell on a continuous masonry foundation according to general specifications.   Roofing to be 240# fiberglass shingles over 15# felt with aluminum flashing.  Gutters and downspouts to be aluminum with all exterior wood trim to be tight knot pine.  Portico posts & headers covered with pine. Soffits maybe ACX plywood.  Siding to be 1/2"x8" beveled cedar.  Included are two solid core exterior doors with hardware and lock sets.  A builder grade wood double hung window will be installed for ever 100 SF of living area as well as two for the garage.   Basic charge for shell, living space, ells or wings, garage, and basement, if any are to be added to this item.  Exterior improvements, such as stoops, decks, driveways, aprons, site work and landscaping, as required by owner, are shown if they are part of the proposal.  ITEMS NOT SHOWN IN THIS DOCUMENT ARE NOT INCLUDED.	
	
10511	E-WF.02
	Square footage associated with the living area for the two and a half story Colonial type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
10512	E-WF.02
	Square footage associated with the living area for an additional one story wing on a Colonial type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
10513	E-WF.02
	Square footage associated with the garage area for the one story Colonial type shell that is described above to be added to the basic shell.  Additional trim and finish items may be added to the basic garage shell.	
	
10700	E-WF.02
	Build a two and a half story Victorian shell on a continuous masonry foundation according to general specifications.   Roofing to be 240# fiberglass shingles over 15# felt with aluminum flashing.  Gutters and downspouts to be aluminum with all exterior wood trim to be tight knot pine.  Portico posts & headers covered with pine. Soffits maybe ACX plywood.  Siding to be 1/2"x8" beveled cedar.  Included are two solid core exterior doors with hardware and lock sets.  A builder grade wood double hung window will be installed for ever 100 SF of living area as well as two for the garage.   Basic charge for shell, living space, ells or wings, garage, and basement, if any are to be added to this item.  Exterior improvements, such as stoops, decks, driveways, aprons, site work and landscaping, as required by owner, are shown if they are part of the proposal.  ITEMS NOT SHOWN IN THIS DOCUMENT ARE NOT INCLUDED.	
	
10701	E-WF.02
	Square footage associated with the living area for the two and a half story Victorian type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
10702	E-WF.02
	Square footage associated with the living area for an additional two story wing on a Victorian type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
10703	E-WF.02
	Square footage associated with the garage area for the one  story Victorian type shell that is described above to be added to the basic shell.  Additional trim and finish items may be added to the basic garage shell.	
	
10800	E-WF.02
	Build a three level Federal style townhome shell on a continuous masonry foundation according to general specifications.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.   Roofing to be 240# fiberglass shingles over 15# felt with aluminum flashing.  Gutters and downspouts to be aluminum with all exterior wood trim to be tight knot pine. . Soffits maybe ACX plywood.  Siding to bedouble 4 vinyl applied over a foam backer.  Included are two solid core exterior doors with hardware and lock sets.  A builder grade wood double hung window will be installed for ever 80 SF of living area as well as two for the garage.   Basic charge for shell; living space, garage, and basement, if any, are to be added to this item.  Exterior improvements, such as stoops, decks, driveways, aprons, site work and landscaping, as required by owner, are shown if they are part of the proposal.  ITEMS NOT SHOWN IN THIS DOCUMENT ARE NOT INCLUDED.	
	
10801	E-WF.02
	Square footage associated with the living area for the three level Federal  Victorian type shell that is described above, to be added to the basic shell.  Additional items maybe added or subtracted as shown below to finish the basic shell.  Additional trim and interior finish items may be added to the shell.	
	
10802	E-WF.02
	Additional charge associated with the living area for an end unit Federal townhouse type shell that is described above, to be added to the basic shell.  	
	
10803	E-WF.02
	Square footage charge associated with the garage area for a Federal townhome to be added on the ground floor that is described above to be added to the basic shell.  Additional trim and finish items may be added to the basic garage shell.  This charge doesn't include any additional grading that may be required.  This amount is in addition to the basic living area charges. 	
	
14853	E-WF.02
	Substitute formed and poured reinforced corners and interior foundation lines from basic shell.	
	
14856	E-WF.02
	Eliminate the setup of temporary electrical service from basic shell.	
	
17901	E-WF.02
	Added to the shell and the basic finish and trim package shown above and includes two bathrooms. Specifications to follow. Additional specifications may be added or deducted. (See below)	
	
17902	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow.	
	
17903	E-WF.02
	Square footage of the garage area to be added to the shell and the basic finish and trim package shown above.  The garage will have one exterior grade solid core birch door install from the garage to the house.  A 9-0 x 7-0 four section overhead type door will be installed and trimmed on the exterior.  One double hung window will be trimmed on the outside.  A single exterior light and GFI outlet will be furnished and install.  Three outlets and one switched light will be installed inside the garage.  Firecode 5/8" drywall will be hung, taped and a single finish coat applied to the house side party wall and ceiling of the garage, with the other three walls to be normal 1/2" drywall hung, taped and a single finish coat applied.	
	
17905	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow. Additional specifications may be added or deducted. (See below)	
	
17906	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow.	
	
17907	E-WF.02
	Square footage of the garage area to be added to the shell and the basic finish and trim package shown above.  The garage will have one exterior grade solid core birch door install from the garage to the house.  A 9-0 x 7-0 four section overhead type door will be installed and trimmed on the exterior.  One double hung window will be trimmed on the outside.  A single exterior light and GFI outlet will be furnished and install.  Three outlets and one switched light will be installed inside the garage.  Firecode 5/8" drywall will be hung, taped and a single finish coat applied to the house side party wall and ceiling of the garage, with the other three walls to be normal 1/2" drywall hung, taped and a single finish coat applied.	
	
17915	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow. Additional specifications may be added or deducted. (See below)	
	
17916	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow.	
	
17917	E-WF.02
	Square footage of the garage area to be added to the shell and the basic finish and trim package shown above.  The garage will have one exterior grade solid core birch door install from the garage to the house.  A 9-0 x 7-0 four section overhead type door will be installed and trimmed on the exterior.  One double hung window will be trimmed on the outside.  A single exterior light and GFI outlet will be furnished and install.  Three outlets and one switched light will be installed inside the garage.  Firecode 5/8" drywall will be hung, taped and a single finish coat applied to the house side party wall and ceiling of the garage, with the other three walls to be normal 1/2" drywall hung, taped and a single finish coat applied.	
	
17920	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow. Additional specifications may be added or deducted. (See below)	
	
17921	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow.	
	
17922	E-WF.02
	Square footage of the garage area to be added to the shell and the basic finish and trim package shown above.  The garage will have one exterior grade solid core birch door install from the garage to the house.  A 9-0 x 7-0 four section overhead type door will be installed and trimmed on the exterior.  One double hung window will be trimmed on the outside.  A single exterior light and GFI outlet will be furnished and install.  Three outlets and one switched light will be installed inside the garage.  Firecode 5/8" drywall will be hung, taped and a single finish coat applied to the house side party wall and ceiling of the garage, with the other three walls to be normal 1/2" drywall hung, taped and a single finish coat applied.	
	
17925	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow. Additional specifications may be added or deducted. (See below)	
	
17926	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow.	
	
17927	E-WF.02
	Square footage of the garage area to be added to the shell and the basic finish and trim package shown above.  The garage will have one exterior grade solid core birch door install from the garage to the house.  A 9-0 x 7-0 four section overhead type door will be installed and trimmed on the exterior.  One double hung window will be trimmed on the outside.  A single exterior light and GFI outlet will be furnished and install.  Three outlets and one switched light will be installed inside the garage.  Firecode 5/8" drywall will be hung, taped and a single finish coat applied to the house side party wall and ceiling of the garage, with the other three walls to be normal 1/2" drywall hung, taped and a single finish coat applied.	
	
17930	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow. Additional specifications may be added or deducted. (See below)	
	
17931	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow.	
	
17932	E-WF.02
	Square footage of the garage area to be added to the shell and the basic finish and trim package shown above.  The garage will have one exterior grade solid core birch door install from the garage to the house.  A 9-0 x 7-0 four section overhead type door will be installed and trimmed on the exterior.  One double hung window will be trimmed on the outside.  A single exterior light and GFI outlet will be furnished and install.  Three outlets and one switched light will be installed inside the garage.  Firecode 5/8" drywall will be hung, taped and a single finish coat applied to the house side party wall and ceiling of the garage, with the other three walls to be normal 1/2" drywall hung, taped and a single finish coat applied.	
	
17935	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  Specifications to follow. Additional specifications may be added or deducted. (See below)	
	
17936	E-WF.02
	Square footage of the living area to be added to the shell and the basic finish and trim package shown above.  	
	
17937	E-WF.02
	Square footage of the garage area to be added to the shell and the basic finish and trim package shown above.  The garage will have one exterior grade solid core birch door install from the garage to the house.  A 9-0 x 7-0 four section overhead type door will be installed and trimmed on the exterior.  One double hung window will be trimmed on the outside.  A single exterior light and GFI outlet will be furnished and install.  Three outlets and one switched light will be installed inside the garage.  Firecode 5/8" drywall will be hung, taped and a single finish coat applied to all walls and ceiling of the garage, drywall hung, taped and a single finish coat applied.	
	
17960	E-WF.02
	Trim and interior finish to include two exterior doors with 2 1/4" casing.  The interior doors will be pre-hung hollow core flush doors with all hardware including a passage and privacy lock.  All the windows will be trimmed with paint grade casing, stops, stools and window hardware.	
	
17961	E-WF.02
	Excavate and connect home to sewer tap as per code requirements. Connection and tap fees not included.  Lay sewer pipe from property line to house. Use 4" PVC up to 50 feet.  Lay a 1" copper water line in the same trench from the water tap to the house a maximum of 50 feet.  Back fill the trench.  Rough in the house for four fixture areas: kitchen, laundry and two bathrooms.	
	
17962	E-WF.02
	This trim and finishing package includes bathtub, two piece floor mounted water closet and a two door vanity base.  The bathtub is a 60" x 32" porcelain enamel on cast iron tub.  The water closet is a two piece vitreous china water closet with elongated bowel with cover and seat.  The trim package includes a 48" two-door vanity base with cultured marble top, molded sink and 4" backsplash.	
	
17963	E-WF.02
	This trim and finishing package includes shower, two piece floor mounted water closet and a wall hung vitreous china lavatory.  The shower is a 36" x 32" fiberglass with shower door.  The water closet is a two piece vitreous china water closet with elongated bowel with cover and seat.  The trim package includes a22" x 24" cultured marble top on vanity with a single bowl including faucets and pop-up drain .
	
17964	E-WF.02
	Install kitchen plumbing kit including a stainless steel kitchen double sink, including faucet and spray with 2 strainers a 1/2 horsepower garbage disposer, builder grade cabinets and a builder grade undercounter dishwater.  Installation to include all labor for plumbing and electrical work that is required.	
	
17965	E-WF.02
	Install 4 1/4" OG base and shoe molding on all walls except for bathrooms. Installation includes clothes closets trimmed with hook strips, poles and shelf.  Also includes Linen closet trimmed with 18" plywood shelves. Install base with either coped or mitered joints.  All finish nails to be set, ready for spackling.	
	
17966	E-WF.02
	Install any shop-built basement stairway with handrail. Install main stairway that has two sides open to the living area. Complete stairway to upper levels. Starting newel, birch handrail with easement and newel cap, pine balusters, oak treads and risers. Stairway to be shop built and installed on job by stair builders.  Access to attic provided by manufactured drop down unit.	
	
17967	E-WF.02
	Install factory built builder grade base cabinet package to kitchen. To include a minimum installation of a 3030 wall cabinet with 2 doors rails and stiles. Includes 20lf base cabinets including two door sink unit as well as a 24" four drawer unit, plus any door and drawer units as required to complete the installation. Includes 20lf of wall cabinets to be 15" high and 36" wide, a broom cabinet and 20lf countertop.  Cabinets shall meet or exceed the recommended minimum construction and performance standards as set by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document and may be done by others.	
	
17968	E-WF.02
	Install brand name appliances delivered and installed just before the final trim and clean-up phase.  All appliances to conform to a profile within 4" of the outer edge of the adjacent counter top, this doesn't apply to the refrigerator.  All appliances and required utilities will be attached and installed according to manufacturer's specifications.	
	
17969	E-WF.02
	Install red oak select grade hardwood flooring that is 3/4" x 2 1/4" on prepared subsurface. Lay tongue and groove in matched oak flooring in such a pattern that all irregularities of room dimensions are absorbed in the outside walls. Nailing to be blind in all courses except the starter course. Installation includes sanding or finishing. Package includes carpeting and pad installed per manufacturer's specs. Sheet vinyl flooring in kitchen and ceramic tile flooring in thin set in bathroom.	
	
17971	E-WF.02
	Paint exterior trim and siding with prime and one coat.  All exterior to be one coat. Paint all doors, windows and interior trim with prime and one coat.  Like the exterior only one color. Paint all interior wall and ceiling areas with prime and one coat. Color to match trim and interior of doors and windows.  Paint any attic and basement stairs with prim and one coat.  Paint main stair except for handrails and treads which are to be stained.  Areas not be painted are to be protected.	
	
18780	E-WF.02
	Substitute asphalt or fiberglass shingles for cedar shingles on any roof deck over  15# roofing felt paper with 5" wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 7' rise in 12' run and 8' rise in 12' run.	
	
18857	E-WF.02
	Set up pre-built 2' x 8' sectional forms in existing excavation.  Pour concrete foundation wall 6 inches thick. Includes cutouts for beams, vents, windows etc. Fill the forms with 2500 # (6sack) concrete mix pured by chute from transit mix truck. Clean and strip forms. Pour continuously, take ACI recommended weather precautions as needed.  This a substitution of concrete wall in place of the block wall called for in the basic shell.	
	
18860	E-WF.02
	Replace the ground floor slab called for in the basic shell with a full basement.  Level out ground for floor slab that is to be formed and pour 3000# (6sack) mix over a vapor barrier on top of4" of gravel fill. Slab to have 6x6 #10 wire embedded in concrete.  The depth of the basement slab will be 4" and the finish will be floated and troweled.  Footings to be 36" below grade with a block foundation wall to 8" above grade with a poured bond beam in top course of block with the required anchor bolts.	
	
18861	E-WF.02
	Replace the ground level slab called for in the basic shell with a full basement under the living area.  The block wall is to be laid on existing footing. Lay up walls plumb and true with courses level.  Lay in bond pattern with metal ladder type reinforcing every other course.  Cutouts inserted as required for beams, windows and doorways. Top course to be 4" solid cap blocks.  Blocks to be 8x8x16.  All joints to be tooled and angles installed as needed.  Bucks as required are to be tied into wall and shall be plumb and true.  Wall to be up to 8 feet above footing, with scaffolding as required.  Includes the 4" basement concrete floor.  Mudsills, beams and support columns as needed along with first floors joists and 5/8"plywood subfloor.	
	
18863	E-WF.02
	Extend the depth of the footing from 36" to 48" with the block wall laid up on existing footing. Lay up walls plumb and true with courses level.  Lay in bond pattern with metal ladder type reinforcing every other course.  Top course to be poured solid. Blocks to be 8x8x16.  All joints to be tooled and steel angles installed as needed.	
	
18864	E-WF.02
	Extend the depth of the footing from 36" to 60" with the block wall laid up on existing footing. Lay up walls plumb and true with courses level.  Lay in bond pattern with metal ladder type reinforcing every other course.  Top course to be poured solid. Blocks to be 8x8x16.  All joints to be tooled and steel angles installed as needed.	
	
18865	E-WF.02
	Add an additional step to the entrance slab that is 48" long by 12" deep.  Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction. Concrete to be 6-7" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Treads to be 48 inches wide. Charge per tread.	
	
18866	E-WF.02
	Add an additional step to the entrance slab that is 60" long by 12" deep.  Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction. Concrete to be 6-7" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Treads to be 60 inches wide. Charge per tread.	
	
18867	E-WF.02
	Add an additional step to the entrance slab that is 72" long by 12" deep.  Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction. Concrete to be 6-7" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Treads to be 72 inches wide. Charge per tread.	
	
18868	E-WF.02
	Add the installation of a brick fireplace on existing fireplace footing. To include the hearth, firebox done with firebrick, cleanout and cleanout pit, damper and smoke shelf ready for chimney. Size 36" wide, 29" high and 16" deep.  Footings and brickwork must accommodate chimney of sufficient height to draw properly and to meet all local codes.	
	
18869	E-WF.02
	Install two 8x8 terra cotta flue inside brick chimney to conform to local code.  To include cement wash to the top of the chimney. Install on existing footing and fireplace; however footings must be to undisturbed soil, exterior footing must be below frost line. Interior footing to be below basement slab grade, if present.  Footing to extend at least 12" out side of brick sides.	
	
18875	E-WF.02
	Substitute truss roof system and asphalt/fiberglass shingles with installation of a flat or shed type roof structure including the overhang and eaves, constructed out of 2x6 roof joists nailed 16" oc with joist headers as needed. The installation to be on a roof with a pitch of less than 4 inches in 12 inches. There will be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Roof covering to be 4-Ply installation.	
	
18876	E-WF.02
	Substitute truss roof system and cedar shingles with installation of a flat or shed type roof structure including the overhang and eaves, constructed out of 2x6 roof joists nailed 16" oc with joist headers as needed. The installation to be on a roof with a pitch of less than 4 inches in 12 inches. There will be a 12 inch overhang unless specified. Headers as required maybe solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Roof covering to be 4-Ply installation.	
	
18877	E-WF.02
	Substitute truss roof system and concrete roof tiles with installation of a flat or shed type roof structure including the overhang and eaves, constructed out of 2x6 roof joists nailed 16" oc with joist headers as needed. The installation to be on a roof with a pitch of less than 4 inches in 12 inches. There will be a 12 inch overhang unless specified. Headers as required maybe solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Roof covering to be 4-Ply installation.	
	
18878	E-WF.02
	Apply on shed or gable wood roof deck, 16" cedar shingle applied with 5" exposure over 15 lb. felt paper woven between courses. Shingles can be applied with no felt if wood deck is 1 x 4 or 1 x 6 spaced wood sheathing. Apply shingles with 3 penny rust resistance nails at a slope of 4 inches IN 12. Use the cedar shingles as substitution for asphalt/fiberglass shingles.	
	
18879	E-WF.02
	Apply manufactured concrete roof tiles on plain shed or gable wood roof deck at a slope less than 4 IN 12. 13" x 16.5" x 1/2" tiles with lugs at head to be applied over a base of 2 layers of 30 lb. roofing felt that is hot mopped together. 2" wooden lath strips to be nailed over each rafter to be followed by a mopping of hot asphalt to imbed the lath strips. 1" x 2" redwood battens to be nailed across the lath strips spaced to hang the tiles on nailing every 3rd course of tile. All roof accessories are included. Use concrete tiles instead of asphalt/fiberglass shingles.	
	
18880	E-WF.02
	Substitute asphalt or fiberglass shingles for cedar shingles on any roof deck over  15# roofing felt paper with 5" wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 7' rise in 12' run and 8' rise in 12' run.	
	
18881	E-WF.02
	Apply manufactured concrete roof tiles on plain shed or gable wood roof deck at a slope less than 4 IN 12. 13" x 16.5" x 1/2" tiles with lugs at head to be applied over a base of 2 layers of 30 lb. roofing felt that is hot mopped together. 2" wooden lath strips to be nailed over each rafter to be followed by a mopping of hot asphalt to imbed the lath strips. 1" x 2" redwood battens to be nailed across the lath strips spaced to hang the tiles on nailing every 3rd course of tile. All roof accessories are included. Use concrete tiles instead of cedar shingles.	
	
18882	E-WF.02
	Substitute asphalt or fiberglass shingles for concrete roofing tile on any roof deck over  15# roofing felt paper with 5" wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 7' rise in 12' run and 8' rise in 12' run.	
	
18883	E-WF.02
	Substitute on any roof deck, 16" cedar shingle applied with 5" exposure over 15 lb. felt paper woven between courses for concrete roofing tiles. Shingles can be applied with no felt if wood deck is 1 x 4 or 1 x 6 spaced wood sheathing. Apply shingles with 3 penny rust resistance nails at a slope of 4 inches IN 12. Use the cedar shingles as substitution for asphalt/fiberglass shingles.	
	
18884	E-WF.02
	Substitute 4" veneer brick wall laid on existing footing, over existing frame wall with ties as required for beveled cedar siding.  Lay up walls plumb and true with courses level.  All joints to be tooled and steel angles installed as needed.  Bucks as required are to be tied into wall and shall be plumb and true.  Facing side of brick to be cleaned after installation.	
	
18885	E-WF.02
	Substitute cementatious stucco for cedar siding.  Install stucco so that it is fortified with plastic cement mortar over frame wall with studs to be 16" oc and with a minimum of 1/2" sheathing.  Stucco to be applied in three coats one inch thick.	
	
18886	E-WF.02
	Substitute cementatious stucco for cedar siding.  Install stucco so that it is fortified with plastic cement mortar over frame wall with studs to be 16" oc and with a minimum of 1/2" sheathing.  Stucco to be applied in three coats one inch thick.	
	
18887	E-WF.02
	Install 16" Cedar Shingles over wood sheath walls. Shingles to be installed over 15 lb. felt or rosin coated paper with 3d galvanized nails with both inside and outside corners to be woven and shingles installed with a 7 1/2" exposure.	
	
18888	E-WF.02
	Substitute cementatious stucco for brick veneer siding.  Install stucco so that it is fortified with plastic cement mortar over frame wall with studs to be 16" oc and with a minimum of 1/2" sheathing.  Stucco to be applied in three coats one inch thick.	
	
18889	E-WF.02
	Substitute 16" Cedar Shingles instead of stucco over wood sheathed walls. Shingles to be installed over 15 lb. felt or rosin coated paper with 3d galvanized nails with both inside and outside corners to be woven and shingles installed with a 7 1/2" exposure.	
	
18890	E-WF.02
	Substitute 16" Cedar Shingles instead of stucco over wood sheathed walls. Shingles to be installed over 15 lb. felt or rosin coated paper with 3d galvanized nails with both inside and outside corners to be woven and shingles installed with a 7 1/2" exposure.	
	
18891	E-WF.02
	Substitute 4" veneer brick wall laid on existing footing, over existing frame wall with ties as required for stucco siding.  Lay up walls plumb and true with courses level.  All joints to be tooled and steel angles installed as needed.  Bucks as required are to be tied into wall and shall be plumb and true.  Facing side of brick to be cleaned after installation.	
	
18892	E-WF.02
	Substitute 6" roof overhang and soffit for standard 12" overhang.	
	
18893	E-WF.02
	Rough-in additional plumbing fixture area.	
	
18894	E-WF.02
	This trim and finishing package includes bathtub, two piece floor mounted water closet and a two door vanity base.  The bathtub is a 60" x 32" porcelain enamel on cast iron tub.  The water closet is a two piece vitreous china water closet with elongated bowel with cover and seat.  The trim package includes a 48" two-door vanity base with cultured marble top, molded sink and 4" backsplash.	
	
18895	E-WF.02
	This trim and finishing package includes bathtub, two piece floor mounted water closet and a wall hung vitreous china lavatory.  The bathtub is a 60" x 32" porcelain enamel on cast iron tub.  The water closet is a two piece vitreous china water closet with elongated bowel with cover and seat.  The trim package includes a 20" x 18" vitreous china lavatory with a single bowl including faucets and pop-up drain .
	
18896	E-WF.02
	Install powder room with wall hung vitreous china lavatory and two piece floor mounted water closet.	
	
18897	E-WF.02
	Install new gas boiler with fiberglass supply and lateral ducts and sheet metal return duct work system. Installation includes re-hooking up gas pipeline that is at the furnace location. Installation does not includes tying to existing electric hookup.	
	
18898	E-WF.02
	Substitute gas radiant heating system in one story house.	
	
18899	E-WF.02
	Substitute gas radiant heating system in two story house.	
	
18900	E-WF.02
	Substitute 18" roof overhang and soffit for standard 12" overhang.	
	
18901	E-WF.02
	Install a pre-assembled premium grade fireplace mantel. Mantel to be ponderosa pine with plane or fluted sides. Installation to include top shelf up to 12" wide with the overall width to be up to 72". Installation to be ready for paint or other finish.	
	
18902	E-WF.02
	Install factory built premium grade base cabinets. Upgrade from the normal builder grade. Cabinets shall meet or exceed the recommended minimum construction and performance standards as set by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document and may be done by others.	
	
18903	E-WF.02
	Install factory built builder grade additional base cabinets to include a minimum installation of a 36" wide base sink two door unit as well as a 24" four drawer unit, plus any door and drawer units as required to complete the installation. Cabinets shall meet or exceed the recommended minimum construction and performance standards as set by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document and may be done by others.	
	
18904	E-WF.02
	Install factory built premium grade additional base cabinets to include a minimum installation of a 36" wide base sink two door unit as well as a 24" four drawer unit, plus any door and drawer units as required to complete the installation. Cabinets shall meet or exceed the recommended minimum construction and performance standards as set by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document and may be done by others.	
	
18905	E-WF.02
	Install factory built builder grade additional wall cabinets with the minimum installation to include two 15" high door units, 36" wide and as many 30" high units as required. Cabinets shall meet or exceed the recommended minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
18906	E-WF.02
	Install factory built premium grade additional wall cabinets with the minimum installation to include two 15" high door units, 36" wide and as many 30" high units as required. Cabinets shall meet or exceed the recommended minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
18907	E-WF.02
	Install additional medium grade countertop of plastic laminate with metal or self edge. Installation to include 4" backsplash.	
	
18908	E-WF.02
	Substitute 12 CF for 18 CF refrigerator with economy grade refrigerator. Installation to include any changes to electrical hookups as required.	
	
18909	E-WF.02
	Substitute 21cf double door refrigerator for 18 CF refrigerator.  Installation to include any changes to electrical hookups as required.	
	
18910	E-WF.02
	Substitute interior carpeting installation including padding instead of oak hardwood flooring. Installation to include tack strips and necessary metal edges.	
	
18911	E-WF.02
	Substitute pre-finished select grade oak flooring for regular carpet installation. Lay tongue and groove in matched oak flooring in such a pattern that all irregularities of room dimensions are absorbed in the outside walls. Nailing to be blind in all courses except the starter course.	
	
18912	E-WF.02
	Substitute 24" roof overhang and soffit for standard 12" overhang.	
	
18913	E-WF.02
	Add Wood sleepers and 5/8 plywood underlayment on  concrete slab with solid bridging. Joists to be nailed 16" oc. Lumber shall be pressure treated.	
	
18914	E-WF.02
	Substitute aluminum sliding window for standard wood double-hung window. Window to be double glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
18915	E-WF.02
	Substitute wood double hung window for standard aluminum window installation. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
18916	E-WF.02
	Install additional double glazed wood window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
18917	E-WF.02
	Install additional double glazed aluminum window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
18918	E-WF.02
	Install 1 light picture window, 4-0 x 4-6. With installation to include frame, sash and brick molding. Sash to be 1/2" insulated glass with all interior trim including stool and apron to be included.	
	
18919	E-WF.02
	Install 1 light picture window, 5-4 x 5-2. With installation to include frame, sash and brick molding. Sash to be 1/2" insulated glass with all interior trim including stool and apron to be included.	
	
18920	E-WF.02
	Install either 50 gas hot water heater or 52 electric hot water heater including 2 inches of insulation. Flue and all labor and materials to connect plumbing hookups and gas supply are included in this installation.	
	
18921	E-WF.02
	Install new gas furnace system with fiberglass supply and lateral ducts and sheet metal return duct work system with thermostat. Installation includes re-hooking up gas pipeline that is at the furnace location. Installation does not includes tying to existing electric hookup. Includes double wall metal chimney.	
	
18922	E-WF.02
	Rough in and finish electric service with new panel breaker box to be installed on existing service cable. Installation to include panel box and breakers as required and to install branch wiring. Duplex outlets installed to code including circuits as required. Installation to include 3 appliance outlets, a dishwasher outlet, disposal outlet & switch, 2 bathroom fans vented to the outside, 1 ductless range hood, 2 wall mounted exterior light outlets, 1 ground fault outlet and 1220 volt outlet. Fixture installation and cost of fixtures not included.	
	
04000	E-WF.04
	Use machine equipment to clear medium levels of brush from site.	
	
04001	E-WF.04
	Use machine equipment to clear thick levels of brush from site.	
	
04002	E-WF.04
	Use machine equipment to strip topsoil and stockpile on site.	
	
04200	E-WF.04
	Rough grading around building with dozer.	
	
08000	E-WF.04
	Connect home to sewer pipe per code requirements.  Connection Fee not included.  Lay sewer pipe from property line to house.  Use 4" PVC.	
	
08001	E-WF.04
	Connect home to sewer pipe per code requirements.  Connection Fee not included.  Lay sewer pipe from property line to house.  Use 4" PVC.	
	
08002	E-WF.04
	Connect home to sewer pipe per code requirements.  Connection Fee not included.  Lay sewer pipe from property line to house.  Use 4" vitrified clay pipe.	
	
08003	E-WF.04
	Connect home to sewer pipe per code requirements.  Connection Fee not included.  Lay sewer pipe from property line to house.  Use 6" vitrified clay pipe.	
	
08004	E-WF.04
	Connect home to water supply per code requirements.  Connection Fee not included.  Lay 1" copper pipe from property line to house.	
	
08005	E-WF.04
	Connect home to water supply per code requirements.  Connection Fee not included.  Lay 1" copper pipe from property line to house.	
	
08006	E-WF.04
	Connect home to main gas supply per code requirements.	
	
10100	E-WF.04
	Place 4" corrugated perforated plastic pipe surrounded with at least 6" of 3/4" washed aggregate along the exterior of the perimeter footing. Cover with a vapor barrier. Cost does not include any digging.	
	
11005	E-WF.04
	Install septic system of 1000 gallons with a drainage field of 1000 square feet.  Includes excavation for tank and drainage field.  The concrete distribution box to have 5 outlets.  All pipe to be 4 inch PVC or 4" perforated pipe as required.  There is to be a 24 inch gravel base and backfill as required.	
	
11006	E-WF.04
	Install septic system of 1000 gallons with a drainage field of 2000 square feet.  Includes excavation for tank and drainage field.  The concrete distribution box to have 5 outlets.  All pipe to be 4 inch PVC or 4" perforated pipe as required.  There is to be a 24 inch gravel base and backfill as required.	
	
11007	E-WF.04
	Install septic system of 2000 gallons with a drainage field of 1000 square feet.  Includes excavation for tank and drainage field.  The concrete distribution box to have 5 outlets.  All pipe to be 4 inch PVC or 4" perforated pipe as required.  There is to be a 24 inch gravel base and backfill as required.	
	
11008	E-WF.04
	Install septic system of 1000 gallons with a drainage field of 2000 square feet.  Includes excavation for tank and drainage field.  The concrete distribution box to have 5 outlets.  All pipe to be 4 inch PVC or 4" perforated pipe as required.  There is to be a 24 inch gravel base and backfill as required.	
	
03003	E-WF.05
	Removal of concrete driveway with bulldozer or track loader.	
	
02000	E-WF.06
	Excavate for house basement or crawl space, including minimum of 2 feet beyond house line at walls.	
	
02001	E-WF.06
	Excavate for house basement or crawl space, including minimum of 2 feet beyond house line at walls.	
	
02002	E-WF.06
	Excavate for house basement or crawl space, including minimum of 2 feet beyond house line at walls.	
	
02003	E-WF.06
	Excavate for house basement or crawl space, including minimum of 2 feet beyond house line at walls.	
	
02004	E-WF.06
	Excavate for house basement or crawl space, including minimum of 2 feet beyond house line at walls.	
	
02005	E-WF.06
	Excavate for house basement or crawl space, including minimum of 2 feet beyond house line at walls.	
	
02006	E-WF.06
	Excavate for house basement or crawl space, including minimum of 2 feet beyond house line at walls.	
	
02100	E-WF.06
	Machine backfill to be by front end loader or bulldozer as required. NO rough grading is included. Per square foot.	
	
02101	E-WF.06
	Machine backfill to be by front end loader or bulldozer as required. NO rough grading is included. Per square foot.	
	
02102	E-WF.06
	Machine backfill to be by front end loader or bulldozer as required. NO rough grading is included. Per square foot.	
	
02103	E-WF.06
	Machine backfill to be by front end loader or bulldozer as required. NO rough grading is included. Per square foot.	
	
02104	E-WF.06
	Machine backfill to be by front end loader or bulldozer as required. NO rough grading is included. Per square foot.	
	
02105	E-WF.06
	Machine backfill to be by front end loader or bulldozer as required. NO rough grading is included. Per square foot.	
	
02205	E-WF.06
	Machine excavation to be by front end loader or bulldozer as required. Per job plus costs per cubic foot.	
	
02206	E-WF.06
	Machine excavation to be by front end loader or bulldozer as required. Per cubic foot.	
	
02207	E-WF.06
	Machine back fill to be by front end loader or bulldozer as required. NO rough grading is included. Per job plus costs per cubic foot.	
	
02208	E-WF.06
	Machine backfill to be by front end loader or bulldozer as required. NO rough grading is included. Per square foot.	
	
02209	E-WF.06
	Machine excavate and load by front end loader into two trucks for hauling and dumping within 30 minutes of the job site. NO dumping fees are included.  Cost is per job plus cubic feet of material moved.	
	
02210	E-WF.06
	Machine excavate and load by front end loader into two trucks for hauling and dumping within 30 minutes of the job site. NO dumping fees are included. Cost is per cubic feet of material moved.	
	
01150	E-WF.07
	Trench footings in undisturbed earth.  Excavate trench to 24" to include spread footing.	
	
01151	E-WF.07
	Trench footings in undisturbed earth.  Excavate trench to 36" to include spread footing.	
	
01152	E-WF.07
	Trench footings in undisturbed earth.  Excavate trench to 48" to include spread footing.	
	
01200	E-WF.07
	Dig out by hand for pier footings that are 36" below grade from the bottom of the footing. The size of the footing itself is to be 24x24 by 12 in height. Pour 2500# (5sack) concrete mix into holes for footings and backfill after footing has setup. Pour continuously, take ACI recommended weather precautions as needed.	
	
01201	E-WF.07
	Dig out by hand for pier footings that are 36" below grade from the bottom of the footing. The size of the footing itself is to be 36x48 by 18 in height. Pour 2500# (5sack) concrete mix into holes for footings and backfill after footing has setup. Pour continuously, take ACI recommended weather precautions as needed.	
	
01405	E-WF.07
	Form and Pour inclined concrete wall footings.  The dimension of the footing is 6" high and 16" wide will be poured using 2500psi (5sack) mix. Pour continuously, take ACI recommended weather precautions as needed.  Cost per each step.	
	
01406	E-WF.07
	Form and Pour inclined concrete wall footings.  The dimension of the footing is 8" high and 20" wide will be poured using 2500 PSI (5sack) mix. Pour continuously, take ACI recommended weather precautions as needed.  Cost per each step.	
	
01407	E-WF.07
	Form and Pour inclined concrete wall footings.  The dimension of the footing is 8" high and 24" wide will be poured using 2500 PSI (5sack) mix. Pour continuously, take ACI recommended weather precautions as needed.  Cost per each step.	
	
01408	E-WF.07
	Form and Pour inclined concrete wall footings.  The dimension of the footing is 8" high and 36" wide will be poured using 2500 PSI (5sack) mix. Pour continuously, take ACI recommended weather precautions as needed.  Cost per each step.	
	
04000	E-WF.07
	One coat of bituminous based foundation damp-proofing sealer applied to block or concrete wall at and below grade to ACI recommended standards.	
	
04001	E-WF.07
	Two coats of bituminous based foundation damp-proofing sealer applied to block or concrete wall at and below grade to ACI recommended standards.	
	
04005	E-WF.07
	Trowel apply a cementatious coating to masonry wall.	
	
05101	E-WF.07
	Set up pre-built 2' x 8' sectional forms in existing excavation.  Pour concrete foundation wall 8 inches thick. Includes cutouts for beams, vents, windows etc. Fill the forms with 2500 # (6sack) concrete mix pured by chute from transit mix truck. Clean and strip forms. Pour continuously, take ACI recommended weather precautions as needed.	
	
05102	E-WF.07
	Set up pre-built 2' x 8' sectional forms in existing excavation.  Pour concrete foundation wall 10 inches thick. Includes cutouts for beams, vents, windows etc. Fill the forms with 2500 # (6sack) concrete mix pured by chute from transit mix truck. Clean and strip forms. Pour continuously, take ACI recommended weather precautions as needed.	
	
05103	E-WF.07
	Set up pre-built 2' x 8' sectional forms in existing excavation.  Pour concrete foundation wall 12 inches thick. Includes cutouts for beams, vents, windows etc. Fill the forms with 2500 # (6sack) concrete mix pured by chute from transit mix truck. Clean and strip forms. Pour continuously, take ACI recommended weather precautions as needed.	
	
06002	E-WF.07
	Block wall laid on existing footing. Lay up walls plumb and true with courses level.  Lay in bond pattern with metal ladder type reinforcing every other course.  Cutouts inserted as required for beams, windows and doorways. Top course to be 4" solid cap blocks.  Blocks to be 8x8x16.  All joints to be tooled and steel angles installed as needed.  Bucks as required are to be tied into wall and shall be plumb and true.  Wall to be only up to 8 feet above footing with scaffolding as required.	
	
06003	E-WF.07
	Block wall laid on existing footing. Lay up walls plumb and true with courses level.  Lay in bond pattern with metal ladder type reinforcing every other course.  Cutouts inserted as required for beams, windows and doorways. Top course to be 4" solid cap blocks.  Blocks to be 10x8x16.  All joints to be tooled and steel angles installed as needed.  Bucks as required are to be tied into wall and shall be plumb and true.  Wall to be only up to 8 feet above footing with scaffolding as required.	
	
06004	E-WF.07
	Block wall laid on existing footing, lay up walls plumb and true with courses level.  Lay in bond pattern with metal ladder type reinforcing every other course.  Top course to be 4" solid cap blocks.  Blocks to be 12x8x16.  All joints to be tooled and steel angles installed as needed.  Bucks as required are to be tied into wall and shall be plumb and true.	
	
09000	E-WF.07
	Treated wood foundation using box panels constructed with 2x4 studs 16"oc covered by 1/2" treated CDX plywood on one side, with batt insulation between studs. 15# felt paper under the plywood with a 6 mil polyethylene vapor barrier. Lying on pressure treated 2x12's on top of 3/4" washed or 1/2 crushed gravel 4" deep. Corrosion resistant fasteners to be used.	
	
09001	E-WF.07
	Treated wood foundation using box panels constructed with 2x6 studs 16"oc covered by 3/4" treated CDX plywood on one side, with batt insulation between studs. 15# felt paper under the plywood with a 6 mil polyethylene vapor barrier. Lying on pressure treated 2x12's on top of 3/4" washed or 1/2" crushed gravel 4" deep. Corrosion resistant fasteners to be used.	
	
09002	E-WF.07
	Treated wood foundation using box panels constructed with 2x8 studs 16"oc covered by 3/4" treated CDX plywood on one side, with batt insulation between studs. 15# felt paper under the plywood with a 6 mil polyethylene vapor barrier. Lying on pressure treated 2x12's on top of 3/4" washed or 1/2" crushed gravel 4" deep. Corrosion resistant fasteners to be used.	
	
01000	E-WF.08
	Pour continuous concrete footing in an existing excavation, filling the trench with 2500 # (5sack) concrete mix. Pour concrete from truck with strip forms. Includes forming footing with 2" lumber. Footing to be 8 inches deep by 16 inches wide.	
	
01001	E-WF.08
	Pour continuous concrete footing in an existing excavation, filling the trench with 2500 # (5sack) concrete mix. Pour concrete from truck with strip forms. Includes forming footing with 2" lumber. Footing to be 10 inches deep by 20 inches wide.	
	
01003	E-WF.08
	Pour continuous concrete footing in an existing excavation, filling the trench with 2500 # (5sack) concrete mix. Pour concrete from truck with strip forms. Includes forming footing with 2" lumber. Footing to be 12 inches deep by 24 inches wide.	
	
01004	E-WF.08
	Pour continuous concrete footing in an existing excavation, filling the trench with 2500 # (5sack) concrete mix. Pour concrete from truck with strip forms. Includes forming footing with 2" lumber. Footing to be 12 inches deep by 36 inches wide.	
	
03031	E-WF.08
	Wheelbarrow or Georgia buggy concrete up to 75' and pour into forms. Includes set up and removal as well as transit-mix truck waiting time.	
	
05028	E-WF.08
	Two continuous 1/2" (#4) steel reinforcement bars in the concrete footings. Bars to be placed in the middle of the footing with care to be taken during pouring that the bars do not move.	
	
05029	E-WF.08
	Three continuous 1/2" (#4) steel reinforcement bars in the concrete footings. Bars to be placed in the middle of the footing with care to be taken during pouring that the bars do not move.	
	
05030	E-WF.08
	A grid of 3/8" (#3) steel reinforcement bars in the concrete wall. taken during pouring that the bars do not move.	
	
07300	E-WF.08
	Pour 3000# (6sack) mix over a vapor barrier on top of 4" of gravel fill. Poured on level ground with no digging out. Pour concrete from transit mix truck by chute using 6 x 6 #10 wire mesh.	
	
07301	E-WF.08
	Pour 3000# (6sack) mix over a vapor barrier on top of 4" of gravel fill. Poured on level ground with no digging out. Pour concrete from transit mix truck by chute using 6 x 6 #10 wire mesh.  Slab to be 6 inches thick and floated and trowled.	
	
07302	E-WF.08
	Level out ground for floor slab that is to be formed and pour 3000# (6sack) mix over a vapor barrier on top of 4" of gravel fill. Slab to have 6x6 #10 wire embedded in concrete.  The depth of the basement slab will be 3" and the finish will be floated and troweled.	
	
07303	E-WF.08
	Level out ground for floor slab that is to be formed and pour 3000# (6sack) mix over a vapor barrier on top of 4" of gravel fill. Slab to have 6x6 #10 wire embedded in concrete.  The depth of the basement slab will be 6" and the finish will be floated and troweled.	
	
11033	E-WF.08
	Pump concrete up to 300' and pour into forms. Includes set up, pump and operator and take down time as well as transit-mix truck waiting time.  Set up charge.	
	
11034	E-WF.08
	Pump concrete up to 300' and pour into forms. Includes set up, pump and operator and take down time as well as transit-mix truck waiting time.  Charge per LF to the pour, maximum distance pumped.	
	
18300	E-WF.08
	Dig footings on undisturbed earth.  Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Pour concrete footings. Build up block with brick facing.  Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction. Concrete to be 5-6" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Cover risers, treads and platform with brick. Ea. plus SF charge.	
	
18301	E-WF.08
	Dig footings on undisturbed earth.  Excavate trench to 36". Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Pour concrete footings. Build up block with brick facing. Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction. Concrete to be 5-6" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Treads to be 48 inches wide. Charge per tread.	
	
18302	E-WF.08
	Dig footings on undisturbed earth.  Excavate trench to 36". Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Pour concrete footings. Build up block with brick facing. Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction. Concrete to be 5-6" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Treads to be 60 inches wide. Charge per tread.	
	
18303	E-WF.08
	Dig footings on undisturbed earth.  Excavate trench to 36". Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Pour concrete footings. Build up block with brick facing. Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction. Concrete to be 5-6" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Treads to be 72 inches wide. Charge per tread.	
	
18400	E-WF.08
	Dig footings on undisturbed earth.  Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Pour concrete footings. Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction.  Concrete to be 5-6" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Tread to be 48 inches wide. Ea. plus per tread charge.	
	
18401	E-WF.08
	Dig footings on undisturbed earth.  Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Pour concrete footings. Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction.  Concrete to be 5-6" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Tread to be 48 inches wide. Ea. plus per tread charge.	
	
18402	E-WF.08
	Dig footings on undisturbed earth.  Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Pour concrete footings. Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction.  Concrete to be 5-6" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Tread to be 60 inches wide. Ea. plus per tread charge.	
	
18403	E-WF.08
	Dig footings on undisturbed earth.  Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Pour concrete footings. Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction.  Concrete to be 5-6" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Tread to be 72 inches wide. Ea. plus per tread charge.	
	
21504	E-WF.08
	Level site by hand that is already close to grade or has been excavated. Provide 4" compacted base of sand, or gravel. Form for 4" slab, place #10 wire mesh and required expansion joints then pour 4" slab with 2500# (5sack) concrete mix. Pour continuously, take ACI recommended weather precautions as needed.	
	
01503	E-WF.09
	Pave 2" asphalt driveway over prepared base. Base to be 6 inches compacted gravel. Pavement to be compacted when hot and to between 92-97% compaction. Surface shall be smooth and flat with no bird baths over 1/4".	
	
09500	E-WF.09
	Level site by hand that is already close to grade or has been excavated. Provide 4" compacted base of sand, or gravel. Form for 4" slab, place #10 wire mesh and required expansion joints then pour 4" slab with 2500# (5sack) concrete mix. Pour continuously, take ACI recommended weather precautions as needed.	
	
09501	E-WF.09
	Level site by hand that is already close to grade or has been excavated. Provide 6" compacted base of sand, or gravel. Form for 5" slab, place #10 wire mesh and required expansion joints then pour 4" slab with 2500# (5sack) concrete mix. Pour continuously, take ACI recommended weather precautions as needed.	
	
09502	E-WF.09
	Level site by hand that is already close to grade or has been excavated. Provide 6" compacted base of sand, or gravel. Form for 6" slab, place #10 wire mesh and required expansion joints then pour 4" slab with 2500# (5sack) concrete mix. Pour continuously, take ACI recommended weather precautions as needed.	
	
01008	E-WF.10
	4" veneer brick wall laid on existing footing, over existing frame wall with ties as required.  Lay up walls plumb and true with courses level.  All joints to be tooled and steel angles installed as needed.  Bucks as required are to be tied into wall and shall be plumb and true.  Facing side of brick to be cleaned after installation.	
	
02104	E-WF.10
	Dig footings on undisturbed earth.  Drill into existing housewall and install four (4) 1/2" steel bars to tie footings into house. Pour concrete footings. Build up block with brick facing.  Form in place with #5 steel rebars placed 12" on center.  Forming to be sufficient to support weight during construction. Concrete to be 5-6" in depth and #3000 (6sack) mix.  Finish to be floated and troweled and the broom finished. Cover risers, treads and platform with brick. Ea. plus SF charge.	
	
04500	E-WF.10
	Install cementatious stucco that has been fortified with plastic cement mortar over solid masonry. Stucco to be applied in three coats one inch thick.	
	
07400	E-WF.10
	Block piers laid on existing footing, lay up piers plumb and true with courses level. Top course to be 4" solid cap blocks or filled solid with concrete. Blocks to be 8x16x16. All joints to be tooled.	
	
07402	E-WF.10
	Brick piers, 12x12, laid on existing footing, lay up piers plumb and true with courses level. All joints to be tooled.	
	
07403	E-WF.10
	Brick piers, 16x16, laid on existing footing, lay up piers plumb and true with courses level. All joints to be tooled.	
	
20213	E-WF.10
	Install brick fireplace on existing fireplace footing. To include the hearth, firebox done with firebrick, cleanout and cleanout pit, damper and smoke shelf ready for chimney. Size 36" wide, 29" high and 16" deep.	
	
20216	E-WF.10
	Raise hearth up to one foot off the floor and match with the bottom of the fireplace firebox.	
	
21200	E-WF.10
	Install one 8x8 terra cotta flue inside brick chimney to conform to local code to include cement wash at the top of the chimney. Install on existing footing; however footings must be to undisturbed soil, exterior footing must be below frost line. Interior footing to be below basement slab grade. Footing to extend at least 12" out side of brick sides.	
	
21201	E-WF.10
	Install two 8x8 terra cotta flue inside brick chimney to conform to local code to include cement wash at the top of the chimney. Install on existing footing; however footings must be to undisturbed soil, exterior footing must be below frost line. Interior footing to be below basement slab grade. Footing to extend at least 12" out side of brick sides.	
	
21202	E-WF.10
	Install one 8x12 terra cotta flue inside brick chimney to conform to local code to include cement wash at the top of the chimney. Install on existing footing; however footings must be to undisturbed soil, exterior footing must be below frost line. Interior footing to be below basement slab grade. Footing to  extend at least 12" out side of brick sides.	
	
21203	E-WF.10
	Install two 8x12 terra cotta flues inside brick chimney to conform to local code to include cement wash at the top of the chimney. Install on existing footing; however footings must be to undisturbed soil, exterior footing must be below frost line. Interior footing to be below basement slab grade. Footing to extend at least 12" out side of brick sides.	
	
03000	E-WF.11
	Steel beam bearing on existing masonry or steel column supports, including bearing plates.	
	
03001	E-WF.11
	Steel beam bearing on existing masonry or steel column supports, including bearing plates.	
	
04008	E-WF.11
	Hollow steel column with base plate and adjustable cap plate up to 8' long.	
	
13114	E-WF.11
	Install prefabricated metal wood-burning fireplace and chimney, including exterior chimney housing. Installation to conform to local fire code. Installation to have a base diameter within 30" x 30" and be 50" from base to chimney section. Installation to include an overall height of 13' from base to top of chimney;  for additional chimney height above 13', see additional specification.	
	
14017	E-WF.11
	Install stainless steel double wall metal chimney at least 10" in diameter.	
	
14115	E-WF.11
	Install additional approved prefabricated metal chimney sections above fireplace installation. Chimney sections to be manufacture approved and conform to local fire code.	
	
03013	E-WF.12
	Install a wood glue-lam 3" x9 " beam with a nominal flange size of 4". Beam installed in accordance with manufacturers designed maximum load.  Beams to bear the seal of a Registered Professional Engineer. Manufacturer to approve the installation and all connections and connectors.	
	
03014	E-WF.12
	Install a wood micro-lam 3" x 12" beam with a nominal flangesize of 4". Beam installed in accordance with manufacturers designed maximum load.  Beams to bear the seal of a Registered Professional Engineer. Manufacturer to approve the installation and all connections and connectors.	
	
03129	E-WF.12
	All engineered joists will be used to full length permissible under applicable building code.  Joists to be attached 16" oc. Lumber to be prefabricated "I" shaped engineered joists.  Joist will be fastened to a bolted mud sill at least every 16".  Bridging is not required.  Solid perimeter banding with joist headers and hangers as required.  Based on square footage of floor.	
	
03130	E-WF.12
	All truss joists type engineered joists will be used to full length permissible under applicable building code.  Truss joists to be attached 16" oc. Joists to be 11" prefabricated "I" shaped truss joists or similar pre-engineered joists.  Joists will be fastened to a bolted mud sill at least every 16".  Bridging is not required.  Solid perimeter banding with joist headers and hangers as required.	
	
04002	E-WF.12
	Wood beam bearing on existing supports. Either solid or built-up wood. Wood to be pressure treated.	
	
04003	E-WF.12
	Wood beam bearing on existing supports. Either solid or built-up wood. Wood to be pressure treated.	
	
04004	E-WF.12
	Wood beam bearing on existing supports. Either solid or built-up wood. Wood to be pressure treated.	
	
04005	E-WF.12
	Wood beam bearing on existing supports. Either solid or built-up wood. Wood to be pressure treated.	
	
04006	E-WF.12
	Steel plate between 2 2x10's on existing supports, including plate, lumber, nuts and bolts.	
	
04007	E-WF.12
	Plywood plate glued and bolted between 2 2x10's on existing supports, including plate, lumber, nuts and bolts.	
	
05025	E-WF.12
	Pressure treated fir or pine 2" x 6" sill plated installed with anchor bolts 4' oc to foundation.	
	
05026	E-WF.12
	Pressure treated fir or pine sill plate 2" x 8" attached to the foundation with anchor bolts 4' oc per applicable building code.	
	
05027	E-WF.12
	Pressure treated fir or pine 4" x 6" sill plated installed with anchor bolts 4' oc to foundation.	
	
05028	E-WF.12
	Pressure treated fir or pine sill plate 4" x 8" attached to the foundation with anchor bolts 4' oc per applicable building code.	
	
05029	E-WF.12
	Redwood 2" x 4" sill plate installed with anchor bolts 4' oc to foundation..	
	
05030	E-WF.12
	Redwood 2" x 4" sill plate installed with anchor bolts 4' oc to foundation..	
	
07050	E-WF.12
	Wood sleepers on existing wood, concrete or masonry deck with solid bridging, joist headers as required over a vapor barrier. Joists to be nailed 16" oc. Lumber shall be Pressure Treated Lumber.	
	
07051	E-WF.12
	Wood sleepers on existing wood, concrete or masonry deck with solid bridging, joist headers as required over a vapor barrier. Joists to be nailed 16" oc. Lumber shall be pressure treated.	
	
07052	E-WF.12
	Wood sleepers on existing wood, concrete or masonry deck with solid bridging, joist headers as required over a vapor barrier. Joists to be nailed 16" oc. Lumber shall be pressure treated.	
	
07053	E-WF.12
	Wood sleepers on existing wood, concrete or masonry deck with solid bridging, joist headers as required over a vapor barrier. Joists to be nailed 16" oc. Lumber shall be pressure treated.	
	
07054	E-WF.12
	Wood sleepers on existing wood, concrete or masonry deck with solid bridging, joist headers as required over a vapor barrier. Joists to be nailed 24" oc. Lumber shall be Pressure Treated Lumber.	
	
07055	E-WF.12
	Wood sleepers on existing wood, concrete or masonry deck with solid bridging, joist headers as required over a vapor barrier. Joists to be nailed 16" oc. Lumber shall be pressure treated.	
	
07056	E-WF.12
	Wood sleepers on existing wood, concrete or masonry deck with solid bridging, joist headers as required over a vapor barrier. Joists to be nailed 24" oc. Lumber shall be pressure treated.	
	
07057	E-WF.12
	Wood sleepers on existing wood, concrete or masonry deck with solid bridging, joist headers as required over a vapor barrier. Joists to be nailed 16" oc. Lumber shall be pressure treated.	
	
07107	E-WF.12
	All joist lumber will be used to full length permissible under applicable building code. Joists to be nailed 16" oc. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Floor joist will be fastened to a bolted mud sill with bridging at least every 8'. Solid perimeter banding with joist headers and hangers as required.	
	
07108	E-WF.12
	All joist lumber will be used to full length permissible under applicable building code. Joists to be nailed 16" oc. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Floor joist will be fastened to a bolted mud sill with bridging at least every 8'. Solid perimeter banding with joist headers and hangers as required.	
	
07109	E-WF.12
	All joist lumber will be used to full length permissible under applicable building code. Joists to be nailed 16" oc. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Floor joist will be fastened to a bolted mud sill with bridging at least every 8'. Solid perimeter banding with joist headers and hangers as required.	
	
07110	E-WF.12
	All joist lumber will be used to full length permissible under applicable building code. Joists to be nailed 16" oc. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Floor joist will be fastened to a bolted mud sill with bridging at least every 8'. Solid perimeter banding with joist headers and hangers as required.	
	
07111	E-WF.12
	All joist lumber will be used to full length permissible under applicable building code. Joists to be nailed 16" oc. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Floor joist will be fastened to top plate of first floor with bridging at least every 8'. Solid perimeter banding with joist headers and hangers as required.	
	
07112	E-WF.12
	All joist lumber will be used to full length permissible under applicable building code. Joists to be nailed 16" oc. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Floor joist will be fastened to top plate of first floor with bridging at least every 8'. Solid perimeter banding with joist headers and hangers as required.	
	
07113	E-WF.12
	All joist lumber will be used to full length permissible under applicable building code. Joists to be nailed 16" oc. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Floor joist will be fastened to top plate of first floor with bridging at least every 8'. Solid perimeter banding with joist headers and hangers as required.	
	
07114	E-WF.12
	All joist lumber will be used to full length permissible under applicable building code. Joists to be nailed 16" oc. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Floor joist will be fastened to top plate of first floor with bridging at least every 8'. Solid perimeter banding with joist headers and hangers as required.	
	
07115	E-WF.12
	Plywood to be CDX grade, glued and nailed as per manufacturers specifications to floor joists.	
	
07116	E-WF.12
	Plywood to be CDX grade, glued and nailed as per manufacturers specifications to floor joists.	
	
07117	E-WF.12
	Plywood to be CDX grade, glued and nailed as per manufacturers specifications to floor joists.	
	
07118	E-WF.12
	Plywood to be CDX grade, glued and nailed as per manufacturers specifications to floor joists.	
	
07120	E-WF.12
	Solid wood subflooring 3/4" thick either  8"  wide in pine, fir or hemlock nailed to the floor joists every 8" to 12" in a diagonal pattern.	
	
07121	E-WF.12
	Solid wood subflooring 3/4" thick either  6"  wide in pine, fir or hemlock nailed to the floor joists every 8" to 12" in a diagonal pattern.	
	
07122	E-WF.12
	Solid wood subflooring 3/4" thick either 8" wide in pine, fir or hemlock nailed to floor joists every 8" to 12" in a horizontal pattern.	
	
07123	E-WF.12
	Solid wood subflooring 3/4" thick either  6" wide in pine, fir or hemlock nailed to floor joists every 8" to 12" in a horizontal pattern.	
	
02109	E-WF.13
	Apply 3/8" oriented strand board over existing wood wall framing.	
	
02110	E-WF.13
	Apply 1/2 " oriented strand board over existing wood wall framing.	
	
02200	E-WF.13
	Apply 3/8" CDX plywood sheathing over existing wood wall framing.	
	
02201	E-WF.13
	Apply 1/2" CDX plywood sheathing over existing wood wall framing.	
	
02202	E-WF.13
	Apply 5/8" CDX plywood sheathing over existing wood wall framing.	
	
02203	E-WF.13
	Apply 1/2" CDX plywood over existing wood wall framing at each corner and sheath the balance of the wall surface with 1/2" asphalt impregnated composition sheathing.	
	
02204	E-WF.13
	Apply 1/2" CDX plywood over existing wood wall framing at each corner and sheath the balance of the wall surface with 1/2" foil faced foam sheathing.	
	
02205	E-WF.13
	Apply 1/2" CDX plywood over existing wood wall framing at each corner and sheath the balance of the wall surface with 5/8" foil faced foam sheathing.	
	
02206	E-WF.13
	Apply 1/2" CDX plywood over existing wood wall framing at each corner and sheath the balance of the wall surface with 3/4" foil faced foam sheathing.	
	
04000	E-WF.13
	Construct an interior bearing or non-bearing walls of 2x4's nailed 16 oc with a sole plate and one or two cap plates.  Headers as required may be solid or laminated and sized to code.  Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.  Requires that the exterior walls are figured seperately.	
	
04001	E-WF.13
	Construct an interior/exterior bearing wall of 2x4's nailed 16 oc with a sole plate and two cap plates.  Headers as required may be solid or laminated and sized to code.  Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
04002	E-WF.13
	Construct an interior/exterior bearing wall of 2x4's nailed 24 oc with a sole plate and two cap plates.  Headers as required may be solid or laminated and sized to code.  Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
04003	E-WF.13
	Construct an interior/exterior bearing wall of 2x6's nailed 16" oc with a sole plate and two cap plates. Headers as required may be solid or laminated and sized to code. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
04004	E-WF.13
	Construct an interior/exterior bearing wall of 2x6's nailed 24" oc with a sole plate and two cap plates. Headers as required may be solid or laminated and sized to code. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
04005	E-WF.13
	Construct 4' kneewall to support rafters. Lumber shall be kiln dried #2 Hem-Fir/Southern Pine/Douglas Fir.  Construction to include sole plate and one cap with studs cut at angle to fit rafters.	
	
04006	E-WF.13
	Construct 6" kneewall to support rafters. Lumber shall be kiln dried #2 or better Hem-fir/Southern pine/Douglas Fir.  Construction to include sole plate, one cap and studs cut at angle to fir rafters.	
	
04010	E-WF.13
	Framing a somewhat difficult structure cut up with windows, doors, closets and the like.	
	
04011	E-WF.13
	More difficult wall framing conditions.	
	
04012	E-WF.13
	Very difficult wall framing conditions.	
	
05000	E-WF.13
	Construct an interior non-bearing wall of 2x3's nailed 16" oc with a sole plate and one cap plate. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
05002	E-WF.13
	Construct an interior non-bearing wall of 2x3's nailed 24" oc with a sole plate and one cap plate. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
05003	E-WF.13
	Construct an interior non-bearing wall of 2x4's nailed 16" oc with a sole plate and one cap plate. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
05004	E-WF.13
	Construct an interior non-bearing wall of 2x4's nailed 24" oc with a sole plate and one cap plate. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
05005	E-WF.13
	Construct an interior non-bearing wall of 2x6's nailed 16" oc with a sole plate and one cap plate. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
05006	E-WF.13
	Construct an interior non-bearing wall of 2x6's nailed 16" oc with a sole plate and one cap plate. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
05100	E-WF.13
	Apply 1x2 wood furring over existing framing 16" oc. Lumber shall be kiln dried #3 Hem-Fir/Southern Pine/Douglas Fir.	
	
05101	E-WF.13
	Apply 1x3 wood furring over existing framing 16" oc. Lumber shall be kiln dried #3 Hem-Fir/Southern Pine/Douglas Fir.	
	
05102	E-WF.13
	Apply 1x2 wood furring over existing framing 24" oc. Lumber shall be kiln dried #3 Hem-Fir/Southern Pine/Douglas Fir.	
	
05103	E-WF.13
	Apply 1x3 wood furring over existing framing 24" oc. Lumber shall be kiln dried #3 Hem-Fir/Southern Pine/Douglas Fir.	
	
05104	E-WF.13
	Apply 1x2 wood furring over existing masonry 16" oc. Lumber shall be kiln dried #3 Hem-Fir/Southern Pine/Douglas Fir.	
	
05105	E-WF.13
	Apply 1x3 wood furring over existing masonry 16" oc. Lumber shall be kiln dried #3 Hem-Fir/Southern Pine/Douglas Fir.	
	
05106	E-WF.13
	Apply 1x2 wood furring over existing masonry 16" oc. Lumber shall be kiln dried #3 Hem-Fir/Southern Pine/Douglas Fir.	
	
05107	E-WF.13
	Apply 1x3 wood furring over existing masonry 24" oc. Lumber shall be kiln dried #3 Hem-Fir/Southern Pine/Douglas Fir.	
	
01000	E-WF.14
	Construct a gable type roof structure including a 12 inch overhang and eaves using 2x6 roof rafters nailed 16" oc with  rafter headers as needed. Headers as required may be solid or laminated and sized to code. Pitch of the roof to be between 3 inches in 12 and 4 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01001	E-WF.14
	Construct a gable type roof structure including a 12 inch overhang and eaves using 2x6 roof rafters nailed 16" oc with  rafter headers as needed. Headers as required may be solid or laminated and sized to code. Pitch of the roof to be between 3 inches in 12 and 6 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01002	E-WF.14
	Construct a gable type roof structure including a 12 inch overhang and eaves using 2x6 roof rafters nailed 16" oc with  rafter headers as needed. Headers as required may be solid or laminated and sized to code. Pitch of the roof to be between 7 inches in 12 and 10 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01003	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x8 roof rafters nailed 16" oc with  rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to between 9 inches in 12 and 10 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01004	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x8 roof rafters nailed 16" oc with  rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 11 inches in 12 and 12 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01005	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x8 roof rafters nailed 16" oc with  rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to between 3 inches in 12 and 4 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01006	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x8 roof rafters nailed 16" oc with  rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to between 3 inches in 12 and 6 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01007	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x8 roof rafters nailed 16" oc with  rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to between 7 inches in 12 and 8 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01008	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x8 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 9 inches in 12 and 10 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01009	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x8 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 11 inches in 12 and 12 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01010	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x10 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 3 inches in 12 and 4 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01013	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x12 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 3 inches in 12 and 4 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01014	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x10 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 5 inches in 12 and 6 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01015	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x10 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 7 inches in 12 and 8 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01016	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x10 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 97 inches in 12 and 10 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01020	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x12 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 11 inches in 12 and 12 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01022	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x12 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 11 inches in 12 and 12 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01023	E-WF.14
	Construct a gambrel type roof structure including the overhang and soffit framing, constructed out of 2x6 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01024	E-WF.14
	Construct a gambrel type roof structure including the overhang and soffit framing, constructed out of 2x8 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01025	E-WF.14
	Construct a gable type roof structure including the overhang and eaves, constructed out of 2x12 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 11 inches in 12 and 12 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01100	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x6 roof joists nailed 16" oc with joist headers as needed. The installation to be on a roof with a pitch of less than 4 inches in 12 inches. There will be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code.  Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01101	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x6 roof joists nailed 16" oc with joist headers as needed. The installation to be on a roof with a pitch between 3 inches in 12 inches and 4 inches in 12 inches. There will be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01102	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x6 roof joists nailed 16" oc with joist headers as needed. The installation to be on a roof with a pitch between 5 inches in 12 inches and 6 inches in 12 inches. There will be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01103	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x6 roof joists nailed 16" oc with joist headers as needed. The installation to be on a roof with a pitch between 7 inches in 12 inches and 8 inches in 12 inches. There will be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01104	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x6 roof joists nailed 16" oc with joist headers as needed. The installation to be on a roof with a pitch greater than 9 inches in 12 inches. There will be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01105	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x6 roof joists nailed 16" oc with joist headers as needed. The installation to be on a roof with a pitch greater than 11 inches in 12 inches. There will be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01106	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x8 roof joists nailed 16" oc with joist headers as needed. Framing to be on a roof with a pitch less than 3 inches in 12 inches. There is to be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01107	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x8 roof joists nailed 16" oc with joist headers as needed. Framing to be on a roof with a pitch less than 4 inches in 12 inches. There is to be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01108	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x8 roof joists nailed 16" oc with joist headers as needed. Framing to be on a roof with a pitch less than 6 inches in 12 inches. There is to be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01109	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x8 roof joists nailed 16" oc with joist headers as needed. Framing to be on a roof with a pitch less than 8 inches in 12 inches. There is to be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01110	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x8 roof joists nailed 16" oc with joist headers as needed. Framing to be on a roof with a pitch greater than 9 inches in 12 inches. There is to be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01111	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x8 roof joists nailed 16" oc with joist headers as needed. Framing to be on a roof with a pitch greater than 11 inches in 12 inches. There is to be a 12 inch overhang unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01112	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x10 roof joists nailed 16" oc with joist headers as needed. Roof pitch is less than 3 inches in 12 inches.  There is to be overhang of 12 inches unless specified.  Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01113	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x10 roof joists nailed 16" oc with joist headers as needed. Roof pitch is less than 4 inches in 12 inches.  There is to be overhang of 12 inches unless specified.  Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01114	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x10 roof joists nailed 16" oc with joist headers as needed. Roof pitch is between 5 inches and 6 inches in 12 inches.  There is to be overhang of 12 inches unless specified.  Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01115	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x10 roof joists nailed 16" oc with joist headers as needed. Roof pitch is between 7 inches and 8 inches in 12 inches.  There is to be overhang of 12 inches unless specified.  Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01116	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x10 roof joists nailed 16" oc with joist headers as needed. Roof pitch is greater than 9 inches in 12 inches.  There is to be overhang of 12 inches unless specified.  Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01117	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x10 roof joists nailed 16" oc with joist headers as needed. Roof pitch is greater than 11 inches in 12 inches.  There is to be overhang of12 inches unless specified.  Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01118	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x12 roof joists nailed 16" oc with joist headers as needed. This task assumes roof pitch is under 3 inches in 12 inches.  There is to be an overhang of 12 inches unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01119	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x12 roof joists nailed 16" oc with joist headers as needed. This task assumes roof pitch is under 4 inches in 12 inches.  There is to be an overhang of 12 inches unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01120	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x12 roof joists nailed 16" oc with joist headers as needed. This task assumes roof pitch is between 5 inches and 8 inches in 12 inches.  There is to be an overhang of 12 inches unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01121	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x12 roof joists nailed 16" oc with joist headers as needed. This task assumes roof pitch is between 7 inches and 8 inches in 12 inches.  There is to be an overhang of 12 inches unless specified. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01122	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x12 roof joists nailed 16" oc with joist headers as needed. This task assumes roof pitch is between 9 inches and 10 inches in 12 inches.  There is to be an overhang of 12 inches unless specified. Headers as required may be solid or laminated and sized to Code.  Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01123	E-WF.14
	Construct a flat or shed type roof structure including the overhang and eaves, constructed out of 2x12 roof joists nailed 16" oc with joist headers as needed. This task assumes roof pitch is between 11 inches and 10 inches in 12 inches.  There is to be an overhang of 12 inches unless specified. Headers as required may be solid or laminated and sized to Code.  Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01200	E-WF.14
	Install 2x6 ceiling joists 16" oc in the roof structure, including blocking for drywall or lath. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01201	E-WF.14
	Install 2x8 ceiling joists 16" oc in the roof structure, including blocking for drywall or lath. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01202	E-WF.14
	Install 2x10 ceiling joists 16" oc in the roof structure, including blocking for drywall or lath. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01203	E-WF.14
	Install 2x12 ceiling joists 16" oc in the roof structure, including blocking for drywall or lath. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01204	E-WF.14
	Install 2x6 ceiling joists 24" oc in the roof structure, including blocking for drywall or lath. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01205	E-WF.14
	Install 2x8 ceiling joists 24" oc in the roof structure, including blocking for drywall or lath. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01206	E-WF.14
	Install 2x10 ceiling joists 24" oc in the roof structure, including blocking for drywall or lath. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01207	E-WF.14
	Install 2x12 ceiling joists 24" oc in the roof structure, including blocking for drywall or lath. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01300	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x6 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Roof pitch between 3 inch and 4 inch in 12.	
	
01301	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x6 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir. Roof pitch to be between 5 inch and 6 inch in 12.	
	
01302	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x6 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 7 inches and 8 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01303	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x6 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 97 inches and 10 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01304	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x6 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 11 inches and 12 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01305	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x8 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 3 inches and 4 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01306	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x8 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 53 inches and 6 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01307	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x8 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 7 inches and 8 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01308	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x8 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 9 inches and 10 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01309	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x8 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 11 inches and 12 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01310	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x10 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 3 inches and 4 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01311	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x10 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 4 inches and 6 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01312	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x10 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 7 inches and 8 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01313	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x10 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 9 inches and 10 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01314	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x10 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 11 inches and 12 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01315	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x12 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 3inches and 4 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01316	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x12 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 5 inches and 6 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01317	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x12 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 7inches and 8 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01318	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x12 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 9 inches and 10 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01319	E-WF.14
	Construct a hip type roof structure including the overhang and soffit framing, constructed out of 2x12 roof rafters nailed 16" oc with rafter headers as needed. Headers as required may be solid or laminated and sized to code. Roof pitch to be between 11 inches and 12 inches in 12. Included in this roof framing are the necessary bird or freeze blocks. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01700	E-WF.14
	Install a gable style roof using 4x8 rafters, 48" oc with framing for the overhang and eaves. The rafters are covered with 2x6 tongue and groove sheathing that will be exposed on the underside of the roof structure. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.  Installation to include 2" rigid foam insulation and 1/2 " CDX plywood sheathing over the planks.	
	
01701	E-WF.14
	Install a gable style roof using 4x8 rafters, 48" oc with framing for the overhang and eaves. The rafters are covered with 2x6 tongue and groove sheathing that will be exposed on the underside of the roof structure. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.  Installation to include 2" rigid foam insulation and 1/2 " CDX plywood sheathing over the planks.	
	
01702	E-WF.14
	Install a gable style roof using 4x8 rafters, 48" oc with framing for the overhang and eaves. The rafters are covered with 2x6 tongue and groove sheathing that will be exposed on the underside of the roof structure. Lumber shall be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.  Installation to include 2" rigid foam insulation and 1/2 " CDX plywood sheathing over the planks.	
	
01703	E-WF.14
	Construct framing to support 18" soffit. Lumber to be kiln dried#2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01704	E-WF.14
	Construct framing to support 18" soffit. Lumber to be kiln dried#2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
01705	E-WF.14
	Construct framing to support 24" soffit. Lumber to be kiln dried #2 or better Hem-Fir/Southern Pine/Douglas Fir.	
	
02500	E-WF.14
	Add a dormer to new roof construction. Includes rafters, ridgeboard, ceiling joists, studs, plates and sheathing.	
	
02501	E-WF.14
	Add a dormer to new roof construction. Includes rafters, ridgeboard, ceiling joists, studs, plates and sheathing.	
	
03600	E-WF.14
	Plywood sheathing,3/8" CDX installed over roof rafters or joists, including aluminum plywood clips.  Roof pitch is under 4 inches in 12.	
	
03601	E-WF.14
	Plywood sheathing,3/8" CDX installed over roof rafters or joists, including aluminum plywood clips.  Roof pitch is under 6 inches in 12.	
	
03602	E-WF.14
	Plywood sheathing,3/8" CDX installed over roof rafters or joists, including aluminum plywood clips.	
	
03603	E-WF.14
	Plywood sheathing,3/8" CDX installed over roof rafters or joists, including aluminum plywood clips.  Roof pitch is greater than 9 inches in 12.	
	
03604	E-WF.14
	Plywood sheathing,3/8" CDX installed over roof rafters or joists, including aluminum plywood clips.  Roof pitch is greater than 11 inches in 12.	
	
03605	E-WF.14
	Plywood sheathing,1/2" CDX installed over roof rafters or joists, including aluminum plywood clips.  Roof pitch to be under 4 inches in 12.	
	
03606	E-WF.14
	Plywood sheathing,1/2" CDX installed over roof rafters or joists, including aluminum plywood clips.  Roof pitch to be between 5 inches and 6 inches in 12.	
	
03607	E-WF.14
	Plywood sheathing,1/2" CDX installed over roof rafters or joists, including aluminum plywood clips.  Roof pitch to be between 5 and 8 inches in 12.	
	
03608	E-WF.14
	Plywood sheathing,1/2" CDX installed over roof rafters or joists, including aluminum plywood clips.  Roof pitch to be between 9 inches and 10 inches in 12.	
	
03610	E-WF.14
	Plywood sheathing,1/2" CDX installed over roof rafters or joists, including aluminum plywood clips.  Roof pitch to be greater than 11 inches in 12.	
	
03611	E-WF.14
	Plywood sheathing 5/8" CDX installed over roof rafters or joists. Roof pitch to be under 4 inches in 12.	
	
03612	E-WF.14
	Plywood sheathing 5/8" CDX installed over roof rafters or joists. Roof pitch to be between  5 inches and 6 inches in 12.	
	
03613	E-WF.14
	Plywood sheathing 5/8" CDX installed over roof rafters or joists. Roof pitch to be between 5 inches and 8 in 12.	
	
03614	E-WF.14
	Plywood sheathing 5/8" CDX installed over roof rafters or joists. Roof pitch to be between 9 inches and 10 inches in 12.	
	
03615	E-WF.14
	Plywood sheathing 5/8" CDX installed over roof rafters or joists. Roof pitch to be greater than 11 inches in 12.	
	
03616	E-WF.14
	Plywood sheathing 3/4" CDX installed over roof rafters or joists.  Roof pitch to be under 4 inches in 12.	
	
03617	E-WF.14
	Plywood sheathing 3/4" CDX installed over roof rafters or joists.  Roof pitch to be under between 5 inches and 6 inches in12.	
	
03618	E-WF.14
	Plywood sheathing 3/4" CDX installed over roof rafters or joists.  Roof pitch to be between 5 inches and 8 inches in 12.	
	
03619	E-WF.14
	Plywood sheathing 3/4" CDX installed over roof rafters or joists.  Roof pitch to be between 9 inches and 10 inches in 12.	
	
03620	E-WF.14
	Plywood sheathing 3/4" CDX installed over roof rafters or joists.  Roof pitch to be greater than 11 inches in 12.	
	
03630	E-WF.14
	Solid wood strip sheathing, 1x3 installed 5 1/2" oc over roof rafters or joists. Sheathing to be applied horizontally. Lumber shall be kiln dried #3 or better Hem-Fir/Southern Pine/Douglas Fir.  Roof pitch between 3 inches and 4 inches in 12.	
	
03631	E-WF.14
	Solid wood strip sheathing, 1x3 installed 5 1/2" oc over roof rafters or joists. Sheathing to be applied horizontally. Lumber shall be kiln dried #3 or better Hem-Fir/Southern Pine/Douglas Fir.  Roof pitch between 5 inches and 6 inches in 12.	
	
03632	E-WF.14
	Solid wood strip sheathing, 1x3 installed 5 1/2" oc over roof rafters or joists. Sheathing to be applied horizontally. Lumber shall be kiln dried #3 or better Hem-Fir/Southern Pine/Douglas Fir.  Roof pitch between 7 inches and 8 inches in 12.	
	
03633	E-WF.14
	Solid wood strip sheathing, 1x3 installed 5 1/2" oc over roof rafters or joists. Sheathing to be applied horizontally. Lumber shall be kiln dried #3 or better Hem-Fir/Southern Pine/Douglas Fir.  Roof pitch between 9 inches and 10 inches in 12.	
	
03634	E-WF.14
	Solid wood strip sheathing, 1x3 installed 5 1/2" oc over roof rafters or joists. Sheathing to be applied horizontally. Lumber shall be kiln dried #3 or better Hem-Fir/Southern Pine/Douglas Fir.  Roof pitch between 11 inches and 12 inches in12.	
	
03635	E-WF.14
	Solid wood strip sheathing, 1x3 installed 7 1/2" oc over roof rafters or joists. Sheathing to be applied horizontally. Lumber shall be kiln dried #3 or better Hem-Fir/Southern Pine/Douglas Fir. Roof pitch under 4 inches in 12.	
	
03636	E-WF.14
	Solid wood strip sheathing, 1x3 installed 7 1/2" oc over roof rafters or joists. Sheathing to be applied horizontally. Lumber shall be kiln dried #3 or better Hem-Fir/Southern Pine/Douglas Fir. Roof pitch to be between 5 inches and 6 inches in 12.	
	
03637	E-WF.14
	Solid wood strip sheathing, 1x3 installed 7 1/2" oc over roof rafters or joists. Sheathing to be applied horizontally. Lumber shall be kiln dried #3 or better Hem-Fir/Southern Pine/Douglas Fir. Roof pitch to be between 5 inches and 8 inches in 12.	
	
03638	E-WF.14
	Solid wood strip sheathing, 1x3 installed 7 1/2" oc over roof rafters or joists. Sheathing to be applied horizontally. Lumber shall be kiln dried #3 or better Hem-Fir/Southern Pine/Douglas Fir. Roof pitch to be between 9 inches and 10 inches in 12.	
	
03639	E-WF.14
	Solid wood strip sheathing, 1x3 installed 7 1/2" oc over roof rafters or joists. Sheathing to be applied horizontally. Lumber shall be kiln dried #3 or better Hem-Fir/Southern Pine/Douglas Fir. Roof pitch to be greater than 11 inches in 12.	
	
04400	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 16" oc.  Truss to be placed either by crane or by hand on a roof pitch 3 inches in 12 inches.	
	
04401	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 16" oc.  Truss to be placed either by crane or by hand on a roof pitch 4 inches in 12 inches.	
	
04402	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 16" oc.  Truss to be placed either by crane or by hand on a roof pitch 5 inches in 12 inches.	
	
04403	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 16" oc.  Truss to be placed either by crane or by hand on a roof pitch 6 inches in 12 inches.	
	
04404	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 16" oc.  Truss to be placed either by crane or by hand on a roof pitch 7 inches in 12 inches.	
	
04405	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 24" oc.  Truss to be placed either by crane or by hand on a roof pitch 7 inches in 12 inches.	
	
04406	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 24" oc.  Truss to be placed either by crane or by hand on a roof pitch 3 inches in 12 inches.	
	
04407	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 24" oc.  Truss to be placed either by crane or by hand on a roof pitch 4 inches in 12 inches.	
	
04408	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 24" oc.  Truss to be placed either by crane or by hand on a roof pitch 5 inches in 12 inches.	
	
04409	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 24" oc.  Truss to be placed either by crane or by hand on a roof pitch 6 inches in 12 inches.	
	
04410	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 24" oc.  Truss to be placed either by crane or by hand on a roof pitch 7 inches in 12 inches.	
	
04411	E-WF.14
	Construct any type roof structure including the overhang, soffit and eave framing using pre-built roof trusses nailed 24" oc.  Truss to be placed either by crane or by hand on a roof pitch 7 inches in 12 inches.	
	
01003	E-WF.15
	Install Cedar beveled siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper. 1/2" x 4" siding installed horizontally. Includes starter strips and 5/4" by 4" outside corners and 5/4" x 5/4" inside corners. Install with galvanized nails.	
	
01004	E-WF.15
	Install Redwood or Cedar beveled siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper. 1/2" x 6" siding installed horizontally. Includes starter strips and 5/4 by 4 outside corners and 5/4 x 5/4 inside corners. Install with galvanized nails.	
	
01005	E-WF.15
	Install Redwood or Cedar beveled siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper. 1/2" x 8" siding installed horizontally. Includes starter strips and 5/4 by 4 outside corners and 5/4 x 5/4 inside corners. Install with galvanized nails.	
	
01006	E-WF.15
	Install Redwood or Cedar beveled siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper. 3/4" x 8" siding installed horizontally. Includes starter strips and 5/4 by 4 outside corners and 5/4 x 5/4 inside corners. Install with galvanized nails.	
	
01007	E-WF.15
	Install Redwood or Cedar beveled siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper. 3/4" x 10" siding installed horizontally. Includes starter strips and 5/4 by 4 outside corners and 5/4 x 5/4 inside corners. Install with galvanized nails.	
	
01008	E-WF.15
	Install Redwood beveled siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper. 1/2" x 4" siding installed horizontally. Includes starter strips and 5/4" by 4" outside corners and 5/4" x 5/4" inside corners. Install with galvanized nails.	
	
01009	E-WF.15
	Install Redwood beveled siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper. 1/2" x 6" siding installed horizontally. Includes starter strips and 5/4 by 4 outside corners and 5/4 x 5/4 inside corners. Install with galvanized nails.	
	
01010	E-WF.15
	Install Redwood beveled siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper. 1/2" x 8" siding installed horizontally. Includes starter strips and 5/4 by 4 outside corners and 5/4 x 5/4 inside corners. Install with galvanized nails.	
	
01011	E-WF.15
	Install Redwood beveled siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper. 3/4" x 8" siding installed horizontally. Includes starter strips and 5/4 by 4 outside corners and 5/4 x 5/4 inside corners. Install with galvanized nails.	
	
01012	E-WF.15
	Install Redwood beveled siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper. 3/4" x 10" siding installed horizontally. Includes starter strips and 5/4 by 4 outside corners and 5/4 x 5/4 inside corners. Install with galvanized nails.	
	
01013	E-WF.15
	Install Cedar Board and Batten Siding on existing sheathing or braced stud wall over 15 lb. felt or rosin coated paper 1 x 8" siding installed vertically. Includes starter strips and 3/4 by 4 outside corners and 3/4 x 3/4 inside corners. Install with galvanized nails.	
	
01014	E-WF.15
	Install Cedar Board and Batten Siding on existing sheathing or braced stud wall over 15 lb. felt or rosin coated paper 1 x 10" siding installed vertically. Includes starter strips and 3/4 by 4 outside corners and 3/4 x 3/4 inside corners. Install with galvanized nails.	
	
01015	E-WF.15
	Install Cedar Board and Batten Siding on existing sheathing or braced stud wall over 15 lb. felt or rosin coated paper 1 x 12" siding installed vertically. Includes starter strips and 3/4 by 4 outside corners and 3/4 x 3/4 inside corners. Install with galvanized nails.	
	
01016	E-WF.15
	Install Redwood Board and Batten Siding on existing sheathing or braced stud wall over 15 lb. felt or rosin coated paper 1 x 8" siding installed vertically. Includes starter strips and 3/4 by 4 outside corners and 3/4 x 3/4 inside corners. Install with galvanized nails.	
	
01017	E-WF.15
	Install Redwood Board and Batten Siding on existing sheathing or braced stud wall over 15 lb. felt or rosin coated paper 1 x 10" siding installed vertically. Includes starter strips and 3/4 by 4 outside corners and 3/4 x 3/4 inside corners. Install with galvanized nails.	
	
01018	E-WF.15
	Install Redwood Board and Batten Siding on existing sheathing or braced stud wall over 15 lb. felt or rosin coated paper 1 x 12" siding installed vertically. Includes starter strips and 3/4 by 4 outside corners and 3/4 x 3/4 inside corners. Install with galvanized nails.	
	
01021	E-WF.15
	Install Cedar tongue & groove siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper.  1 x 8"siding installed vertically. Includes starter strips and 3/4 by 4 outside corners and 3/4 x 3/4 inside corners. Install with galvanized nails.	
	
01022	E-WF.15
	Install Cedar tongue & groove siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper.  1 x 10" siding installed vertically. Includes starter strips and 3/4by 4 outside corners and 3/4 x 3/4 inside corners. Install with galvanized nails.	
	
01025	E-WF.15
	Install Redwood tongue & groove siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper.  1 x 8"siding installed vertically. Includes starter strips and 3/4 by 4 outside corners and 3/4 x 3/4 inside corners. Install with galvanized nails.	
	
01026	E-WF.15
	Install Redwood tongue & groove siding on existing sheath or braced stud wall over 15 lb. felt or rosin coated paper.  1 x 10" siding installed vertically. Includes starter strips and 3/4by 4 outside corners and 3/4 x 3/4 inside corners. Install with galvanized nails.	
	
01037	E-WF.15
	Install Drip Cap and 1 x 4 Water Table under the first course of siding.	
	
01101	E-WF.15
	Install 16" Cedar Shingles over wood sheath walls. Shingles to be installed over 15 lb. felt or rosin coated paper with 3d galvanized nails with both inside and outside corners to be woven and shingles installed with a 7 1/2" exposure.	
	
01103	E-WF.15
	Install 16" Fire Retardant Cedar Shingles over wood sheath walls. Shingles to be installed over 15 lb. felt or rosin coated paper with 3d galvanized nails with both inside and outside   corners to be woven and shingles installed with a 7 1/2" exposure.	
	
01105	E-WF.15
	Install 18" Cedar Shingles over wood sheath walls. Shingles to be installed over 15 lb. felt or rosin coated paper with 3d galvanized nails with both inside and outside   corners to be woven and shingles installed with a 7 1/2" exposure.	
	
01108	E-WF.15
	Install 18" Fire Retardant Cedar Shingles over wood sheath walls. Shingles to be installed over 15 lb. felt or rosin coated paper with 3d galvanized nails with both inside and outside corners to be woven and shingles installed with a 7 1/2"exposure.	
	
01116	E-WF.15
	Install #1 Red Cedar Shakes or Shingles that have been manufactured as a panel 8'long and fasten to plywood sheathing to yield a 7" exposure. Panels to be installed over 15 lb. felt or rosin coated paper. Galvanized nails to be used.	
	
01300	E-WF.15
	Install Texture 1-11 Plywood panels with either 4", 6", or 8" OC patterns over 15 lb. felt or rosin filled paper. Use rough sawn 1 x 3 or 1 x 4 for inside and outside corner trim. Panels to be 4' x 8' sheets of 3/8" cedar plywood. All panels to be installed with galvanized nails.	
	
01301	E-WF.15
	Install Texture 1-11 Plywood panels with either 4", 6", or 8" OC patterns over 15 lb. felt or rosin filled paper. Use rough sawn 1 x 3 or 1 x 4 for inside and outside corner trim. Panels to be 4' x 8' sheets of 5/8" cedar plywood. All panels to be installed with galvanized nails.	
	
01302	E-WF.15
	Install Texture 1-11 Plywood panels with either 4", 6", or 8" OC patterns over 15 lb. felt or rosin filled paper. Use rough sawn 1 x 3 or 1 x 4 for inside and outside corner trim. Panels to be 4' x 8' sheets of 3/8" redwood plywood. All panels to be installed with galvanized nails.	
	
01303	E-WF.15
	Install Texture 1-11 Plywood panels with either 4", 6", or 8" OC patterns over 15 lb. felt or rosin filled paper. Use rough sawn 1 x 3 or 1 x 4 for inside and outside corner trim. Panels to be 4' x 8' sheets of 5/8" redwood plywood. All panels to be installed with galvanized nails.	
	
01304	E-WF.15
	Install Texture 1-11 Plywood panels with either 4", 6", or 8" OC patterns over 15 lb. felt or rosin filled paper. Use rough sawn 1 x 3 or 1 x 4 for inside and outside corner trim. Panels to be 4' x 8' sheets of 3/8" fir plywood. All panels to be installed with galvanized nails.	
	
01305	E-WF.15
	Install Texture 1-11 Plywood panels with either 4", 6", or 8" OC patterns over 15 lb. felt or rosin filled paper. Use rough sawn 1 x 3 or 1 x 4 for inside and outside corner trim. Panels to be 4' x 8' sheets of 5/8" fir plywood. All panels to be installed with galvanized nails.	
	
01306	E-WF.15
	Install Texture 1-11 Plywood panels with either 4", 6", or 8" OC patterns over 15 lb. felt or rosin filled paper. Use rough sawn 1 x 3 or 1 x 4 for inside and outside corner trim. Panels to be 4' x 8' sheets of 3/8" pine plywood. All panels to be installed with galvanized nails.	
	
01307	E-WF.15
	Install Texture 1-11 Plywood panels with either 4", 6", or 8" OC patterns over 15 lb. felt or rosin filled paper. Use rough sawn 1 x 3 or 1 x 4 for inside and outside corner trim. Panels to be 4' x 8' sheets of 5/8" pine plywood. All panels to be installed with galvanized nails.	
	
02400	E-WF.15
	Install aluminum siding over sheathed subwalls. Siding to be .024 gauge applied over 15 lb. felt or rosin paper with insulation board backing. Siding to be 8" smooth horizontal aluminum siding to include all accessories such as inside and outside corners. Siding to be installed with aluminum nails, not driven in tightly so that siding panels hang on the nail and allow for expansion and contraction.	
	
02401	E-WF.15
	Install aluminum siding over sheathed subwalls. Siding to be .024 gauge applied over 15 lb. felt or rosin paper with insulation board backing. Siding to be 8" double 4 finish horizontal aluminum siding to include all accessories such as inside and outside corners. Siding to be installed with aluminum nails, not driven in tightly so that siding panels hang on the nail and  allow for expansion and contraction.	
	
02402	E-WF.15
	Install aluminum siding over sheathed subwalls. Siding to be .024 gauge applied over 15 lb. felt or rosin paper with insulation board backing. Siding to be 10" smooth horizontal aluminum siding to include all accessories such as inside and outside corners. Siding to be installed with aluminum nails, not driven in tightly so that siding panels hang on the nail and  allow for expansion and contraction.	
	
02403	E-WF.15
	Install aluminum siding over sheathed subwalls. Siding to be .024 gauge applied over 15 lb. felt or rosin paper with insulation board backing. Siding to be 10" double 5 finish horizontal aluminum siding to include all accessories such as inside and outside corners. Siding to be installed with aluminum nails, not driven in tightly so that siding panels hang on the nail and  allow for expansion and contraction.	
	
02404	E-WF.15
	Install aluminum siding over sheathed subwalls. Siding to be .024 gauge applied over 15 lb. felt or rosin paper with insulation board backing. Siding to be 12" vertical board and batten aluminum siding to include all accessories such as inside and outside corners. Siding to be installed with aluminum nails, not driven in tightly so that siding panels hang on the nail and allow for expansion and contraction.	
	
04200	E-WF.15
	Install Hardboard Lap Siding on wood sheathing. Siding to be 7/16" thick installed over 15 lb. felt or rosin coated paper with 5/4" x 4" outside corners and 5/4" x 5/4" inside corners with corner material to be rough sawn cedar. Hardboard siding to be 8" wide by 16' lengths and shall be primed before installation.	
	
04201	E-WF.15
	Install Hardboard Lap Siding on wood sheathing. Siding to be 7/16" thick installed over 15 lb. felt or rosin coated paper with 5/4" x 4" outside corners and 5/4" x 5/4" inside corners with corner material to be rough sawn cedar. Hardboard siding to be 12" wide by 16' lengths and shall be primed before installation.	
	
04202	E-WF.15
	Install Hardboard Lap Siding on wood sheathing. Siding to be 7/16" thick installed over 15 lb. felt or rosin coated paper with 5/4" x 4" outside corners and 5/4" x 5/4" inside corners with corner material to be rough sawn cedar. Hardboard siding to be 8" wide by 16' lengths and shall be prefinished before installation.	
	
04203	E-WF.15
	Install Hardboard Lap Siding on wood sheathing. Siding to be 7/16" thick installed over 15 lb. felt or rosin coated paper with 5/4" x 4" outside corners and 5/4" x 5/4" inside corners with corner material to be rough sawn cedar. Hardboard siding to be 12" wide by 16' lengths and shall be prefinished before installation.	
	
07501	E-WF.15
	Install cementatious stucco that has been fortified with plastic cement mortar over frame wall with studs to be 16" oc and with a minimum of 1/2" sheathing.  Stucco to be applied in three coats one inch thick.	
	
08405	E-WF.15
	Install solid PVC vinyl siding over sheath subwall with insulation board backing. Siding to be installed over 15 lb. felt or rosin paper. Siding panels to be 8" smooth finish and to include all accessories such as inside and outside corners and starter strip. Siding to be nailed with aluminum or galvanized nails, nails to be installed loosely so that siding hangs on nails and allows for expansion and contraction.	
	
08406	E-WF.15
	Install solid PVC vinyl siding over sheath subwall with insulation board backing. Siding to be installed over 15 lb. felt or rosin paper. Siding panels to be 8" double 4 finish and to include all accessories such as inside and outside corners and starter strip. Siding to be nailed with aluminum or galvanized nails, nails to be installed loosely so that siding hangs on nails and allows for expansion and contraction.	
	
08407	E-WF.15
	Install solid PVC vinyl siding over sheath subwall with insulation board backing. Siding to be installed over 15 lb. felt or rosin paper. Siding panels to be 10" smooth finish and to include all accessories such as inside and outside corners and starter strip. Siding to be nailed with aluminum or galvanized nails, nails to be installed loosely so that siding hangs on nails and allows for expansion and contraction.	
	
08408	E-WF.15
	Install solid PVC vinyl siding over sheath subwall with insulation board backing. Siding to be installed over 15 lb. felt or rosin paper. Siding panels to be 10" double 5 finish and to include all accessories such as inside and outside corners  and starter strip. Siding to be nailed with aluminum or galvanized nails, nails to be installed loosely so that siding hangs on nails and allows for expansion and contraction.	
	
01010	E-WF.16
	Install redwood cupola on roof.  The cupola will 24" by 24" and have an aluminum roof.	
	
01011	E-WF.16
	Install redwood cupola on roof.  The cupola will 30" by 30" and have an aluminum roof.	
	
01012	E-WF.16
	Install redwood cupola on roof.  The cupola will be 36" by 36" and have an aluminum roof.	
	
01013	E-WF.16
	Install redwood cupola on roof.  The cupola will 24" by 24" and have a copper roof.	
	
01014	E-WF.16
	Install redwood cupola on roof.  The cupola will 30" by 30" and have a copper roof.	
	
01015	E-WF.16
	Install redwood cupola on roof.  The cupola will be 36" by 36" and have a copper roof.	
	
03010	E-WF.16
	Install 3/8" Fir plywood and 2x4 framing members to form a 12" boxed eave at the gutter end of trussed or framed roof framing members forming an integral eave, gutter and facia.	
	
03011	E-WF.16
	Install 3/8" Fir plywood and 2x4 framing members to form a 16" boxed eave at the gutter end of trussed or framed roof framing members forming an integral eave, gutter and facia.	
	
03012	E-WF.16
	Install 3/8" Fir plywood and 2x4 framing members to form a 20" boxed eave at the gutter end of trussed or framed roof framing members forming an integral eave, gutter and facia.	
	
03013	E-WF.16
	Install 3/8" Fir plywood and 2x4 framing members to form a 24" boxed eave at the gutter end of trussed or framed roof framing members forming an integral eave, gutter and facia.	
	
03014	E-WF.16
	Apply as required 3/4" x 1 5/8" Pine/Fir/Hemlock (paint grade) molding with galvanized nails, prime as quickly as appropriate.	
	
03015	E-WF.16
	Apply as required 3/4" x 2 1/4" Pine/Fir/Hemlock (paint grade) molding with galvanized nails, prime as quickly as appropriate.	
	
03016	E-WF.16
	Apply as required 3/4" x 3 1/4" Pine/Fir/Hemlock (paint grade) molding with galvanized nails, prime as quickly as appropriate.	
	
05000	E-WF.16
	Apply 1 x 6 #2 Pine/Spruce/Hemlock/Fir directly to the exposed rafter ends or frieze blocking. Fascia to be applied with galvanized nails and with all joints to be directly over a rafter end.	
	
05001	E-WF.16
	Apply 1 x 8 #2 Pine/Spruce/Hemlock/Fir directly to the exposed rafter ends or frieze blocking. Fascia to be applied with galvanized nails and with all joints to be directly over a rafter end.	
	
05002	E-WF.16
	Apply 1 x 10 #2 Pine/Spruce/Hemlock/Fir directly to the exposed rafter ends or frieze blocking. Fascia to be applied with galvanized nails and with all joints to be directly over a rafter end.	
	
05003	E-WF.16
	Apply 1 x 12 #2 Pine/Spruce/Hemlock/Fir directly to the exposed rafter ends or frieze blocking. Fascia to be applied with galvanized nails and with all joints to be directly over a rafter end.	
	
05004	E-WF.16
	Apply 2 x 6 #2 Pine/Spruce/Hemlock/Fir directly to the exposed rafter ends or frieze blocking. Fascia to be applied with galvanized nails and with all joints to be directly over a rafter end.	
	
05005	E-WF.16
	Apply 2 x 8 #2 Pine/Spruce/Hemlock/Fir directly to the exposed rafter ends or frieze blocking. Fascia to be applied with galvanized nails and with all joints to be directly over a rafter end.	
	
05006	E-WF.16
	Apply solid #2 Pine/Spruce/Hemlock/Fir soffit material to bottom side of the lower chord of the roof rafters 6" wide.	
	
05007	E-WF.16
	Apply solid #2 Pine/Spruce/Hemlock/Fir soffit material to bottom side of the lower chord of the roof rafters 8" wide.	
	
05008	E-WF.16
	Apply solid #2 Pine/Spruce/Hemlock/Fir soffit material to bottom side of the lower chord of the roof rafters 10" wide.	
	
05009	E-WF.16
	Apply solid #2 Pine/Spruce/Hemlock/Fir soffit material to bottom side of the lower chord of the roof rafters 12" wide.	
	
05010	E-WF.16
	Apply 3/8" Fir plywood of AC exterior grade soffit material to bottom side of the lower chord of the roof rafters 12" wide.	
	
05011	E-WF.16
	Apply 3/8" Fir plywood of AC exterior grade soffit material to bottom side of the lower chord of the roof rafters 16" wide.	
	
05012	E-WF.16
	Apply 3/8" Fir plywood of AC exterior grade soffit material to bottom side of the lower chord of the roof rafters 18" wide.	
	
05013	E-WF.16
	Apply 3/8" Fir plywood of AC exterior grade soffit material to bottom side of the lower chord of the roof rafters 24" wide.	
	
05014	E-WF.16
	Apply 3/8" Fir plywood of AC exterior grade soffit material to bottom side of the lower chord of the roof rafters 30" wide.	
	
05018	E-WF.16
	Apply #2 Pine/Fir/Hemlock 1 x 6 rake along gable ends of roof and install rake (shingle) molding. Rake and rake molding to be applied with galvanized nails.	
	
05020	E-WF.16
	Install pre-manufactured architectural cornice moulding manufactured out of expanded PVC as a single piece.  Individual molding piece to be installed in such a way that the joints overlap and joints are either coped or mitered. Nails are to be set and ready for finish.	
	
05021	E-WF.16
	Install architectural dentil moulding manufactured out of expanded PVC or other synthetic material as a single piece applied on top of existing cornice or trim.  Individual molding piece to be installed in such a way that the joints are either coped or mitered. Nails are to be set and ready for finish.	
	
07022	E-WF.16
	Install pre-assembled redwood lattice curtain wall. Lattice size to be 1/4" x 1 3/4" installed with 1 3/4" spacing.	
	
07023	E-WF.16
	Install custom made Lattice curtain wall with pressure treated kiln dried lumber. Lattice size to be 3/4" x 1 1/8" installed 2 1/4" on center.	
	
07024	E-WF.16
	Install custom made Lattice curtain wall with pressure treated kiln dried lumber. Lattice size to be 3/4" x 1 5/8" installed 3 1/4" on center.	
	
08100	E-WF.16
	Install Redwood Attic Louver including insect screens that are 24" in diameter. Box gable framing as required.	
	
08101	E-WF.16
	Install Redwood Attic Louver including insect screens that are half circle 30" x 18". Box gable framing as required.	
	
08102	E-WF.16
	Install Redwood Attic Louver including insect screens that are rectangular 16" x 14". Box gable framing as required.	
	
08112	E-WF.16
	Install gable louver vent 18 x 24" at center height. Box out gable framing as required.	
	
08113	E-WF.16
	Install gable louver vent 24 x 24" at center height. Box out gable framing as required.	
	
08114	E-WF.16
	Install aluminum rectangular louver 12" x 18" at center height. Box out gable framing as required.	
	
08115	E-WF.16
	Install aluminum rectangular louver 14" x 24" at center height. Box out gable framing as required.	
	
08116	E-WF.16
	Install aluminum rectangular louver 24" x 20" at center height. Box out gable framing as required.	
	
08117	E-WF.16
	Install adjustable gable vent.	
	
08118	E-WF.16
	Install adjustable gable vent.	
	
08119	E-WF.16
	Install foundation vent including insect screen, box framing as required, 6" x 14".	
	
08120	E-WF.16
	Install aluminum continuous soffit vents.	
	
03000	E-WF.17
	Install asphalt or fiberglass shingles that weigh between 215-225 lbs. per square(considered 20 year life wear) on a plain shed or gable wooden roof deck over  15# roofing felt paper with 5" wide galvanized metal drip edge on lower or gutter edge of the roof.  All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 7' rise in 12' run and 8' rise in 12' run.	
	
03001	E-WF.17
	Install asphalt or fiberglass shingles that weigh between 215-225 lbs. per square(considered 20 year life wear) on a plain shed or gable wooden roof deck over  15# roofing felt paper with 5" wide galvanized metal drip edge on lower or gutter edge of the roof.  All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 5' rise in 12' run and 6' rise in 12' run.	
	
03002	E-WF.17
	Install asphalt or fiberglass shingles that weigh between 215-225 lbs. per square (considered 20 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 7' rise in 12' run and 8' rise in 12' run.	
	
03003	E-WF.17
	Install asphalt or fiberglass shingles that weigh between 215-225 lbs. per square (considered 20 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 9' rise in 12' run and 10' rise in 12' run.	
	
03004	E-WF.17
	Install asphalt or fiberglass shingles that weigh between 215-225 lbs. per square (considered 20 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 11' rise in 12' run and12' rise in 12' run.	
	
03005	E-WF.17
	Install asphalt or fiberglass shingles that weigh 240 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 3' rise in 12' run and 4' rise in 12' run.	
	
03006	E-WF.17
	Install asphalt or fiberglass shingles that weigh 240 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 5' rise in 12' run and 6' rise in 12' run.	
	
03007	E-WF.17
	Install asphalt or fiberglass shingles that weigh 240 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 7' rise in 12' run and 8' rise in 12' run.	
	
03008	E-WF.17
	Install asphalt or fiberglass shingles that weigh 240 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 9' rise in 12' run and 10' rise in 12' run.	
	
03009	E-WF.17
	Install asphalt or fiberglass shingles that weigh 240 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 11' rise in 12' run and 12' rise in 12' run.	
	
03010	E-WF.17
	Install asphalt or fiberglass shingles that weigh 260 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 3' rise in 12' run and 6' rise in 12' run.	
	
03011	E-WF.17
	Install asphalt or fiberglass shingles that weigh 260 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 5' rise in 12' run and 6' rise in 12' run.	
	
03012	E-WF.17
	Install asphalt or fiberglass shingles that weigh 260 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 7' rise in 12' run and 8' rise in 12' run.	
	
03013	E-WF.17
	Install asphalt or fiberglass shingles that weigh 260 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 9' rise in 12' run and 10' rise in 12' run.	
	
03014	E-WF.17
	Install asphalt or fiberglass shingles that weigh 260 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 11' rise in 12' run and 12' rise in 12' run.	
	
03018	E-WF.17
	Install asphalt or fiberglass shingles that weigh 300 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 3' rise in 12' run and 6' rise in 12' run.	
	
03019	E-WF.17
	Install asphalt or fiberglass shingles that weigh 300 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 5' rise in 12' run and 6' rise in 12' run.	
	
03020	E-WF.17
	Install asphalt or fiberglass shingles that weigh 300 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 7' rise in 12' run and 8' rise in 12' run.	
	
03021	E-WF.17
	Install asphalt or fiberglass shingles that weigh 300 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 9' rise in 12' run and 10' rise in 12' run.	
	
03022	E-WF.17
	Install asphalt or fiberglass shingles that weigh 300 lbs. per square (considered 25 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 11' rise in 12' run and 12' rise in 12' run.	
	
03023	E-WF.17
	Install asphalt or fiberglass shingles that weigh 375 lbs. per square (considered 30 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 3' rise in 12' run and 6' rise in 12' run.	
	
03024	E-WF.17
	Install asphalt or fiberglass shingles that weigh 375 lbs. per square (considered 30 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 5' rise in 12' run and 6' rise in 12' run.	
	
03025	E-WF.17
	Install asphalt or fiberglass shingles that weigh 375 lbs. per square (considered 30 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 7' rise in 12' run and 8' rise in 12' run.	
	
03026	E-WF.17
	Install asphalt or fiberglass shingles that weigh 375 lbs. per square (considered 30 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 9' rise in 12' run and 10' rise in 12' run.	
	
03027	E-WF.17
	Install asphalt or fiberglass shingles that weigh 375 lbs. per square (considered 30 year wear life) on a plain shed or gable wooden roof deck over 15 # roofing felt paper with 5 inch wide galvanized metal drip edge on lower or gutter edge of the roof. All fasteners, whether nails or staples are to be galvanized and applied 4 fasteners per three butt self sealing shingle. Roof slope is between a 11' rise in 12' run and 12' rise in 12' run.	
	
03032	E-WF.17
	Install asphalt or fiberglass selvage rolled roofing that weighs 110 to 120 lbs. per square on a plain shed or gable wooden roof deck. Roofing to be applied with a 17" exposure. All fasteners, whether nails or staples are to be galvanized and apply fasteners 6" oc with the seams to be tarred. Roof slope is between a 1' rise in 12' run and 6' rise in 12' run.	
	
03038	E-WF.17
	Install ice and water shed 36" wide.  Rubberized material will be placed under starter course and in the valleys.	
	
04100	E-WF.17
	Install on shed or gable-type wood roof deck handsplit and resawn cedar shakes 24" long with 10" exposed, thickness 1/2" to 3/4". Shakes to be applied over 15 lb. felt woven between courses. All shakes to be applied with 6 penny rust resistance nails. Applied at a slope of 4 inches IN 12.	
	
04101	E-WF.17
	Install on shed or gable-type wood roof deck handsplit and resawn cedar shakes 24" long with 10" exposed, thickness 1/2" to 3/4". Shakes to be applied over 15 lb. felt woven between courses. All shakes to be applied with 6 penny rust resistance nails. Applied at a slope of between 5 inches and 6 inches IN 12.	
	
04102	E-WF.17
	Install on shed or gable-type wood roof deck handsplit and resawn cedar shakes 24" long with 10" exposed, thickness 1/2" to 3/4". Shakes to be applied over 15 lb. felt woven between courses. All shakes to be applied with 6 penny rust resistance nails. Applied at a slope of 7 to 8 IN 12.	
	
04103	E-WF.17
	Install on shed or gable-type wood roof deck handsplit and resawn cedar shakes 24" long with 10" exposed, thickness 1/2" to 3/4". Shakes to be applied over 15 lb. felt woven between courses. All shakes to be applied with 6 penny rust resistance nails. Applied at a slope of 9 to 10 IN 12.	
	
04104	E-WF.17
	Install on shed or gable-type wood roof deck handsplit and resawn cedar shakes 24" long with 10" exposed, thickness 1/2" to 3/4". Shakes to be applied over 15 lb. felt woven between courses. All shakes to be applied with 6 penny rust resistance nails. Applied at a slope of 11 to 12 IN 12.	
	
04110	E-WF.17
	Apply on shed or gable wood roof deck, 16" cedar shingle applied with 5" exposure over 15 lb. felt paper woven between courses. Shingles can be applied with no felt if wood deck is 1 x 4 or 1 x 6 spaced wood sheathing. Apply shingles with 3 penny rust resistance nails at a slope of 4 inches IN 12.	
	
04111	E-WF.17
	Apply on shed or gable wood roof deck, 16" cedar shingle applied with 5" exposure over 15 lb. felt paper woven between courses. Shingles can be applied with no felt if wood deck is 1 x 4 or 1 x 6 spaced wood sheathing. Apply shingles with 3 penny rust resistance nails at a slope of 5 to 6 inches IN 12.	
	
04112	E-WF.17
	Apply on shed or gable wood roof deck, 16" cedar shingle applied with 5" exposure over 15 lb. felt paper woven between courses. Shingles can be applied with no felt if wood deck is 1 x 4 or 1 x 6 spaced wood sheathing. Apply shingles with 3 penny rust resistance nails at a slope of 7 to 8 IN 12.	
	
04113	E-WF.17
	Apply on shed or gable wood roof deck, 16" cedar shingle applied with 5" exposure over 15 lb. felt paper woven between courses. Shingles can be applied with no felt if wood deck is 1 x 4 or 1 x 6 spaced wood sheathing. Apply shingles with 3 penny rust resistance nails at a slope of 9 to 10 IN 12.	
	
04114	E-WF.17
	Apply on shed or gable wood roof deck, 16" cedar shingle applied with 5" exposure over 15 lb. felt paper woven between courses. Shingles can be applied with no felt if wood deck is 1 x 4 or 1 x 6 spaced wood sheathing. Apply shingles with 3 penny rust resistance nails at a slope of 11 to 12 IN 12.	
	
06231	E-WF.17
	Apply 30 gauge galvanized standing seam sheet metal with baked enamel finish over 15 lb. roofing felt. For appropriate slope use either 9.217 or 9.218. Standing seam to be roll formed. All roof accessories and fasteners included.	
	
06232	E-WF.17
	Apply 30 gauge galvanized standing seam sheet metal with baked enamel finish over 15 lb. roofing felt at a slope of up to 6 IN 12. Standing seam to be roll formed. All roof accessories and fasteners included.	
	
06233	E-WF.17
	Apply 30 gauge galvanized standing seam sheet metal with baked enamel finish over 15 lb. roofing felt at a slope of 7 to 12 IN 12. Standing seam to be roll formed. All roof accessories and fasteners included.	
	
07100	E-WF.17
	Apply manufactured concrete roof tiles on plain shed or gable wood roof deck at a slope less than 4 IN 12. 13" x 16.5" x 1/2" tiles with lugs at head to be applied over a base of 2 layers of 30 lb. roofing felt that is hot mopped together. 2" wooden lath strips to be nailed over each rafter to be followed by a mopping of hot asphalt to imbed the lath strips. 1" x 2" redwood battens to be nailed across the lath strips spaced to hang the tiles on nailing every 3rd course of tile. All roof accessories are   included.	
	
07101	E-WF.17
	Apply manufactured concrete roof tiles on plain shed or gable wood roof deck at a slope greater than 3 IN 12. 13" x 16.5" x  1/2" tiles with lugs at head to be applied over a base of 2 layers of 30 lb. roofing felt that is hot mopped together. 2" wooden lath strips to be nailed over each rafter to be followed by a mopping of hot asphalt to imbed the lath strips. All roof accessories are included.	
	
07102	E-WF.17
	Apply manufactured concrete roof tiles on plain shed or gable wood roof deck at a slope of 4 IN 12. 13" x 16.5" x  1/2" tiles with lugs at head to be applied over a base of 2 layers of 30 lb. roofing felt that is hot mopped together. 2" wooden lath strips to be nailed over each rafter to be followed by a mopping of hot asphalt to imbed the lath strips. All roof accessories are included.	
	
07103	E-WF.17
	Apply manufactured concrete roof tiles on plain shed or gable wood roof deck at a slope greater than 3 IN 12. 13" x 16.5 x  1/2" tiles with lugs at head to be applied over existing 1x6 sheathing. 2" wooden lath strips to be nailed over each rafter to be followed by a mopping of hot asphalt to imbed the lath strips. All roof accessories are included.	
	
07104	E-WF.17
	Apply manufactured concrete roof tiles on plain shed or gable wood roof deck at a slope of 9 IN 12. 13" x 16.5" x  1/2" tiles with lugs at head to be applied over a base of 2 layers of 30 lb. roofing felt that is hot mopped together. 2" wooden lath strips to be nailed over each rafter to be followed by a mopping of hot asphalt to imbed the lath strips. 1" x 2" redwood battens to be nailed across the lath strips spaced to hang the tiles on nailing every 3rd course of tile. All roof accessories are included.	
	
07105	E-WF.17
	Apply manufactured concrete roof tiles on plain shed or gable wood roof deck at a slope of 114 IN 12. 13" x 16.5" x  1/2" tiles with lugs at head to be applied over a base of 2 layers of30 lb. roofing felt that is hot mopped together. 2" wooden lath strips to be nailed over each rafter to be followed by a mopping of hot asphalt to imbed the lath strips. 1" x 2" redwood battens to be nailed across the lath strips spaced to hang the tiles on nailing every 3rd course of tile. All roof accessories are included.	
	
07106	E-WF.17
	Apply manufactured concrete roof tiles on plain shed or gable wood roof deck at a slope between 7 inches and 9 inches IN 12. 13" x 16.5" x  1/2" tiles with lugs at head to be applied over existing 1x6 sheathing. 2" wooden lath strips to be nailed over each rafter to be followed by a mopping of hot asphalt to imbed the lath strips. 1" x 2" redwood battens to be nailed across the lath strips spaced to hang the tiles on nailing every 3rd course of tile. All roof accessories are included.	
	
07107	E-WF.17
	Apply manufactured concrete roof tiles on plain shed or gable wood roof deck at a slope between 11 inches and 12 inches IN 12.13" x 16 1/2" x  1/2" tiles with lugs at head to be applied over existing 1x6 sheathing. 2" wooden lath strips to be nailed over each rafter to be followed by a mopping of hot asphalt to imbed the lath strips. 1" x 2" redwood battens to be nailed across the lath strips spaced to hang the tiles on nailing every 3rd course of tile. All roof accessories are included.	
	
07200	E-WF.17
	Apply on plain shed or gable wood sheath roof deck Supradur mineral fiber shingles 9 7/16" x 16" 1/4" shingles. Shingles to weigh 500 lb. per applied square with 7" exposure over 15 lb. roof felt. Shingles to be applied with rust resistant nails.	
	
07201	E-WF.17
	Apply on plain shed or gable wood sheath roof deck Supradur mineral fiber shingles 9 7/16" x 16" 1/4" shingles. Shingles to weigh 500 lb. per applied square with 7" exposure over 15 lb. roof felt. Shingles to be applied with rust resistant nails.	
	
07202	E-WF.17
	Apply on plain shed or gable wood sheath roof deck Supradur mineral fiber shingles 9 7/16" x 16" 1/4" shingles. Shingles to weigh 500 lb. per applied square with 7" exposure over 15 lb. roof felt. Shingles to be applied with rust resistant nails.	
	
07203	E-WF.17
	Apply on plain shed or gable wood sheath roof deck Supradur mineral fiber shingles 9 7/16" x 16" 1/4" shingles. Shingles to weigh 500 lb. per applied square with 7" exposure over 15 lb. roof felt. Shingles to be applied with rust resistant nails.	
	
07204	E-WF.17
	Apply on plain shed or gable wood sheath roof deck Supradur mineral fiber shingles 14" x 30" 3/16" shingles. Shingles to weigh 325 lb. per applied square with 6" exposure over 15 lb. roof felt. Shingles to be applied with rust resistant nails. Roof pitch between 3 inches and 6 inches in 12.	
	
07205	E-WF.17
	Apply on plain shed or gable wood sheath roof deck Supradur mineral fiber shingles 14" x 30" 3/16" shingles. Shingles to weigh 325 lb. per applied square with 6" exposure over 15 lb. roof felt. Shingles to be applied with rust resistant nails. Roof pitch to be between 7 inches and 8 inches in 12.	
	
07206	E-WF.17
	Apply on plain shed or gable wood sheath roof deck Supradur mineral fiber shingles 14" x 30" 3/16" shingles. Shingles to weigh 325 lb. per applied square with 6" exposure over 15 lb. roof felt. Shingles to be applied with rust resistant nails. Roof pitch to be between 9 inches and 10 inches in 12.	
	
07207	E-WF.17
	Apply on plain shed or gable wood sheath roof deck Supradur mineral fiber shingles 14" x 30" 3/16" shingles. Shingles to weigh 325 lb. per applied square with 6" exposure over 15 lb. roof felt. Shingles to be applied with rust resistant nails. Roof pitch to be between 11 inches and 12 inches in slope.	
	
07208	E-WF.17
	Apply red Spanish clay tile on plain shed or gable wood roof deck. Deck to have 30 lb. roof felt, hot mopped to surface before applying tile 11" on center with a 15" exposure with 3" lap. Clay tile to be applied with roof resistant nails with all ridge and roof accessories included. Roof slope to be 3 to 6 IN 12.	
	
07209	E-WF.17
	Apply red Spanish clay tile on plain shed or gable wood roof deck. Deck to have 30 lb. roof felt, hot mopped to surface before applying tile 11" on center with a 15" exposure with 3" lap. Clay tile to be applied with rust resistant nails with all ridge and roof accessories included. Roof slope to be 7 to 12 IN 12.	
	
07210	E-WF.17
	Apply red Spanish clay tile on plain shed or gable wood roof deck. Deck to have 30 lb. roof felt, hot mopped to surface before applying tile 11" on center with a 15" exposure with 3" lap. Clay tile to be applied with rust resistant nails with all ridge and roof accessories included. Roof slope to be 9 to 10 IN 12.	
	
07211	E-WF.17
	Apply red Spanish clay tile on plain shed or gable wood roof deck. Deck to have 30 lb. roof felt, hot mopped to surface before applying tile 11" on center with a 15" exposure with 3" lap. Clay tile to be applied with rust resistant nails with all ridge and roof accessories included. Roof slope to be 11 to 12 IN 12.	
	
07221	E-WF.17
	Apply mission tile on wood roof deck. Tile to be applied over 30 lb. roof felt that has been hot mopped to surface. 1 x 4 wood  nailing strips to be applied so that 18" tile can be laid 10  3/4" on center with a 14" exposure and 4" lap. Tile to be installed with rust resistant nails, all ridge and roof accessories to be included. Roof slope to be 3 to 6 IN 12.	
	
07222	E-WF.17
	Apply mission tile on wood roof deck. Tile to be applied over 30 lb. roof felt that has been hot mopped to surface. 1 x 4 wood  nailing strips to be applied so that 18" tile can be laid 10  3/4" on center with a 14" exposure and 4" lap. Tile to be installed with rust resistant nails, all ridge and roof accessories to be included. Roof slope to be 7 to 8 IN 12.	
	
07223	E-WF.17
	Apply mission tile on wood roof deck. Tile to be applied over 30 lb. roof felt that has been hot mopped to surface. 1 x 4 wood  nailing strips to be applied so that 18" tile can be laid 10  3/4" on center with a 14" exposure and 4" lap. Tile to be installed with rust resistant nails, all ridge and roof accessories to be included. Roof slope to be 9 to 10 IN 12.	
	
07224	E-WF.17
	Apply mission tile on wood roof deck. Tile to be applied over 30 lb. roof felt that has been hot mopped to surface. 1 x 4 wood  nailing strips to be applied so that 18" tile can be laid 10  3/4" on center with a 14" exposure and 4" lap. Tile to be installed with rust resistant nails, all ridge and roof accessories to be included. Roof slope to be 11 to 12 IN 12.	
	
07225	E-WF.17
	Apply wood batten strips as required under clay tile roof.	
	
12046	E-WF.17
	Apply over a stable wood or concrete roof deck, 1 ply 30 lb. base sheet to be followed by 2 plys 15 lb. felt with interply mopping coats of D-312 hot asphalt applied at a minimum of 350 degrees F. Ballast roof with local ballast material, minimum slope 1/8" per foot.	
	
12048	E-WF.17
	Apply over a stable wood or concrete roof deck, 1 ply 30 lb. base sheet to be followed by 3 plys 15 lb. felt with interply mopping coats of D-312 hot asphalt applied at a minimum of 350 degrees F. Ballast roof with local ballast material, minimum slope 1/8" per foot.	
	
18500	E-WF.17
	Install flashing on average sized exterior/interior chimney with step flashing and counter flashing turned 1/2" into sawed open joint. Flashing material to be aluminum and includes caulking  with appropriate caulking material.	
	
18501	E-WF.17
	Install flashing on average sized exterior/interior chimney with step flashing and counter flashing turned 1/2" into sawed open joint. Flashing material to be copper and includes caulking with appropriate caulking material.	
	
18502	E-WF.17
	Install aluminum step flashing between gable roof and brick wall in open masonry joints.	
	
18503	E-WF.17
	Install copper step flashing between gable roof and brick wall in open masonry joints.	
	
18504	E-WF.17
	Install aluminum step flashing between gable roof and wood sheathed wall.	
	
18505	E-WF.17
	Install copper step flashing between gable roof and wood sheathed wall.	
	
18506	E-WF.17
	Flash top of flat or shed type roof to wood sheathed wall or into open joint with aluminum flashing.	
	
18507	E-WF.17
	Flash top of flat or shed type roof to wood sheath wall or into open joint with copper flashing.	
	
18508	E-WF.17
	Install 18" wide valley flashing with aluminum flashing material. Seal edges with plastic roof cement.	
	
18509	E-WF.17
	Install 18" wide valley flashing with copper flashing material. Seal edges with plastic roof cement.	
	
18510	E-WF.17
	Saw joints in masonry wall to receive flashings. Mortar joints to be of a soft nature.	
	
18511	E-WF.17
	Saw joints in masonry wall to receive flashings. Mortar joints to be of a hard nature.	
	
18512	E-WF.17
	Install aluminum flashing on parapet wall up to 12 inches high and up to 12 inches wide.	
	
18513	E-WF.17
	Install copper flashing on parapet wall up to 12 inches high and up to 12 inches wide.	
	
18514	E-WF.17
	Replace flashing on plumbing vent with new manufactured vent collar tying to existing roof as required.	
	
18515	E-WF.17
	Install wind directed turbine style ventilator with rotating top.	
	
18516	E-WF.17
	Install roof vent up to 9 inches in diameter. Vent to be either plastic or metal  screened manufactured roof vent installed in a fiberglass/asphalt shingle, roll roofing or wood shingle roof.	
	
18527	E-WF.17
	Install continuous painted aluminum ridge vent with louvered side openings in roof per manufacturer's specifications.  Installation includes cutting existing shingles and sheathing.	
	
18528	E-WF.17
	Install colored vinyl continuous roof ridge vent with louvered side openings per manufacturer's specifications.  Includes cutting existing shingles and sheathing.	
	
18529	E-WF.17
	Installation of painted aluminum continuous roof ridge vent with louvered side openings per manufacturer's specifications. Includes installation only.	
	
18530	E-WF.17
	Install colored vinyl continuous roof ridge vent with louvered side openings per manufacturer's specifications.  Does not include cutting existing shingles and sheathing.	
	
19226	E-WF.17
	Apply copper batten seam 16 oz. roofing over wood sheath deck. Copper roofing to be roll or break form. All seams to be machined crimped.	
	
19227	E-WF.17
	Apply copper batten seam 16 oz. roofing over wood sheath deck. Copper roofing to be roll or break form. All seams to be machined crimped.	
	
19228	E-WF.17
	Apply copper standing seam 16 oz. roofing over wood sheath deck. Copper roofing to be roll or break form. All seams to be machined crimped.	
	
19229	E-WF.17
	Apply copper flat seam 16 oz. roofing over wood sheath deck. Copper roofing to be roll or break form. All seams to be machined crimped.	
	
20517	E-WF.17
	Install white aluminum gutter and downspout system. Gutters to be of .027 gauge material. All accessories are included.	
	
20518	E-WF.17
	Install white aluminum gutter and downspout system. Gutters to be of .032 gauge material. All accessories are included.	
	
20520	E-WF.17
	Install galvanized steel 5" OG gutter and downspout system. All accessories are included.	
	
20521	E-WF.17
	Install galvanized steel 6" OG gutter and downspout system. All accessories are included.	
	
20522	E-WF.17
	Install 5" half round gutters and appropriate downspouts, including all required accessories.	
	
20523	E-WF.17
	Install 6" half round gutters and appropriate downspouts, including all required accessories.	
	
20524	E-WF.17
	Install 4" x 5" treated fir or hemlock gutters.	
	
20525	E-WF.17
	Install colored or white vinyl 5" gutters with downspouts, including all required accessories.	
	
20526	E-WF.17
	Install aluminum mesh 5" wide gutter guard. All accessories are included.	
	
03900	E-WF.18
	Install aluminum sliding window, 2-0 x 3-0. Window to be single glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03901	E-WF.18
	Install aluminum sliding window, 3-0 x 3-0. Window to be single glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03902	E-WF.18
	Install aluminum sliding window, 3-0 x 4-0. Window to be single glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03903	E-WF.18
	Install aluminum sliding window, 4-0 x 3-0. Window to be single glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03904	E-WF.18
	Install aluminum sliding window, 4-0 x 3-6. Window to be single glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03905	E-WF.18
	Install aluminum sliding window, 4-0 x 4-0. Window to be single glazed and includes weather-stripping, hardware and  screen. Interior trim including casings and sill.	
	
03906	E-WF.18
	Install aluminum sliding window, 5-0 x 3-6. Window to be single glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03907	E-WF.18
	Install aluminum sliding window, 5-0 x 4-0. Window to be single glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03908	E-WF.18
	Install aluminum sliding window, 6-0 x 4-0. Window to be single glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03909	E-WF.18
	Install aluminum sliding window, 2-0 x 3-0. Window to be double glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03910	E-WF.18
	Install aluminum sliding window, 3-0 x 3-0. Window to be double glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03911	E-WF.18
	Install aluminum sliding window, 3-0 x 4-0. Window to be double glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03912	E-WF.18
	Install aluminum sliding window, 4-0 x 3-0. Window to be double glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03914	E-WF.18
	Install aluminum sliding window, 4-0 x 4-0. Window to be double glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03915	E-WF.18
	Install aluminum sliding window, 5-0 x 3-6. Window to be double glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03916	E-WF.18
	Install aluminum sliding window, 5-0 x 4-0. Window to be double glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03917	E-WF.18
	Install aluminum sliding window, 6-0 x 4-0. Window to be double glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
03918	E-WF.18
	Install aluminum sliding window, 6-0 x 4-0. Window to be double glazed and includes weather-stripping, hardware and screen. Interior trim including casings and sill.	
	
05000	E-WF.18
	Install wood double hung window, 4 light, 1-8 x 3-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05001	E-WF.18
	Install wood double hung window, 4 light, 1-8 x 3-10 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05002	E-WF.18
	Install wood double hung window, 4 light, 1-8 x 4-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05003	E-WF.18
	Install wood double hung window, 4 light, 1-8 x 4-6 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05004	E-WF.18
	Install wood double hung window, 6 light, 2-0 x 3-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05005	E-WF.18
	Install wood double hung window, 6 light, 2-0 x 3-10 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05006	E-WF.18
	Install wood double hung window, 6 light, 2-0 x 4-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05007	E-WF.18
	Install wood double hung window, 6 light, 2-0 x 4-6  window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05008	E-WF.18
	Install wood double hung window, 6 light, 2-4 x 3-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05009	E-WF.18
	Install wood double hung window, 6 light, 2-4 x 3-10 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05010	E-WF.18
	Install wood double hung window, 6 light, 2-4 x 4-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05011	E-WF.18
	Install wood double hung window, 6 light, 2-4 x 4-6 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05012	E-WF.18
	Install wood double hung window, 6 light, 2-8 x 3-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05013	E-WF.18
	Install wood double hung window, 6 light, 2-8 x 3-10 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05014	E-WF.18
	Install wood double hung window, 6 light, 2-8 x 4-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05015	E-WF.18
	Install wood double hung window, 6 light, 2-8 x 4-6 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05016	E-WF.18
	Install wood double hung window, 6 light, 2-8 x 5-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05017	E-WF.18
	Install wood double hung window, 6 light, 2-8 x 5-6 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05018	E-WF.18
	Install wood double hung window, 8 light, 3-0 x 3-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05019	E-WF.18
	Install wood double hung window, 8 light, 3-0 x 3-10 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05020	E-WF.18
	Install wood double hung window, 8 light, 3-0 x 4-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05021	E-WF.18
	Install wood double hung window, 8 light, 3-0 x 4-6 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05022	E-WF.18
	Install wood double hung window, 8 light, 3-0 x 5-2 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05023	E-WF.18
	Install wood double hung window, 8 light, 3-0 x 5-6 window. Install in existing opening including frame and exterior brick molding, single glazed sash, sash lock, and interior trim and casing with stops. Interior window trim to include stool and apron.	
	
05100	E-WF.18
	Install builder quality wood double hung window, 2 light, 1-8 x 4-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05101	E-WF.18
	Install builder quality wood double hung window, 2 light, 1-8 x 4-6. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05102	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-0 x 3-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05103	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-0 x 4-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05104	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-0 x 4-6. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05105	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-0 x 5-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05107	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-4 x 3-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05108	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-4 x 3-10. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05109	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-4 x 4-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05110	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-4 x 4-6. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05111	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-4 x 5-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05113	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-8 x 3-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating  glass with interior trim, casing, stops, stool and apron.  Hardware to include sash lock and screen.	
	
05114	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-8 x 3-10. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05115	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-8 x 4-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05116	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-8 x 4-6. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05117	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-8 x 5-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05118	E-WF.18
	Install builder quality wood double hung window, 2 light, 2-8 x 5-6. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05121	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-0 x 3-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05122	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-0 x 3-10. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05123	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-0 x 4-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05124	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-0 x 4-6. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05125	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-0 x 5-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05126	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-0 x 5-6. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05128	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-4 x 3-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05129	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-4 x 3-10. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05130	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-4 x 4-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05131	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-4 x 4-6. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05132	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-4 x 5-2. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05133	E-WF.18
	Install builder quality wood double hung window, 2 light, 3-4 x 5-6. Installation to include frame, sash and brick mould in existing opening. Sash to be primed with 1/2" insulating glass with interior trim, casing, stops, stool and apron. Hardware to include sash lock and screen.	
	
05141	E-WF.18
	Install 1 light picture window, 4-0 x 4-2. With installation to include frame, sash and brick molding. Sash to be 1/2" insulated glass with all interior trim including stool and apron to be included.	
	
05142	E-WF.18
	Install 1 light picture window, 4-0 x 4-6. With installation to include frame, sash and brick molding. Sash to be 1/2" insulated glass with all interior trim including stool and apron to be included.	
	
05143	E-WF.18
	Install 1 light picture window, 4-0 x 5-2. With installation to include frame, sash and brick molding. Sash to be 1/2" insulated glass with all interior trim including stool and apron to be included.	
	
05144	E-WF.18
	Install 1 light picture window, 5-4 x 4-6. With installation to include frame, sash and brick molding. Sash to be 1/2" insulated glass with all interior trim including stool and apron to be included.	
	
05145	E-WF.18
	Install 1 light picture window, 5-4 x 5-2. With installation to include frame, sash and brick molding. Sash to be 1/2" insulated glass with all interior trim including stool and apron to be included.	
	
05146	E-WF.18
	For installation of picture windows with insulated sash that have side mounted double hung windows including all trim. Total the cost of the picture windows and double hung windows and add.	
	
05500	E-WF.18
	Install wood single glazed awning window, 2-0 x 1-8. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05501	E-WF.18
	Install wood single glazed awning window, 3-0 x 1-8. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05502	E-WF.18
	Install wood single glazed awning window, 3-0 x 2-0. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05503	E-WF.18
	Install wood single glazed awning window, 3-0 x 2-4. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05504	E-WF.18
	Install wood single glazed awning window, 3-0 x 3-0. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05505	E-WF.18
	Install wood single glazed awning window, 3-0 x 3-4. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05506	E-WF.18
	Install wood single glazed awning window, 4-0 x 1-8. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05508	E-WF.18
	Install wood single glazed awning window, 4-0 x 2-0. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05509	E-WF.18
	Install wood single glazed awning window, 4-0 x 2-4. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05512	E-WF.18
	Install wood double glazed awning window, 2-0 x 1-8. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05513	E-WF.18
	Install wood double glazed awning window, 2-0 x 2-0. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05514	E-WF.18
	Install wood double glazed awning window, 2-0 x 2-4. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05515	E-WF.18
	Install wood double glazed awning window, 3-0 x 1-8. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05516	E-WF.18
	Install wood double glazed awning window, 2-0 x 2-0. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05517	E-WF.18
	Install wood double glazed awning window, 3-0 x 2-4. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05518	E-WF.18
	Install wood double glazed awning window, 3-0 x 3-0. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05519	E-WF.18
	Install wood double glazed awning window, 3-0 x 3-4. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05520	E-WF.18
	Install wood double glazed awning window, 4-0 x 1-8. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05521	E-WF.18
	Install wood double glazed awning window, 4-0 x 2-4. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05522	E-WF.18
	Install wood double glazed awning window, 4-0 x 2-4. Installation to include single glaze sash, frame, exterior brick mould and weather-stripping. Interior to include casing, stool  and apron. Hardware to include drip cap, sash lock and screen.	
	
05524	E-WF.18
	Install single glazed wood casement window, 1-11 x 3-0. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and  apron. Hardware to include hinges, rotary operator and screen.	
	
05525	E-WF.18
	Install single glazed wood casement window, 1-11 x 3-4. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and  apron. Hardware to include hinges, rotary operator and screen.	
	
05526	E-WF.18
	Install single glazed wood casement window, 1-11 x 4-0. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and  apron. Hardware to include hinges, rotary operator and screen.	
	
05527	E-WF.18
	Install single glazed wood casement window, 1-11 x 4-4. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and  apron. Hardware to include hinges, rotary operator and screen.	
	
05528	E-WF.18
	Install single glazed wood casement window, 1-11 x 5-0. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and  apron. Hardware to include hinges, rotary operator and screen.	
	
05529	E-WF.18
	Install single glazed wood casement window, 2-4 x 3-0. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and  apron. Hardware to include hinges, rotary operator and screen.	
	
05530	E-WF.18
	Install single glazed wood casement window, 2-4 x 3-4. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and  apron. Hardware to include hinges, rotary operator and screen.	
	
05531	E-WF.18
	Install single glazed wood casement window, 2-4 x 4-0. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and  apron. Hardware to include hinges, rotary operator and screen.	
	
05532	E-WF.18
	Install single glazed wood casement window, 2-4 x 4-4. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and  apron. Hardware to include hinges, rotary operator and screen.	
	
05533	E-WF.18
	Install single glazed wood casement window, 2-4 x 5-0. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and  apron. Hardware to include hinges, rotary operator and screen.	
	
05542	E-WF.18
	Install insulated glass, premium quality, vinyl covered wood sash, wood casement window, 1-11 x 3-0. Installation in standard opening and includes exterior frame and brick molding with   interior trim including casing, stool and apron. Hardware to  include hinges, rotary operator and screen.	
	
05543	E-WF.18
	Install insulated glass, premium quality, vinyl covered wood sash, wood casement window, 1-11 x 3-4. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and apron. Hardware to include hinges, rotary operator and screen.	
	
05544	E-WF.18
	Install insulated glass, premium quality, vinyl covered wood sash, wood casement window, 1-11 x 4-0. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and apron. Hardware to include hinges, rotary operator and screen.	
	
05545	E-WF.18
	Install insulated glass, premium quality, vinyl covered wood sash, wood casement window, 1-11 x 5-0. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and apron. Hardware to include hinges, rotary operator and screen.	
	
05546	E-WF.18
	Install insulated glass, premium quality, vinyl covered wood sash, wood casement window, 2-4 x 3-0. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and apron. Hardware to include hinges, rotary operator and screen.	
	
05547	E-WF.18
	Install insulated glass, premium quality, vinyl covered wood sash, wood casement window, 2-4 x 3-4. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and apron. Hardware to include hinges, rotary operator and screen.	
	
05548	E-WF.18
	Install insulated glass, premium quality, vinyl covered wood sash, wood casement window, 2-4 x 4-0. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and apron. Hardware to include hinges, rotary operator and screen.	
	
05549	E-WF.18
	Install insulated glass, premium quality, vinyl covered wood sash, wood casement window, 2-4 x 4-4. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and apron. Hardware to include hinges, rotary operator and screen.	
	
05550	E-WF.18
	Install insulated glass, premium quality, vinyl covered wood sash, wood casement window, 2-4 x 5-0. Installation in standard opening and includes exterior frame and brick molding with interior trim including casing, stool and apron. Hardware to include hinges, rotary operator and screen.	
	
05600	E-WF.18
	Install builder quality, wood, single glazed window, 3-0 x 3-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05601	E-WF.18
	Install builder quality, wood, single glazed window, 3-0 x 3-6. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05602	E-WF.18
	Install builder quality, wood, single glazed window, 4-0 x 3-6. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05603	E-WF.18
	Install builder quality, wood, single glazed window, 4-0 x 4-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05604	E-WF.18
	Install builder quality, wood, single glazed window, 5-0 x 3-6. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05605	E-WF.18
	Install builder quality, wood, single glazed window, 5-0 x 4-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05606	E-WF.18
	Install builder quality, wood, single glazed window, 5-0 x 5-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05607	E-WF.18
	Install builder quality, wood, single glazed window, 6-0 x 4-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05608	E-WF.18
	Install builder quality, wood, single glazed window, 6-0 x 5-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05609	E-WF.18
	Install builder quality, wood, insulated glass window, 3-0 x 3-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05610	E-WF.18
	Install builder quality, wood, insulated glass window, 3-0 x 3-6. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05611	E-WF.18
	Install builder quality, wood, insulated glass window, 4-0 x 3-6. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05612	E-WF.18
	Install builder quality, wood, insulated glass window, 4-0 x 4-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05613	E-WF.18
	Install builder quality, wood, insulated glass window, 5-0 x 3-6. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05614	E-WF.18
	Install builder quality, wood, insulated glass window, 5-0 x 4-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05615	E-WF.18
	Install builder quality, wood, insulated glass window, 5-0 x 5-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05616	E-WF.18
	Install builder quality, wood, insulated glass window, 6-0 x 4-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
05617	E-WF.18
	Install builder quality, wood, insulated glass window, 6-0 x 5-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
06200	E-WF.18
	Install premium quality wood double hung window, 1-8 x 4-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06201	E-WF.18
	Install premium quality wood double hung window, 1-8 x 4-6. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06202	E-WF.18
	Install premium quality wood double hung window, 2-0 x 3-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06203	E-WF.18
	Install premium quality wood double hung window, 2-0 x 4-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06204	E-WF.18
	Install premium quality wood double hung window, 2-0 x 4-6. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06205	E-WF.18
	Install premium quality wood double hung window, 2-0 x 5-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06206	E-WF.18
	Install premium quality wood double hung window, 2-4 x 2-10. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06207	E-WF.18
	Install premium quality wood double hung window, 2-4 x 3-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06208	E-WF.18
	Install premium quality wood double hung window, 2-4 x 3-10. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06209	E-WF.18
	Install premium quality wood double hung window, 2-4 x 4-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06210	E-WF.18
	Install premium quality wood double hung window, 2-4 x 4-6. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06211	E-WF.18
	Install premium quality wood double hung window, 2-4 x 5-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06213	E-WF.18
	Install premium quality wood double hung window, 2-8 x 3-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06214	E-WF.18
	Install premium quality wood double hung window, 2-8 x 3-10. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06215	E-WF.18
	Install premium quality wood double hung window, 2-8 x 4-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06216	E-WF.18
	Install premium quality wood double hung window, 2-8 x 4-6. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06217	E-WF.18
	Install premium quality wood double hung window, 2-8 x 5-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06218	E-WF.18
	Install premium quality wood double hung window, 2-8 x 5-6. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06221	E-WF.18
	Install premium quality wood double hung window, 3-0 x 3-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06222	E-WF.18
	Install premium quality wood double hung window, 3-0 x 3-10. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06223	E-WF.18
	Install premium quality wood double hung window, 3-0 x 4-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06224	E-WF.18
	Install premium quality wood double hung window, 3-0 x 4-6. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06225	E-WF.18
	Install premium quality wood double hung window, 3-0 x 5-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06226	E-WF.18
	Install premium quality wood double hung window, 3-0 x 5-6. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06228	E-WF.18
	Install premium quality wood double hung window, 3-4 x 3-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06229	E-WF.18
	Install premium quality wood double hung window, 3-4 x 3-10. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06230	E-WF.18
	Install premium quality wood double hung window, 3-4 x 4-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06231	E-WF.18
	Install premium quality wood double hung window, 3-4 x 4-6. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06232	E-WF.18
	Install premium quality wood double hung window, 3-4 x 5-2. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06233	E-WF.18
	Install premium quality wood double hung window, 3-4 x 5-6. Window to be constructed of primed sash with 1/2" insulating glass, vinyl covered wood frame. Trim to include exterior brick molding and interior trim, stops, stool and apron. Hardware will include sash lock and screen.	
	
06241	E-WF.18
	Install premium quality picture window with insulated glass/sash, 4-0 x 4-2. Window to be constructed of vinyl covered wood frame with trim to include exterior brick molding and interior trim, stops, stool and apron.	
	
06242	E-WF.18
	Install premium quality picture window with insulated glass/sash, 4-0 x 4-6. Window to be constructed of vinyl covered wood frame with trim to include exterior brick molding and interior trim, stops, stool and apron.	
	
06243	E-WF.18
	Install premium quality picture window with insulated glass/sash, 4-0 x 5-2. Window to be constructed of vinyl covered wood frame with trim to include exterior brick molding and interior trim, stops, stool and apron.	
	
06244	E-WF.18
	Install premium quality picture window with insulated glass/sash, 5-4 x 4-6. Window to be constructed of vinyl covered wood frame with trim to include exterior brick molding and interior trim, stops, stool and apron.	
	
06245	E-WF.18
	Install premium quality picture window with insulated glass/sash, 5-4 x 5-2. Window to be constructed of vinyl covered wood frame with trim to include exterior brick molding and interior trim, stops, stool and apron.	
	
06246	E-WF.18
	Install premium quality picture window with insulated sash and side mounted double hung windows. Total costs for the double hung windows and picture window and add.	
	
06618	E-WF.18
	Install wood, insulated glass, premium quality vinyl covered wood sash window, 3-0 x 3-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
06619	E-WF.18
	Install wood, insulated glass, premium quality vinyl covered wood sash window, 3-0 x 3-6. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
06620	E-WF.18
	Install wood, insulated glass, premium quality vinyl covered wood sash window, 4-0 x 3-6. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
06621	E-WF.18
	Install wood, insulated glass, premium quality vinyl covered wood sash window, 4-0 x 4-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
06622	E-WF.18
	Install wood, insulated glass, premium quality vinyl covered wood sash window, 5-0 x 3-6. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
06623	E-WF.18
	Install wood, insulated glass, premium quality vinyl covered wood sash window, 5-0 x 4-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
06624	E-WF.18
	Install wood, insulated glass, premium quality vinyl covered wood sash window, 5-0 x 5-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
06625	E-WF.18
	Install wood, insulated glass, premium quality vinyl covered wood sash window, 6-0 x 4-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
06626	E-WF.18
	Install wood, insulated glass, premium quality vinyl covered wood sash window, 6-0 x 5-0. Installation to include exterior trim, interior trim, including casing, stool and apron. Normal installation hardware and exterior screen is part of the installation.	
	
10650	E-WF.18
	Install builder quality wood round top window, 2-2x 1-4. Installation to include exterior trim, interior trim, including 2 1/4 arched casing, stool and apron.	
	
10651	E-WF.18
	Install builder quality wood round top window, 2-6x 1-4. Installation to include exterior trim, interior trim, including 2 1/4 arched casing, stool and apron.	
	
10652	E-WF.18
	Install builder quality wood round top window, 2-10x 1-4. Installation to include exterior trim, interior trim, including 2 1/4 arched casing, stool and apron.	
	
10653	E-WF.18
	Install builder quality wood round top window, 3-2x 1-4. Installation to include exterior trim, interior trim, including 2 1/4 arched casing, stool and apron.	
	
10654	E-WF.18
	Install builder quality wood round top window, 3-6x 2-0. Installation to include exterior trim, interior trim, including 2 1/4 arched casing, stool and apron.	
	
10655	E-WF.18
	Install premium quality wood round top window, 2-2x 1-4. Installation to include exterior trim, interior trim, including 2 1/4 arched casing, stool and apron.	
	
10656	E-WF.18
	Install premium quality wood round top window, 2-6x 1-4. Installation to include exterior trim, interior trim, including 2 1/4 arched casing, stool and apron.	
	
10657	E-WF.18
	Install premium quality wood round top window, 2-10x 1-4. Installation to include exterior trim, interior trim, including 2 1/4 arched casing, stool and apron.	
	
10658	E-WF.18
	Install premium quality wood round top window, 3-2 x 1-4. Installation to include exterior trim, interior trim, including 2 1/4 arched casing, stool and apron.	
	
10659	E-WF.18
	Install premium quality wood round top window, 3-6 x 2-0. Installation to include exterior trim, interior trim, including 2 1/4 arched casing, stool and apron.	
	
10918	E-WF.18
	Install wood frame and sash in existing opening in basement wall.  Window to be single glazed with opening of 2-8 x 1-4. Window comprised of 1 panel. Installation includes hardware and screen. Interior trim includes casing and sill.	
	
10919	E-WF.18
	Install wood frame and sash in existing opening in basement wall.  Window to be single glazed with opening of 2-8 x 1-8. Window comprised of 1 panel. Installation includes hardware and screen. Interior trim includes casing and sill.	
	
10920	E-WF.18
	Install wood frame and sash in existing opening in basement wall.  Window to be single glazed with opening of 2-8 x 2-0. Window comprised of 1 panel. Installation includes hardware and screen. Interior trim includes casing and sill.	
	
10921	E-WF.18
	Install aluminum frame sliding window in an existing opening in basement wall.  Window to be single glazed with opening of 3-0 x1-0. Window comprised of 1 panel, one operating sash and one stationary sash. Installation includes hardware and screen. Interior trim includes casing and sill.	
	
10922	E-WF.18
	Install aluminum frame sliding window in an existing opening in basement wall.  Window to be single glazed with opening of 3-0 x1-6. Window comprised of 1 panel, one operating sash and one stationary sash. Installation includes hardware and screen. Interior trim includes casing and sill.	
	
10923	E-WF.18
	Install aluminum frame sliding window in an existing opening in basement wall.  Window to be single glazed with opening of 3-0 x2-0. Window comprised of 1 panel, one operating sash and one stationary sash. Installation includes hardware and screen. Interior trim includes casing and sill.	
	
12700	E-WF.18
	Install roof window with outside frame dimensions of 30 3/4" x 38 1/2". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and center pivoting. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12701	E-WF.18
	Install roof window with outside frame dimensions of 30 3/4" x 55". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and center pivoting. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12702	E-WF.18
	Install roof window with outside frame dimensions of 36 7/8" x 62 7/8". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and center pivoting. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12703	E-WF.18
	Install roof window with outside frame dimensions of 44 7/8" x 48 1/2". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and center pivoting. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12704	E-WF.18
	Install roof window with outside frame dimensions of 27 1/2" x 46 1/2". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and center pivoting. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12705	E-WF.18
	Install roof window with outside frame dimensions of 21 5/8" x 38 1/2". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and center pivoting. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12706	E-WF.18
	Install roof window with outside frame dimensions of 52 3/4" x 38 1/2". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and center pivoting. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12707	E-WF.18
	Install roof window with outside frame dimensions of 52 3/4" x 55". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and center pivoting. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12708	E-WF.18
	Install roof window with outside frame dimensions of 21 5/8" x 27 1/2". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and center pivoting. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12709	E-WF.18
	Install roof window with outside frame dimensions of 30 3/4" x 38 1/2". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and top-hung. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12710	E-WF.18
	Install roof window with outside frame dimensions of 30 3/4" x 55". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and top-hung. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12711	E-WF.18
	Install roof window with outside frame dimensions of 44 7/8" x 46 1/2". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and top-hung. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
12712	E-WF.18
	Install roof window with outside frame dimensions of 21 5/8" x 38 1/2". This installation to occur during new construction, building a curve on existing frame opening. Window to be aluminum clad wood with insulated glass sash and top-hung. Installation to include interior finished well and trim. Hardware for installation to include the exterior awning, insect screen and lock.	
	
15146	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15147	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15148	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15149	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15150	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15151	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15152	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15153	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15154	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15155	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15156	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15157	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15158	E-WF.18
	Install divided light grilles, either plastic or wood for each picture window.	
	
15159	E-WF.18
	Install divided light grilles, either plastic or wood for each picture window.	
	
15160	E-WF.18
	Install divided light grilles, either plastic or wood for each picture window.	
	
15161	E-WF.18
	Install divided light grilles, either plastic or wood for each picture window.	
	
15246	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15247	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15248	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15249	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15250	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15251	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15252	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15253	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15254	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15255	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15256	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15257	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15258	E-WF.18
	Install divided light grilles, either plastic or wood for each picture window.	
	
15259	E-WF.18
	Install divided light grilles, either plastic or wood for each picture window.	
	
15260	E-WF.18
	Install divided light grilles, either plastic or wood for each picture window.	
	
15261	E-WF.18
	Install divided light grilles, either plastic or wood for each picture window.	
	
15551	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15552	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15553	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15554	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15555	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15556	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15557	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15558	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15559	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15560	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15627	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15628	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15629	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15630	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15631	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15632	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15633	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15634	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15635	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15660	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15661	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15662	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15663	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
15664	E-WF.18
	Install divided light grilles, either plastic or wood for each window.	
	
19713	E-WF.18
	Install hatch type skylight in new work with fixed insulated glass in rough opening of 22" x 30". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19714	E-WF.18
	Install hatch type skylight in new work with fixed insulated glass in rough opening of 22" x 45 1/2". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19715	E-WF.18
	Install hatch type skylight in new work with fixed insulated glass in rough opening of 30" x 22". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19716	E-WF.18
	Install hatch type skylight in new work with fixed insulated glass in rough opening of 30" x 30". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19717	E-WF.18
	Install hatch type skylight in new work with fixed insulated glass in rough opening of 30" x 45 1/2". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19718	E-WF.18
	Install hatch type skylight in new work with fixed insulated glass in rough opening of 45 1/2" x 30". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19719	E-WF.18
	Install hatch type skylight in new work with fixed insulated glass in rough opening of 45 1/2" x 45 1/2". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19720	E-WF.18
	Install hatch type skylight in new work with ventilating insulated glass in rough opening of 22" x 30". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19721	E-WF.18
	Install hatch type skylight in new work with ventilating insulated glass in rough opening of 22" x 45 1/2". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19722	E-WF.18
	Install hatch type skylight in new work with ventilating insulated glass in rough opening of 30 x 22". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19723	E-WF.18
	Install hatch type skylight in new work with ventilating insulated glass in rough opening of 30 x 30". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19724	E-WF.18
	Install hatch type skylight in new work with ventilating insulated glass in rough opening of 30 x 45 1/2". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19725	E-WF.18
	Install hatch type skylight in new work with ventilating insulated glass in rough opening of 45 1/2" x 30". Glass to be installed in a double aluminum frame with copper flashing covers and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
19726	E-WF.18
	Install hatch type skylight in new work with ventilating insulated glass in rough opening of 45 1/2" x 45 1/2. Glass to be installed in a double aluminum frame with copper flashing cover and a marine grade plywood liner box. Interior trim will include liner box and necessary casing.	
	
20800	E-WF.18
	Install prefabricated premium quality bow window in existing rough opening of 8-4 1/2 x 5-8. Windows to be four premium quality wood casement window with insulating glass, 2-0 x 5-6. Trim to include exterior brick molding and all interior casings. Hardware to include casement operators and locks.	
	
20801	E-WF.18
	Install prefabricated premium quality bow window, in existing rough opening of 8-4 1/2 x 5-8, aluminum clad. Windows to be four premium quality wood casement window with insulating glass,2-0 x 5-6. Trim to include exterior brick molding and all interior casings. Hardware to include casement operators and locks.	
	
20802	E-WF.18
	Install in the area below the bottom of the bow casement windows and the floor a seat that is installed flush with the interior walls. Installation to be of 3/4" plywood and include vertical headboard and plywood seat with knee braces.	
	
20803	E-WF.18
	Install roof over bow window projection with 2 x 4 framing, 1/2" plywood roof sheathing, 3/4" x 3/4" cove fascia, felt paper and asphalt shingles.	
	
20804	E-WF.18
	Install roof over bow window projection with 2 x 4 framing, 1/2" plywood roof sheathing, 3/4" x 3/4" cove fascia, felt paper and asphalt shingles.	
	
20805	E-WF.18
	Install prefabricated premium quality bay window in existing rough opening. Windows to be two premium quality wood vinyl clad double-hung windows with insulating glass, 1-8 x 4-6 and one of same quality 4-4x4-6. Trim to include exterior brick molding and all interior casings. Projection to be 14".	
	
20806	E-WF.18
	Install prefabricated premium quality bay window in existing rough opening. Windows to be two premium quality wood vinyl clad double-hung windows with insulating glass, 1-8 x 4-6 and one of same quality 4-4x4-6. Trim to include exterior brick molding and all interior casings. Projection to be 20".	
	
20807	E-WF.18
	Install prefabricated premium quality bay window in existing rough opening. Windows to be two premium quality wood vinyl clad double-hung windows with insulating glass, 1-5 x 4-6 and one of same quality 4-4x4-6. Trim to include exterior brick molding and all interior casings. Projection to be 23".	
	
20808	E-WF.18
	Install in the area below the bottom of the bay window and the floor a seat that is installed flush with the interior walls. Installation to be of 3/4" plywood and include vertical headboard and plywood seat with knee braces.	
	
20809	E-WF.18
	Install roof over bay window projection with 2 x 4 framing, 1/2" plywood roof sheathing, 3/4" x 3/4" cove fascia, felt paper and asphalt shingles.	
	
20810	E-WF.18
	Install roof over bay window projection with 2 x 4 framing, 1/2" plywood roof sheathing, 3/4" x 3/4" cove fascia, felt paper and asphalt shingles.	
	
02033	E-WF.19
	Install a metal clad prehung, 6 panel door, 3-0 x 6-8 x 1 3/4" foam core door. Prehung hardware to include three exterior 4 x 4 butts, aluminum threshold, and magnetic weather-stripping. Install exterior keyed lock in predrilled holes. Prehung unit to include exterior frame and brick molding as well as interior  trim.	
	
04013	E-WF.19
	Install exterior three panel, four light fir door, 2-8 x 6-8. Included in installation are frame and jambs, interior trim, brick molding, and hardware to include exterior butts and key lock.	
	
04014	E-WF.19
	Install exterior French fir door 1 3/4" thick with 10 lights. Installation to include frame, jambs, brick mould and oak sill. Hardware to be installed to include three 4 x 4 brass butts, and exterior keyed lock.	
	
04015	E-WF.19
	Install exterior French fir door 1 3/4" thick with 10 lights. Installation to include frame, jambs, brick mould and oak sill. Hardware to be installed to include three 4 x 4 brass butts, and exterior keyed lock.	
	
04016	E-WF.19
	Install exterior French fir door 1 3/4" thick with 10 lights. Installation to include frame, jambs, brick mould and oak sill. Hardware to be installed to include three 4 x 4 brass butts, and exterior keyed lock.	
	
04017	E-WF.19
	Install two Flush birch exterior doors to include frame and jambs brick molding and sill as well as three 4 x 4 brass butts on both doors. Standard key lock and dead bolt lock to be included. Center T-astragel to be mounted. Doors to be 3-0 x 6-8 each.	
	
04018	E-WF.19
	Install two Colonial fir exterior doors to include frame and jambs brick molding and sill as well as three 4 x 4 brass butts on both doors. Standard key lock and dead bolt lock to be included. Center T-astragel to be mounted. Doors to be 3-0 x 6-8 each.	
	
04019	E-WF.19
	Install two Colonial fir exterior doors to include frame and jambs brick molding and sill as well as three 4 x 4 brass butts on both doors. Standard key lock and dead bolt lock to be included. Center T-astragel to be mounted. Doors to be 3-0 x 6-8each.	
	
04020	E-WF.19
	Install exterior double Dutch doors, fir, 2 panel with 9 lights. Installation to include frame and jambs with exterior brick   molding, interior casing and oak sill. Installed hardware to  include 2 pair of 4 x 4 brass butts, Dutch door quadrant, and  exterior keyed lock.	
	
04021	E-WF.19
	Install exterior double Dutch doors, fir, 2 panel with 9 lights. Installation to include frame and jambs with exterior brick   molding, interior casing and oak sill. Installed hardware to  include 2 pair of 4 x 4 brass butts, Dutch door quadrant, and  exterior keyed lock.	
	
04022	E-WF.19
	Add to cost if using Crossbuck style of door.	
	
04023	E-WF.19
	Install exterior double Dutch Crossbuck doors, fir, 2 panel with9 lights. Installation to include frame and jambs with exterior brick   molding, interior casing and oak sill. Installed hardware to  include 2 pair of 4 x 4 brass butts, Dutch door quadrant, and  exterior keyed lock.	
	
04026	E-WF.19
	Install a prehung solid core birch door that is 2-8 x 6-8, 1 3/4" thick. Install prehung unit in rough opening with prehung unit to  include frame and jambs, exterior brick mould, threshold and exterior casing. An exterior keyed lock will be installed in predrilled hole.	
	
04027	E-WF.19
	Install a prehung solid core birch door that is 3-0 x 6-8, 1 3/4" thick. Install prehung unit in rough opening with prehung unit to include frame and jambs, exterior brick mould, threshold and exterior casing. An exterior keyed lock will be installed in predrilled hole.	
	
04028	E-WF.19
	Install a prehung solid core birch door that is 3-0 x 7-0, 1 3/4" thick. Install prehung unit in rough opening with prehung unit to include frame and jambs, exterior brick mould, threshold and exterior casing. An exterior keyed lock will be installed in predrilled hole.	
	
04100	E-WF.19
	Install Flush birch exterior door 2-8 x 6-8 that is 1 3/4" thick. Installation to include solid door with particle core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04101	E-WF.19
	Install Flush birch exterior door 3-0 x 6-8 that is 1 3/4" thick. Installation to include solid door with particle core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04102	E-WF.19
	Install Flush birch exterior door 3-0 x 7-0 that is 1 3/4" thick. Installation to include solid door with particle core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04103	E-WF.19
	Install Flush birch exterior door 2-8 x 6-8 that is 1 3/4" thick. Installation to include solid door with lumber core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04104	E-WF.19
	Install Flush birch exterior door 3-0 x 6-8 that is 1 3/4" thick. Installation to include solid door with lumber core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04105	E-WF.19
	Install Flush birch exterior door 3-0 x 7-0 that is 1 3/4" thick. Installation to include solid door with lumber core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04106	E-WF.19
	Install Colonial fir 6-panel door 2-8 x 6-8 that is 1 3/4" thick. Installation to include solid door with particle core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04107	E-WF.19
	Install Colonial fir 6-panel door 3-0 x 6-8 that is 1 3/4" thick. Installation to include solid door with particle core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04108	E-WF.19
	Install Colonial fir 6-panel door 3-0 x 7-0 that is 1 3/4" thick. Installation to include solid door with particle core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04109	E-WF.19
	Install Colonial pine 6-panel door 2-8 x 6-8 that is 1 3/4" thick. Installation to include solid door with particle core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04110	E-WF.19
	Install Colonial pine 6-panel door 3-0 x 6-8 that is 1 3/4" thick. Installation to include solid door with particle core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04111	E-WF.19
	Install Colonial pine 6-panel door 3-0 x 7-0 that is 1 3/4" thick. Installation to include solid door with particle core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04112	E-WF.19
	Install Colonial fir 3-panel 4 light door 2-8 x 7-0 that is 1 3/4" thick. Installation to include solid door with particle core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04113	E-WF.19
	Install Colonial fir 3-panel 4 light door 3-0 x 7-0 that is 1 3/4" thick. Installation to include solid door with particle core, includes jamb frame material, brick molding, interior casing and three 4" x 4" brass butts. Standard entrance key lock and installation are also included. All door installations are custom installed to fit opening.	
	
04114	E-WF.19
	Install a prehung solid core colonial fir, 6 panel door that is 3-0 x 6-8, 1 3/4" thick. Install prehung unit in rough opening with prehung unit to include frame and jambs, exterior brick mould, threshold and exterior casing. An exterior keyed lock will be installed in predrilled hole.	
	
04115	E-WF.19
	Install a prehung solid core colonial fir, 6 panel door that is 3-0 x 6-8, 1 3/4" thick. Install prehung unit in rough opening with prehung unit to include frame and jambs, exterior brick mould, threshold and exterior casing. An exterior keyed lock will be installed in predrilled hole.	
	
04116	E-WF.19
	Install a prehung solid core colonial fir, 6 panel door that is 3-0 x 7-0, 1 3/4" thick. Install prehung unit in rough opening with prehung unit to include frame and jambs, exterior brick mould, threshold and exterior casing. An exterior keyed lock will be installed in predrilled hole.	
	
04117	E-WF.19
	Install a prehung solid core colonial pine, 6 panel door that is 3-0 x 6-8, 1 3/4" thick. Install prehung unit in rough opening with prehung unit to include frame and jambs, exterior brick  mould, threshold and exterior casing. An exterior keyed lock  will be installed in predrilled hole.	
	
04118	E-WF.19
	Install a prehung solid core colonial pine, 6 panel door that is 3-0 x 6-8, 1 3/4" thick. Install prehung unit in rough opening with prehung unit to include frame and jambs, exterior brick  mould, threshold and exterior casing. An exterior keyed lock  will be installed in predrilled hole.	
	
04119	E-WF.19
	Install a prehung solid core colonial pine, 6 panel door that is 3-0 x 7-0, 1 3/4" thick. Install prehung unit in rough opening with prehung unit to include frame and jambs, exterior brick  mould, threshold and exterior casing. An exterior keyed lock  will be installed in predrilled hole.	
	
05009	E-WF.19
	Install exterior metal door 2-8 x 6-8. Door to be 1 3/4 inch thick foam core steel clad. Included in installation are frame and jambs, interior trim, brick molding, and hardware to include exterior butts and key lock.	
	
05010	E-WF.19
	Install exterior metal door 3-0 x 6-8. Door to be 1 3/4 inch thick foam core steel clad. Included in installation are frame and jambs, interior trim, brick molding, and hardware to include exterior butts and key lock.	
	
05011	E-WF.19
	Install exterior metal door 2-8 x 6-8. Door to be 1 3/4 inch thick foam core steel clad. Door has one tempered glass light. Included in installation are frame and jambs, interior trim, brick molding, and hardware to include exterior butts and key lock.	
	
05012	E-WF.19
	Install exterior metal door 3-0 x 6-8. Door to be 1 3/4 inch thick foam core steel clad. Door has one tempered glass light. Included in installation are frame and jambs, interior trim, brick molding, and hardware to include exterior butts and key lock.	
	
10118	E-WF.19
	Install wood garage door, 8-0 x 7-0, 4 section 4 panel door with one row of lights. Installation to include all required hardware and trim. Door will be scribed and cut to fit garage floor.   Install rubber gasket on the bottom of garage door that meets  concrete garage floor.	
	
10119	E-WF.19
	Install wood garage door, 9-0 x 7-0, 4 section 4 panel door with one row of lights. Installation to include all required hardware and trim. Door will be scribed and cut to fit garage floor.   Install rubber gasket on the bottom of garage door that meets  concrete garage floor.	
	
10120	E-WF.19
	Install wood garage door, 16-0 x 7-0, 4 section 4 panel door with one row of lights. Installation to include all required hardware and trim. Door will be scribed and cut to fit garage floor. Install rubber gasket on the bottom of garage door that meets concrete garage floor.	
	
10121	E-WF.19
	Install metal garage door, 8-0 x 7-0, 4 section 4 panel door with one row of lights. Installation to include all required hardware and trim.	
	
10122	E-WF.19
	Install metal garage door, 9-0 x 7-0, 4 section 4 panel door with one row of lights. Installation to include all required hardware and trim.	
	
10123	E-WF.19
	Install metal garage door, 16-0 x 7-0, 4 section 4 panel door with one row of lights. Installation to include all required hardware and trim.	
	
10124	E-WF.19
	Install fiberglass garage door, 8-0 x 7-0, 4 section 4 panel door with one row of lights. Installation to include all required hardware and trim.	
	
10125	E-WF.19
	Install fiberglass garage door, 9-0 x 7-0, 4 section 4 panel door with one row of lights. Installation to include all required hardware and trim.	
	
10126	E-WF.19
	Install fiberglass garage door, 16-0 x 7-0, 4 section 4 panel door with one row of lights. Installation to include all required hardware and trim.	
	
10127	E-WF.19
	Install a 1 car automatic garage door operator in existing garage door installation. Installation to include the automatic control, a 1/4 or better horsepower reversible motor and chain drive. For doors up to 16-0 x 7-0.	
	
10128	E-WF.19
	Install a 2 car automatic garage door operator in existing garage door installation. Installation to include the automatic control, a 1/4 or better horsepower reversible motor and chain drive. For doors up to 16-0 x 7-0.	
	
10129	E-WF.19
	Install a 1 car automatic garage door operator in existing garage door installation. Installation to include the automatic control, a 1/3 or better horsepower reversible motor and chain drive. For doors up to 18-0 x 7-0.	
	
10130	E-WF.19
	Install a 2 car automatic garage door operator in existing garage door installation. Installation to include the automatic control, a 1/3 or better horsepower reversible motor and chain drive. For doors up to 18-0 x 7-0.	
	
12100	E-WF.19
	Install an exterior wood patio door that is economy grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12103	E-WF.19
	Install an exterior wood patio door that is economy grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12104	E-WF.19
	Install an exterior wood patio door that is economy grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12105	E-WF.19
	Install an exterior wood patio door that is economy grade. Installation to include three door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12106	E-WF.19
	Install an exterior wood patio door that is economy grade. Installation to include three door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12110	E-WF.19
	Install an exterior wood patio door that is medium grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12111	E-WF.19
	Install an exterior wood patio door that is medium grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12112	E-WF.19
	Install an exterior wood patio door that is medium grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12113	E-WF.19
	Install an exterior wood patio door that is medium grade. Installation to include three door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12114	E-WF.19
	Install an exterior wood patio door that is medium grade. Installation to include three door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12116	E-WF.19
	Install an exterior aluminum patio door that is premium grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12117	E-WF.19
	Install an exterior aluminum patio door that is premium grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12118	E-WF.19
	Install an exterior aluminum patio door that is premium grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12119	E-WF.19
	Install an exterior aluminum patio door that is premium grade. Installation to include three door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12120	E-WF.19
	Install an exterior wood patio door that is premium grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12121	E-WF.19
	Install an exterior aluminum patio door that is premium grade. Installation to include three door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12122	E-WF.19
	Install an exterior wood patio door that is premium grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12123	E-WF.19
	Install an exterior wood patio door that is premium grade. Installation to include two door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12124	E-WF.19
	Install an exterior wood patio door that is premium grade. Installation to include three door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
12125	E-WF.19
	Install an exterior wood patio door that is premium grade. Installation to include three door panels with insulated glass, and hardware. Apply exterior and interior trim.	
	
14040	E-WF.19
	Install ornamental entrance pilasters that frame the entrance way with 12" wide sidelights.	
	
14041	E-WF.19
	Install ornamental entrance pilasters that frame the entrance way with 6" wide sidelights.	
	
14043	E-WF.19
	Install ornamental entrance pilasters that frame the entrance way, 4".	
	
14044	E-WF.19
	Install ornamental entrance pilasters that frame the entrance way, 6".	
	
14045	E-WF.19
	Install ornamental entrance pilasters that frame the entrance way, 12".	
	
16025	E-WF.19
	Install in existing exterior door a deadbolt lock with outside key and inside thumb turn of premium quality.	
	
16035	E-WF.19
	Install in existing exterior door a deadbolt lock with outside key and inside thumb turn of standard quality.	
	
02007	E-WF.20
	Install hot and cold supply to four areas in a one story house using 3/4 copper tubing. Run 4" PVC drain pipe and 4" PVC soil stack to each area.  Installation includes vent piping using 2" PVC as required.	
	
02008	E-WF.20
	Install hot and cold supply to five  locations in a one story house using 3/4 copper tubing. Run 4" PVC drain pipe and 4" PVC soil stack to each area.  Installation includes vent piping using 2" PVC as required.	
	
02009	E-WF.20
	Install hot and cold supply to six  locations in a one story house using 3/4 copper tubing. Run 4" PVC drain pipe and 4" PVC soil stack to each area.  Installation includes vent piping using 2" PVC as required.	
	
02010	E-WF.20
	Install hot and cold supply to seven  locations in a one story house using 3/4 copper tubing. Run 4" PVC drain pipe and 4" PVC soil stack to each area.  Installation includes vent piping using 2" PVC as required.	
	
02012	E-WF.20
	Install hot and cold supply to four locations in a two story house using 3/4 copper tubing. Run 4" PVC drain pipe and 4" PVC soil stack to each area.  Installation includes vent piping using 2" PVC as required.	
	
02013	E-WF.20
	Install hot and cold supply to five  locations in a two story house using 3/4 copper tubing. Run 4" PVC drain pipe and 4" PVC soil stack to each area.  Installation includes vent piping using 2" PVC as required.	
	
02014	E-WF.20
	Install hot and cold supply to six  locations in a two story house using 3/4 copper tubing. Run 4" PVC drain pipe and 4" PVC soil stack to each area.  Installation includes vent piping using 2" PVC as required.	
	
02022	E-WF.20
	Install 2 new hose bibb. Installation to include necessary plumbing hookups.	
	
02023	E-WF.20
	Install 2 new frost free hose bibbs. Installation to include necessary plumbing hookups.	
	
09017	E-WF.20
	Install 40 gal. gas hot water heater including 2 inches of insulation. Flue and all labor and materials to connect plumbing hookups and gas supply are included in this installation.	
	
09018	E-WF.20
	Install 40 gal. gas hot water heater including 2 inches of insulation. Flue and all labor and materials to connect plumbing hookups and gas supply are included in this installation.	
	
09019	E-WF.20
	Install 40 gal. electric water heater. Installation to include all labor and materials necessary to connect to existing water supply. A 220 volt home run line from existing electrical panel to heater is included in this installation.	
	
09020	E-WF.20
	Install 52 gal. electric water heater. Installation to include all labor and materials necessary to connect to existing water supply. A 220 volt home run line from existing electrical panel to heater is included in this installation.	
	
09021	E-WF.20
	Install 82 gal. electric water heater. Installation to include all labor and materials necessary to connect to existing water supply. A 220 volt home run line from existing electrical panel to heater is included in this installation.	
	
01112	E-WF.21
	Install central vacuum system including power unit and three hose stations in new work. Installation to include hose and cleaning tools as well as necessary tubing and other plumbing-like materials as required. Electrical hookup of existing unit is included.	
	
01113	E-WF.21
	Install on existing central vacuum system additional stations as located. Installation to include necessary tubing installation and control wiring.	
	
02000	E-WF.21
	Install oil fired furnace	
	
02001	E-WF.21
	Install oil fired furnace	
	
02005	E-WF.21
	Install new gas furnace with fiberglass supply and lateral ducts and sheet metal return duct work system. Installation includes re-hooking up gas pipeline that is at the furnace location. Installation does not includes tying to existing electric hookup.	
	
02006	E-WF.21
	Install new gas furnace with fiberglass supply and lateral ducts and sheet metal return duct work system. Installation includes re-hooking up gas pipeline that is at the furnace location. Installation does not includes tying to existing electric hookup.	
	
02009	E-WF.21
	Install oil fired boiler	
	
02010	E-WF.21
	Install oil fired boiler	
	
03012	E-WF.21
	Install new gas boiler with fiberglass supply and lateral ducts and sheet metal return duct work system. Installation includes re-hooking up gas pipeline that is at the furnace location. Installation does not includes tying to existing electric hookup.	
	
03013	E-WF.21
	Install new gas boiler with fiberglass supply and lateral ducts and sheet metal return duct work system. Installation includes re-hooking up gas pipeline that is at the furnace location. Installation does not includes tying to existing electric hookup.	
	
03014	E-WF.21
	Install new gas boiler with fiberglass supply and lateral ducts and sheet metal return duct work system. Installation includes re-hooking up gas pipeline that is at the furnace location. Installation does not includes tying to existing electric hookup.	
	
05002	E-WF.21
	Install oil fired furnace	
	
05003	E-WF.21
	Install oil fired furnace	
	
05007	E-WF.21
	Install new gas furnace and air conditioning with fiberglass supply and lateral ducts and sheet metal return duct work system. Installation includes re-hooking up gas pipeline that is at the furnace location. Installation does not includes tying to existing electric hookup.	
	
05008	E-WF.21
	Install new gas furnace and air conditioning with fiberglass supply and lateral ducts and sheet metal return duct work system. Installation includes re-hooking up gas pipeline that is at the furnace location. Installation does not includes tying to existing electric hookup.	
	
05015	E-WF.21
	Install new electric heat pump on existing duct work system. Heat pump installation to be sized to do both heating and air conditioning with some additional electric resistant heat necessary. Installation to be rated at 19 kW (3 ton). Installation to include all necessary labor and material to install but no electrical connections or hookups are included.	
	
05016	E-WF.21
	Install new electric heat pump on existing duct work system. Heat pump installation to be sized to do both heating and air conditioning with some additional electric resistant heat necessary. Installation to be rated at 19 kW (3 ton). Installation to include all necessary labor and material to install but no electrical connections or hookups are included.	
	
02004	E-WF.22
	Install outlet for garbage disposal. Installation to be on existing 20 amp circuit served with 12 gauge wire and ground.	
	
02005	E-WF.22
	Install outlet for dishwasher. Installation to be on existing 20 amp circuit served with 12 Ga. wire and ground.	
	
02006	E-WF.22
	Install outlet for hood and fan. Installation to be on existing 20 amp. circuit, served with 12 Ga. wire and ground.	
	
02007	E-WF.22
	Install outlet for appliance. Installation to be on existing 20 amp circuit, served with 12 Ga. wire and ground.	
	
02008	E-WF.22
	Install ground fault circuit interrupt outlet on existing 15 or 20 amp. circuit. Installation to include labor for installing GFCI receptacle.	
	
02009	E-WF.22
	Install an approved ground fault circuit interrupt breaker on an15 or 20 amp. branch circuit. Installation to include breaker and installation labor.	
	
02010	E-WF.22
	Install outlet for trash compactor. Installation to be on existing 20 amp. circuit, served with 12 Ga. wire and ground.	
	
02011	E-WF.22
	Install a 220-volt outlet for the hot water heater.  Installation to include necessary labor and material to install outlet receptacle and necessary wiring to existing panel breaker.	
	
02012	E-WF.22
	Install in a 220-volt outlet for an air conditioning unit, clothes dryer, range or oven. Installation to include necessary labor and material to install outlet receptacle and necessary wiring to existing panel breaker.	
	
02100	E-WF.22
	Install duplex outlets in new work. Installation to include circuits to panel box.	
	
02110	E-WF.22
	Install either telephone and or cable outlets in new work. Installation to include circuits to panel box.	
	
03115	E-WF.22
	Install in existing circuit one single pole switch. Installation to include mounting the box and labor to make the installation of the switch.	
	
04111	E-WF.22
	Install thermostatically controlled attic exhaust fan rated at 1100 to 1500 CFM. Installation to include all necessary electrical connection on existing circuit. Installation to be gable mounted.	
	
07000	E-WF.22
	Rent a portable generator to supply electricity.	
	
07001	E-WF.22
	Rough in and finish electric service with new panel breaker box to be installed on existing service cable. Installation to include panel box and breakers as required and to install branch wiring. Duplex outlets installed to code including circuits as required. Fixture installation and cost of fixtures not included. Capacity of new installation to be 200 amp.	
	
07002	E-WF.22
	Rough in and finish electric service with new panel breaker box to be installed on existing service cable. Installation to include panel box and breakers as required and to install branch wiring. Duplex outlets installed to code including circuits as required. Fixture installation and cost of fixtures not included. Capacity of new installation to be 100 amp.	
	
07003	E-WF.22
	Install weatherproof outlet in existing circuit. Installation to include weatherproof box and outlet.	
	
11114	E-WF.22
	Install hardwired automatic smoke and fire detectors. Installation to be code approved. Receptacles and detection devices to be UL listed.	
	
14110	E-WF.22
	Install necessary metal duct work for hood and fan installation. Installation does not include wall break through.	
	
04000	E-WF.24
	Install fiberglass blanket of 3 1/2" depth that is unfaced in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04001	E-WF.24
	Install fiberglass blanket of 6" depth that is unfaced in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04002	E-WF.24
	Install fiberglass blanket of 9" depth that is unfaced in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04003	E-WF.24
	Install fiberglass blanket of 12" depth that is unfaced in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04004	E-WF.24
	Install fiberglass blanket of 3 1/2" depth that is kraftback in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04005	E-WF.24
	Install fiberglass blanket of 6" depth that is kraftback in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04006	E-WF.24
	Install fiberglass blanket of 9" depth that is kraftback in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04007	E-WF.24
	Install fiberglass blanket of 12" depth that is kraftback in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04008	E-WF.24
	Install fiberglass blanket of 3 1/2" depth that is foilback in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04009	E-WF.24
	Install fiberglass blanket of 6" depth that is foilback in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04010	E-WF.24
	Install fiberglass blanket of 9" depth that is foilback in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04011	E-WF.24
	Install fiberglass blanket of 9" depth that is foilback in new work application. Installation to be stapled to open framing or laid flat between ceiling joists on installed drywall.	
	
04012	E-WF.24
	Install fiberglass blanket of 3 1/2" depth that is unfaced in new work application. Installation to be stapled to open 24 "oc framing or laid flat between ceiling joists on installed drywall.	
	
04013	E-WF.24
	Install fiberglass blanket of 6" depth that is unfaced in new work application. Installation to be stapled to open 24 "oc framing or laid flat between ceiling joists on installed drywall.	
	
04014	E-WF.24
	Install fiberglass blanket of 9" depth that is unfaced in new work application. Installation to be stapled to open 24 "oc framing or laid flat between ceiling joists on installed drywall.	
	
04015	E-WF.24
	Install fiberglass blanket of 12" depth that is unfaced in new work application. Installation to be stapled to open 24 "oc framing or laid flat between ceiling joists on installed drywall.	
	
04016	E-WF.24
	Install fiberglass blanket of 3 1/2" depth that is kraftback in new work application. Installation to be stapled to open 24"oc framing or laid flat between ceiling joists on installed drywall.	
	
04017	E-WF.24
	Install fiberglass blanket of 6" depth that is kraftback in new work application. Installation to be stapled to open 24"oc framing or laid flat between ceiling joists on installed drywall.	
	
04018	E-WF.24
	Install fiberglass blanket of 9" depth that is kraftback in new work application. Installation to be stapled to open 24"oc framing or laid flat between ceiling joists on installed drywall.	
	
04019	E-WF.24
	Install fiberglass blanket of 12" depth that is kraftback in new work application. Installation to be stapled to open 24"oc framing or laid flat between ceiling joists on installed drywall.	
	
04020	E-WF.24
	Install fiberglass blanket of 3 1/2" depth that is foilback in new work application. Installation to be stapled to 24" oc open framing or laid flat between ceiling joists on installed drywall.	
	
04021	E-WF.24
	Install fiberglass blanket of 6" depth that is foilback in new work application. Installation to be stapled to 24" oc open framing or laid flat between ceiling joists on installed drywall.	
	
04022	E-WF.24
	Install fiberglass blanket of 9" depth that is foilback in new work application. Installation to be stapled to 24" oc open framing or laid flat between ceiling joists on installed drywall.	
	
04023	E-WF.24
	Install fiberglass blanket of 12" depth that is foilback in new work application. Installation to be stapled to 24" oc open framing or laid flat between ceiling joists on installed drywall.	
	
04107	E-WF.24
	Install blown-in fiberglass insulation in attic area between open ceiling joists where access is unrestricted. Installation will have a R-11 rating.	
	
04108	E-WF.24
	Install blown-in fiberglass insulation in attic area between open ceiling joists where access is unrestricted. Installation will have a R-19 rating.	
	
04109	E-WF.24
	Install blown-in fiberglass insulation in attic area between open ceiling joists where access is unrestricted. Installation will have a R-30 rating.	
	
04110	E-WF.24
	Install blown-in fiberglass insulation in attic area between open ceiling joists where access is unrestricted. Installation will have a R-38 rating.	
	
04111	E-WF.24
	Install blown-in, fire-retardant treated cellulose insulation in unrestricted attic. Installation will have a R-11 rating.	
	
04112	E-WF.24
	Install blown-in, fire-retardant treated cellulose insulation in unrestricted attic. Installation will have a R-19 rating.	
	
04113	E-WF.24
	Install blown-in, fire-retardant treated cellulose insulation in unrestricted attic. Installation will have a R-30 rating.	
	
04114	E-WF.24
	Install blown-in, fire-retardant treated cellulose insulation in unrestricted attic. Installation will have a R-38 rating.	
	
01015	E-WF.25
	Install 1/2" blueboard plaster base on existing framing.	
	
01016	E-WF.25
	Apply skim white coat plaster over installed blueboard with joints and corners to be reinforced.	
	
01017	E-WF.25
	Apply 1/2" blueboard to existing ceiling joists or furring strips. Blueboard to be applied as a base for skim coat plaster.	
	
01100	E-WF.25
	Apply 3/8" gypsum lath nailed to existing ceiling joists or furring strips.	
	
01101	E-WF.25
	Apply 1/2" gypsum lath nailed to existing ceiling joists or furring strips.	
	
01102	E-WF.25
	Apply 3.4 lb. per sq. yd. expanded metal lath to existing ceiling joists or furring strips.	
	
01104	E-WF.25
	Apply gypsum plaster over existing gypsum lath. Plaster to consist of a minimum of one brown coat and one white coat. Finish to be suitable for painting.	
	
01105	E-WF.25
	Apply gypsum plaster over existing gypsum lath. Plaster to consist of a minimum of one brown coat and two white coats. Finish to be suitable for painting.	
	
01106	E-WF.25
	Apply three coats of plaster over existing metal lath. Plaster to be applied with one brown coat and two white or finish coats. Finish to be suitable for painting.	
	
01107	E-WF.25
	Apply skim coat of white plaster to existing blueboard base. Finish to be trowelled suitable for painting.	
	
01115	E-WF.25
	Apply 3/8" gypsum lath to existing wood studs. Installation to include corner beads   as required. Install lath with approved ring shank nails.	
	
01116	E-WF.25
	Apply 1/2" gypsum lath to existing wood studs. Installation to include corner beads   as required. Install lath with approved ring shank nails.	
	
01117	E-WF.25
	Install 3.4 lbs. per square yard, expanded metal lath to existing wood studs. Lath to be installed with approved bluecoat nails. Installation to include all accessories such as corner  bead.	
	
01119	E-WF.25
	Install 1" x 1" wood grounds for plastering. Grounds to be installed around all openings and at floor level.	
	
01121	E-WF.25
	Install gypsum plaster over existing gypsum lath. Installation to be one brown coat and one white coat.	
	
01122	E-WF.25
	Install gypsum plaster over existing gypsum lath. Installation to be three coats with one brown coat and two white coats.	
	
01123	E-WF.25
	Apply gypsum plaster over existing metal lath in three coats. Installation to be one brown coats and two white coats.	
	
01124	E-WF.25
	Apply gypsum plaster over existing wood lath in three coats. Installation to be one brown coats and two white coats.	
	
01127	E-WF.25
	Apply skim coat plaster over taped gypsum or blueboard. Plaster to be lime putty plaster finished, commonly called white coat.	
	
04000	E-WF.25
	Apply gypsum drywall over new framing. Framing to be a maximum of 16" o.c.. and shall include all necessary blocking for drywall installation. Drywall is to be applied to framing members with approved coated drywall nails or screws and fastners to be dimpled for finish purposes. All joints to be taped with either paper or fiberglass tape embedded in pre-manufactured drywall mud with minimum of three coats of joint compound to be applied over the tape. Edges to be feathered and sanded and ready for paint.  Set up charges.	
	
04001	E-WF.25
	Apply 3/8" gypsum drywall over new framing. Framing to be a maximum of 16" o.c.. and shall include all necessary blocking for drywall installation. Drywall is to be applied to framing members with approved coated drywall nails and nails to be dimpled for finish purposes. All joints to be taped with either paper or fiberglass tape embedded in pre-manufactured drywall mud with minimum of three coats of joint compound to be applied over the tape. Edges to be feathered and sanded and ready for paint.	
	
04002	E-WF.25
	Apply 1/2" gypsum drywall over new framing. Framing to be a maximum of 24" o.c.. and shall include all necessary blocking for drywall installation. Drywall is to be applied to framing members with approved coated drywall nails and nails to be dimpled for finish purposes. All joints to be taped with either paper or fiberglass tape embedded in pre-manufactured drywall mud with minimum of three coats of joint compound to be applied over the tape. Edges to be feathered and sanded and ready for paint.	
	
04003	E-WF.25
	Apply 5/8" firecode gypsum drywall over new framing. Framing to be a maximum of 24" o.c.. and shall include all necessary blocking for drywall installation. Drywall is to be applied to framing members with approved coated drywall nails and nails to be dimpled for finish purposes. All joints to be taped with either paper or fiberglass tape embedded in pre-manufactured drywall mud with minimum of three coats of joint compound to be applied over the tape. Edges to be feathered and sanded and ready for paint.	
	
04004	E-WF.25
	Apply 1/2" moisture resistant gypsum drywall over new framing. Framing to be a maximum of 24" o.c.. and shall include all necessary blocking for drywall installation. Drywall is to be applied to framing members with approved coated drywall nails and nails to be dimpled for finish purposes. All joints to be taped with either paper or fiberglass tape embedded in pre-manufactured  drywall mud with minimum of three coats of joint compound to be applied over the tape. Edges to be feathered and sanded and ready for paint.	
	
04009	E-WF.25
	Apply 3/8" drywall over existing studs or furring. This is for installation for drywall board only.	
	
04010	E-WF.25
	Apply 1/2" drywall over existing studs or furring. This is for installation for drywall board only.	
	
04011	E-WF.25
	Apply 5/8" firecode drywall over existing studs or furring. This is for installation for drywall board only.	
	
04012	E-WF.25
	Apply 1/2" moisture resistant drywall over existing studs or furring. This is for installation for drywall board only.	
	
04014	E-WF.25
	Existing drywall board will be finished. Finish to include taping joints and three finish coats. Finish to be sanded, ready for paint.	
	
05001	E-WF.25
	Apply 3/8" drywall board to ceiling joist or furring strips. Board to be nailed with approved ring shank drywall nails or screws with their heads to be dimpled for finish purposes. Joints and nail heads to be finished, with joints to be taped with either paper or fiberglass tape embedded in a taping coat with a minimum of three finish coats to follow. All finish work to be sanded, ready for painting.	
	
05002	E-WF.25
	Apply 1/2" drywall board to ceiling joist or furring strips. Board to be nailed with approved ring shank drywall nails or screws with their heads to be dimpled for finish purposes. Joints and nail heads to be finished, with joints to be taped with either paper or fiberglass tape embedded in a taping coat with a minimum of three finish coats to follow. All finish work to be sanded, ready for painting.	
	
05003	E-WF.25
	Apply 5/8" firecode drywall board to ceiling joist or furring strips. Board to be nailed with  approved ring shank drywall nails or screws with their heads to be dimpled for finish purposes. Joints and nail heads to be finished, with joints to be taped with either paper of fiberglass tape embedded in a taping coat with a minimum of three finish coats to follow.  All finish work to be sanded ready for painting.	
	
05004	E-WF.25
	Apply 1/2" moisture resistant drywall board to ceiling joist or furring strips. Board to be nailed with approved ring shank drywall nails or screws with their heads to be dimpled for finish purposes. Joints and nail heads to be finished, with joints to be taped with either paper or fiberglass tape embedded in a taping coat with a minimum of three finish coats to follow. All finish work to be sanded, ready for painting.	
	
05010	E-WF.25
	Hang 3/8" drywall board applied to ceiling joist or furring strips. No finish is included.	
	
05011	E-WF.25
	Hang 1/2" drywall board applied to ceiling joist or furring strips. No finish is included.	
	
05012	E-WF.25
	Hang 5/8" firecode drywall board applied to ceiling joist or furring strips. No finish is included.	
	
05015	E-WF.25
	Finish existing drywall board. Finish to include taping all joints with either paper or fiberglass tape embedded in taping coat to be followed with three finish coats with finish to be sanded, ready for paint.	
	
11017	E-WF.25
	Spray finished drywall with texturing material. Texture material may be different for ceiling and walls; However, texture    material will be of the same manufacture and color.	
	
11028	E-WF.25
	Spray textured finish material on drywall ceilings. Texture can be of a different texture than wall texture but must be of the same manufacture and color.	
	
01400	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01401	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01402	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01403	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01404	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01405	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01406	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01407	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01408	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01409	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01410	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01411	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01412	E-WF.26
	Install pre-hung mahogany hollow core door, 1-6 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01413	E-WF.26
	Install pre-hung mahogany hollow core door, 1-6 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01414	E-WF.26
	Install pre-hung mahogany hollow core door, 2-4 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01415	E-WF.26
	Install pre-hung mahogany hollow core door, 2-6 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01416	E-WF.26
	Install pre-hung mahogany hollow core door, 2-8 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01417	E-WF.26
	Install pre-hung mahogany hollow core door, 3-0 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01418	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01419	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01420	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01421	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01422	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01423	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01424	E-WF.26
	Install flush pine louvered hollow core door, 1-6 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01425	E-WF.26
	Install flush pine louvered hollow core door, 2-0 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01426	E-WF.26
	Install flush pine louvered hollow core door, 2-4 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01427	E-WF.26
	Install flush pine louvered hollow core door, 2-6 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01428	E-WF.26
	Install flush pine louvered hollow core door, 2-8 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01429	E-WF.26
	Install flush pine louvered hollow core door, 3-0 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01430	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01431	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01432	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01433	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01434	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01435	E-WF.26
	Interior prehung door units to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01436	E-WF.26
	Interior prehung oak door to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01437	E-WF.26
	Interior prehung oak door to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01438	E-WF.26
	Interior prehung oak door to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01439	E-WF.26
	Interior prehung oak door to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01440	E-WF.26
	Interior prehung oak door to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01441	E-WF.26
	Interior prehung oak door to include primed split jamb, stops, hinges and privacy lock. Casing for both sides of door is included.	
	
01500	E-WF.26
	Install flush birch hollow core door, 1-6 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01501	E-WF.26
	Install flush birch hollow core door, 1-8 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01502	E-WF.26
	Install flush birch hollow core door, 2-0 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01503	E-WF.26
	Install flush birch hollow core door, 2-4 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01504	E-WF.26
	Install flush birch hollow core door, 2-6 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01505	E-WF.26
	Install flush birch hollow core door, 3-0 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01506	E-WF.26
	Install flush hardboard hollow core door, 1-6 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01507	E-WF.26
	Install flush hard hardboard hollow core door, 1-8 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01508	E-WF.26
	Install flush hardboard hollow core door, 2-0 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01509	E-WF.26
	Install flush hardboard hollow core door, 2-4 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01510	E-WF.26
	Install flush hardboard hollow core door, 2-6 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01511	E-WF.26
	Install flush hardboard hollow core door, 3-0 x 6-8 x 1 3/8". Installation to include jambs, stop, and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
01512	E-WF.26
	Install colonial 6 panel hardboard faced interior door, 1-6 x 6-8 x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1 pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01513	E-WF.26
	Install colonial 6 panel hardboard faced interior door, 1-8 x 6-8 x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1 pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01514	E-WF.26
	Install colonial 6 panel hardboard faced interior door, 2-0 x 6-8 x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1 pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01515	E-WF.26
	Install colonial 6 panel hardboard faced interior door, 2-4 x 6-8 x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1 pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01516	E-WF.26
	Install colonial 6 panel hardboard faced interior door, 2-6 x 6-8 x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01517	E-WF.26
	Install colonial 6 panel hardboard faced interior door, 3-0 x 6-8 x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1 pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01518	E-WF.26
	Install colonial 6 panel pine hardboard interior door, 1-6 x 6-8x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1 pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01519	E-WF.26
	Install colonial 6 panel pine hardboard interior door, 1-8 x 6-8x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1 pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01520	E-WF.26
	Install colonial 6 panel pine hardboard interior door, 2-0 x 6-8x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1 pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01521	E-WF.26
	Install colonial 6 panel pine hardboard interior door, 2-4 x 6-8x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1 pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01522	E-WF.26
	Install colonial 6 panel pine hardboard interior door, 2-6 x 6-8x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1 pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01523	E-WF.26
	Install colonial 6 panel pine hardboard interior door, 3-0 x 6-8x 1 3/8". Installation includes building the jambs, stops and casing both sides of the door opening. Hardware to include 1 pair of 3 1/2 x 3 1/2 interior butts and privacy lock.	
	
01524	E-WF.26
	Install interior louver pine door, 1-6 x 6-8 x 1 3/8". Installation to include jambs, stops, and both sides of the opening cased. Door design may include cross rail and slats 1/4" x 1 3/8". Hardware to be 1 pair of 3 1/2 x 3 1/2 butts and a  passage set.	
	
01525	E-WF.26
	Install interior louver pine door, 1-8 x 6-8 x 1 3/8". Installation to include jambs, stops, and both sides of the opening cased. Door design may include cross rail and slats 1/4" x 1 3/8". Hardware to be 1 pair of 3 1/2 x 3 1/2 butts and a  passage set.	
	
01526	E-WF.26
	Install interior louver pine door, 2-0 x 6-8 x 1 3/8". Installation to include jambs, stops, and both sides of the opening cased. Door design may include cross rail and slats 1/4" x 1 3/8". Hardware to be 1 pair of 3 1/2 x 3 1/2 butts and a  passage set.	
	
01527	E-WF.26
	Install interior louver pine door, 2-4 x 6-8 x 1 3/8". Installation to include jambs, stops, and both sides of the opening cased. Door design may include cross rail and slats 1/4" x 1 3/8". Hardware to be 1 pair of 3 1/2 x 3 1/2 butts and a  passage set.	
	
01528	E-WF.26
	Install interior louver pine door, 2-6 x 6-8 x 1 3/8". Installation to include jambs, stops, and both sides of the opening cased. Door design may include cross rail and slats 1/4"x 1 3/8". Hardware to be 1 pair of 3 1/2 x 3 1/2 butts and a  passage set.	
	
01529	E-WF.26
	Install interior louver pine door, 3-0 x 6-8 x 1 3/8". Installation to include jambs, stops, and both sides of the opening cased. Door design may include cross rail and slats 1/4" x 1 3/8". Hardware to be 1 pair of 3 1/2 x 3 1/2 butts and a  passage set.	
	
03600	E-WF.26
	Install interior Bi-fold pine louvered or birch hollow core doors, 2 door set, 2-0 x 6-8 x 1 1/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03601	E-WF.26
	Install interior Bi-fold pine louvered or birch hollow core doors, 2 door set, 3-0 x 6-8 x 1 1/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03602	E-WF.26
	Install interior Bi-fold pine louvered or birch hollow core doors, 4 door set, 4-0 x 6-8 x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03603	E-WF.26
	Install interior Bi-fold pine louvered or birch hollow core doors, 4 door set, 5-0 x 6-8 x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03604	E-WF.26
	Install interior Bi-fold pine louvered or birch hollow core doors, 4 door set, 6-0 x 6-8 x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03614	E-WF.26
	Install interior Bi-fold pine louvered doors, 2 door set, 2-0 x 6-8 x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03615	E-WF.26
	Install interior Bi-fold pine louvered doors, 2 door set, 2-6 x 6-8 x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03616	E-WF.26
	Install interior Bi-fold pine louvered doors, 2 door set, 3-0 x 6-8 x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03617	E-WF.26
	Install interior Bi-fold pine louvered doors, 4 door set, 4-0 x 6-8 x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03618	E-WF.26
	Install interior Bi-fold pine louvered doors, 4 door set, 5-0 x 6-8 x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03619	E-WF.26
	Install interior Bi-fold pine louvered doors, 4 door set, 6-0 x 6-8 x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03620	E-WF.26
	Install interior Bi-fold pine panel doors, 2 door set, 2-6 x 6-8x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03621	E-WF.26
	Install interior Bi-fold pine panel doors, 2 door set, 3-0 x 6-8x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03622	E-WF.26
	Install interior Bi-fold pine panel doors, 4 door set, 4-0 x 6-8x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03623	E-WF.26
	Install interior Bi-fold pine panel doors, 4 door set, 5-0 x 6-8x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
03624	E-WF.26
	Install interior Bi-fold pine panel doors, 4 door set, 6-0 x 6-8x 1 3/8". Installation to include jambs, stops, and casing on both sides of opening. Bi-fold hardware to be included.	
	
04645	E-WF.26
	Install interior birch flush hollow core sliding door, 4-0 x 6-8x 1 3/8". Installation to include two doors, jambs, stops, with both sides of the opening to be cased. This will be a double door  installation and includes all necessary hardware.	
	
04646	E-WF.26
	Install interior birch flush hollow core sliding door, 5-0 x 6-8x 1 3/8". Installation to include two doors, jambs, stops, with both sides of the opening to be cased. This will be a double door  installation and includes all necessary hardware.	
	
04647	E-WF.26
	Install interior birch flush hollow core sliding door, 6-0 x 6-8x 1 3/8". Installation to include two doors, jambs, stops, with both sides of the opening to be cased. This will be a double door  installation and includes all necessary hardware.	
	
04648	E-WF.26
	Install interior pine, hemlock or fir louvered sliding door, 4-0x 6-8 x 1 3/8". Installation to include two doors, jambs, stops, with both sides of the opening to be cased. This will be a double door installation and includes all necessary hardware.	
	
04649	E-WF.26
	Install interior pine, hemlock or fir louvered sliding door, 5-0x 6-8 x 1 3/8". Installation to include two doors, jambs, stops, with both sides of the opening to be cased. This will be a double door installation and includes all necessary hardware.	
	
04650	E-WF.26
	Install interior pine, hemlock or fir louvered sliding door, 6-0x 6-8 x 1 3/8". Installation to include two doors, jambs, stops, with both sides of the opening to be cased. This will be a double door installation and includes all necessary hardware.	
	
04651	E-WF.26
	Install interior pine panel sliding door, 4-0 x 6-8 x 1 3/8". Installation to include two doors, jambs, stops, with both sides of the opening to be cased. This will be a double door installation and includes all necessary hardware.	
	
04652	E-WF.26
	Install interior pine, hemlock or fir louvered sliding door, 5-0x 6-8 x 1 3/8". Installation to include two doors, jambs, stops, with both sides of the opening to be cased. This will be a double door installation and includes all necessary hardware.	
	
04653	E-WF.26
	Install interior pine, hemlock or fir louvered sliding door, 6-0x 6-8 x 1 3/8". Installation to include two doors, jambs, stops, with both sides of the opening to be cased. This will be a double door installation and includes all necessary hardware.	
	
05700	E-WF.26
	Install flush birch hollow core door, 2-0 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
05701	E-WF.26
	Install flush birch hollow core door, 2-4 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
05702	E-WF.26
	Install flush birch hollow core door, 2-6 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
05703	E-WF.26
	Install flush birch hollow core door, 3-0 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
05704	E-WF.26
	Install pine hollow core pocket door, 2-0 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
05705	E-WF.26
	Install pine hollow core pocket door, 2-4 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
05706	E-WF.26
	Install pine hollow core pocket door, 2-6 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
05707	E-WF.26
	Install pine hollow core pocket door, 3-0 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2 x 3 1/2 butts with a privacy lock.	
	
05708	E-WF.26
	Install hardboard faced hollow core pocket door, 2-4 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2x 3 1/2 butts with a privacy lock.	
	
05709	E-WF.26
	Install hardboard faced hollow core pocket door, 2-4 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2x 3 1/2 butts with a privacy lock.	
	
05710	E-WF.26
	Install hardboard faced hollow core pocket door, 2-6 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2x 3 1/2 butts with a privacy lock.	
	
05711	E-WF.26
	Install hardboard faced hollow core pocket door, 3-0 x 6-8 x 1 3/8". Installation to include track and roller hardware and casing both sides of the opening. Hardware to be 1 pair of 3 1/2x 3 1/2 butts with a privacy lock.	
	
03409	E-WF.27
	Install an medium grade countertop of plastic laminate with metal or self edge. Installation to include 4" backsplash.	
	
03410	E-WF.27
	Install ceramic tile countertop including trim. Installation to be mud set ceramic tile.	
	
03411	E-WF.27
	Install ceramic tile countertop including trim. Installation to be mastic set ceramic tile.	
	
03412	E-WF.27
	Install custom cutting board constructed of 1 1/2" x 18" x 25" laminated maple. Installation to be in new countertop.	
	
05100	E-WF.27
	Install factory built builder grade base cabinets to include a minimum installation of a 36" wide base sink two door unit as well as a 24" four drawer unit, plus any door and drawer units as required to complete the installation. Cabinets shall meet or exceed the recommended minimum construction and performance standards as set by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document and may be done by others.	
	
05101	E-WF.27
	Install factory built builder grade wall cabinets with the minimum installation to include two 15" high door units, 36" wide and as many 30" high units as required. Cabinets shall meet or exceed the recommended minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05102	E-WF.27
	Install factory built additional builder grade drawer unit with 4 drawers 15" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05103	E-WF.27
	Install factory built additional builder grade drawer unit with 4 drawers 18" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05104	E-WF.27
	Install factory built additional builder grade drawer unit with 4 drawers 21" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05105	E-WF.27
	Install factory built additional builder grade drawer unit with 4 drawers 24" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05106	E-WF.27
	Install factory built additional builder grade sink or burner base, 30" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05107	E-WF.27
	Install factory built additional builder grade sink or burner base, 36" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05108	E-WF.27
	Install factory built additional builder grade sink or burner base, 42" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05113	E-WF.27
	Install factory built builder grade island base 30" wide, doors 2 sides & drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05114	E-WF.27
	Install factory built builder grade island base 36" wide, doors 2 sides & drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05115	E-WF.27
	Install factory built builder grade island base 42" wide, doors 2 sides & drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05116	E-WF.27
	Install factory built builder grade island base 48" wide, doors 2 sides & drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05117	E-WF.27
	Install factory built builder grade corner base (lazy Susan) with 36" along each wall. Cabinets shall meet or exceed the minimum construction and performance standards set forth by American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05118	E-WF.27
	Install factory built additional builder grade broom cabinet 18" x 12", 7' high. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05119	E-WF.27
	Install factory built additional builder grade broom cabinet 18" x 24", 7' high. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
05120	E-WF.27
	Install factory built builder grade oven cabinet 18" x 12", 7' high. Cabinets shall meet or exceed the minimum construction and performance standards set by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06200	E-WF.27
	Install factory built premium grade base cabinets to include a minimum installation of a 36" wide base sink two door unit as well as a 24" four drawer unit, plus any door and drawer units as required to complete the installation. Cabinets shall meet or exceed the recommended minimum construction and performance standards as set by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document and may be done by others.	
	
06201	E-WF.27
	Install factory built premium grade wall cabinets with the minimum installation to include two 15" high door units, 36" wide and as many 30" high units as required. Cabinets shall meet or exceed the recommended minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06202	E-WF.27
	Install factory built additional premium grade drawer unit with 4 drawers 15" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06203	E-WF.27
	Install factory built additional premium grade drawer unit with 4 drawers 18" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06204	E-WF.27
	Install factory built additional premium grade drawer unit with 4 drawers 21" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06205	E-WF.27
	Install factory built additional premium grade drawer unit with 4 drawers 24" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06206	E-WF.27
	Install factory built additional premium grade sink or burner base, 30" wide. Cabinets shall meet or exceed the       minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06207	E-WF.27
	Install factory built additional premium grade sink or burner base, 36" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06208	E-WF.27
	Install factory built additional premium grade sink or burner base, 42" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06213	E-WF.27
	Install factory built premium grade island base 30" wide, doors 2 sides & drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06214	E-WF.27
	Install factory built premium grade island base 36" wide, doors 2 sides & drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06215	E-WF.27
	Install factory built premium grade island base 42" wide, doors 2 sides & drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06216	E-WF.27
	Install factory built premium grade island base 48" wide, doors 2 sides & drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06217	E-WF.27
	Install factory built premium grade corner base (lazy Susan) with 36" along each wall. Cabinets shall meet or exceed the minimum construction and performance standards set forth by American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06218	E-WF.27
	Install factory built additional premium grade broom cabinet 18" x 12", 7' high. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06219	E-WF.27
	Install factory built additional premium grade broom cabinet 18" x 24", 7' high. Cabinets shall meet or exceed the  minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
06220	E-WF.27
	Install factory built premium grade oven cabinet 18" x 12", 7' high. Cabinets shall meet or exceed the minimum construction and performance standards set by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in  this document.	
	
06300	E-WF.27
	Install factory built top quality grade base cabinet to include minimum installation of a 36" wide base sink two door unit as well as a 24" four drawer unit, plus any door and drawer units as required to complete the installation. Cabinets shall meet or exceed the recommended minimum construction and performance standards as set by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document and may be done by others.	
	
06301	E-WF.27
	Install factory built top quality wall cabinets with the minimum installation to include two 15" high door units, 36" wide and as many 30" high units as required. Cabinets shall meet or exceed the recommended minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07302	E-WF.27
	Install factory built additional top quality grade drawer unit with 4 drawers 15" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07303	E-WF.27
	Install factory built additional top quality grade drawer unit with 4 drawers 18" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07304	E-WF.27
	Install factory built additional top quality grade drawer unit with 4 drawers 21" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07305	E-WF.27
	Install factory built additional top quality grade drawer unit with 4 drawers 24" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07306	E-WF.27
	Install factory built additional top quality grade sink or burner base 30" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07307	E-WF.27
	Install factory built additional top quality grade sink or burner base 36" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07308	E-WF.27
	Install factory built additional top quality grade sink or burner base 42" wide. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07309	E-WF.27
	Install factory built additional top quality sink or burner front, 30" with no sides. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07313	E-WF.27
	Install factory built top quality grade island base 24" wide, doors 2 sides, drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07314	E-WF.27
	Install factory built top quality grade island base 36" wide, doors 2 sides, drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07315	E-WF.27
	Install factory built top quality grade island base 42" wide, doors 2 sides, drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07316	E-WF.27
	Install factory built top quality grade island base 48" wide, doors 2 sides, drawers 1 side. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07317	E-WF.27
	Install factory built top quality grade corner base (lazy Susan) with 36" along each wall. Cabinets shall meet or exceed the minimum construction and performance standards set forth by American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in  this document.	
	
07318	E-WF.27
	Install factory built top quality grade broom cabinet 18" x 12",7' high. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07319	E-WF.27
	Install factory built top quality grade broom cabinet 18" x 24",7' high. Cabinets shall meet or exceed the minimum construction and performance standards set forth by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in this document.	
	
07320	E-WF.27
	Install factory built top quality grade oven cabinet 18" x 12", 7' high. Cabinets shall meet or exceed the minimum construction and performance standards set by the American National Standards Institute (ANSI). Cabinets are to be factory finished or the finish will be specified later in  this document.	
	
09413	E-WF.27
	Install bulkhead and drywall from ceiling to top of cabinets as required.	
	
11000	E-WF.27
	Install economy grade clothes washer with the installation to include all labor and fittings that are required. Also included are the necessary plumbing and electrical connections.	
	
11001	E-WF.27
	Install medium grade clothes washer with the installation to include all labor and fittings that are required. Also included are the necessary plumbing and electrical connections.	
	
11002	E-WF.27
	Install premium grade clothes washer with the installation to include all labor and fittings that are required. Also included are the necessary plumbing and electrical connections.	
	
11003	E-WF.27
	Install electric dryer with an economy grade electric clothes dryer.	
	
11004	E-WF.27
	Install electric dryer with a medium grade electric clothes dryer.	
	
11005	E-WF.27
	Install electric dryer with a premium grade electric clothes dryer.	
	
11006	E-WF.27
	Install economy grade gas clothes dryer with the installation to include all labor and fittings that are required. Also included are the necessary plumbing, electrical and gas connections, to include necessary gas venting.	
	
11007	E-WF.27
	Install medium grade gas clothes dryer with the installation to include all labor and fittings that are required. Also included are the necessary plumbing, electrical and gas connections, to include necessary gas venting.	
	
11008	E-WF.27
	Install premium grade gas clothes dryer with the installation to include all labor and fittings that are required. Also included are the necessary plumbing, electrical and gas connections, to include necessary gas venting.	
	
11009	E-WF.27
	Install 28" x 20" electric cooktop, using existing electrical connections. Any additional materials or fittings required are included in this installation.	
	
11010	E-WF.27
	Install 35" x 20" electric cooktop, using existing electrical connections. Any additional materials or fittings required are included in this installation.	
	
11011	E-WF.27
	Install electric double wall oven, using existing electrical connections. Any additional materials or fittings required are included in this installation.	
	
11012	E-WF.27
	Install electric single wall oven, using existing electrical connections. Any additional materials or fittings required are included in this installation.	
	
11013	E-WF.27
	Install electric free standing range, economy grade, using existing electrical connections. Any additional materials or fittings required are included in this installation.	
	
11014	E-WF.27
	Install electric free standing range, medium grade, using existing electrical connections. Any additional materials or fittings required are included in this installation.	
	
11015	E-WF.27
	Install electric free standing range, premium grade, using existing electrical connections. Any additional materials or fittings required are included in this installation.	
	
11500	E-WF.27
	Install gas cooktop, 28" x 20" with the installation to include all labor and fittings that are required. Also included are the necessary plumbing, electrical and gas connections, to include necessary gas venting.	
	
11501	E-WF.27
	Install gas cooktop, 35" x 20" with the installation to include all labor and fittings that are required. Also included are the necessary plumbing, electrical and gas connections, to include necessary gas venting.	
	
11502	E-WF.27
	Install gas wall oven, double, with the installation to include all labor and fittings that are required. Also included are the necessary plumbing, electrical and gas connections, to include necessary gas venting.	
	
11503	E-WF.27
	Install gas wall oven, single, with the installation to include all labor and fittings that are required. Also included are the necessary plumbing, electrical and gas connections, to include necessary gas venting.	
	
11504	E-WF.27
	Install free standing gas range, economy grade, with the installation to include all labor and fittings that are required. Also included are the necessary plumbing, electrical and gas connections, to include necessary gas venting.	
	
11505	E-WF.27
	Install free standing gas range, medium grade, with the installation to include all labor and fittings that are required. Also included are the necessary plumbing, electrical and gas connections, to include necessary gas venting.	
	
11506	E-WF.27
	Install free standing gas range, premium grade, with the installation to include all labor and fittings that are required. Also included are the necessary plumbing, electrical and gas connections, to include necessary gas venting.	
	
11507	E-WF.27
	Install microwave oven with economy grade microwave oven. Installation to include any changes to electrical hookups as required.	
	
11508	E-WF.27
	Install microwave oven with medium grade microwave oven. Installation to include any changes to electrical hookups as required.	
	
11509	E-WF.27
	Install microwave oven with premium grade microwave oven. Installation to include any changes to electrical hookups as required.	
	
11510	E-WF.27
	Install refrigerator with economy grade refrigerator. Installation to include any changes to electrical hookups as required.	
	
11511	E-WF.27
	Install refrigerator with medium grade refrigerator. Installation to include any changes to electrical hookups as required.	
	
11512	E-WF.27
	Replace existing refrigerator with premium grade refrigerator. Installation to include any changes to electrical hookups as required.	
	
01200	E-WF.28
	Apply 12 x 12 or 12 x 24 tile over existing ceiling or furring strips. Apply tile with hidden staples or adhesive in a pattern that squares up the existing room. Any cut tile should be along the exterior walls. Tile to have retail cost of .35 per SF.	
	
01201	E-WF.28
	Apply 12 x 12 or 12 x 24 tile over existing ceiling or furring strips. Apply tile with hidden staples or adhesive in a pattern that squares up the existing room. Any cut tile should be along the exterior walls. Tile to have retail cost of .40 per SF.	
	
01202	E-WF.28
	Apply 12 x 12 or 12 x 24 tile over existing ceiling or furring strips. Apply tile with hidden staples or adhesive in a pattern that squares up the existing room. Any cut tile should be along the exterior walls. Tile to have retail cost of .45 per SF.	
	
01203	E-WF.28
	Apply 12 x 12 or 12 x 24 tile over existing ceiling or furring strips. Apply tile with hidden staples or adhesive in a pattern that squares up the existing room. Any cut tile should be along the exterior walls. Tile to have retail cost of .50 per SF.	
	
01204	E-WF.28
	Apply 12 x 12 or 12 x 24 tile over existing ceiling or furring strips. Apply tile with hidden staples or adhesive in a pattern that squares up the existing room. Any cut tile should be along the exterior walls. Tile to have retail cost of .55 per SF.	
	
01205	E-WF.28
	Apply 12 x 12 or 12 x 24 tile over existing ceiling or furring strips. Apply tile with hidden staples or adhesive in a pattern that squares up the existing room. Any cut tile should be along the exterior walls. Tile to have retail cost of .60 per SF.	
	
01206	E-WF.28
	Apply 12 x 12 or 12 x 24 tile over existing ceiling or furring strips. Apply tile with hidden staples or adhesive in a pattern that squares up the existing room. Any cut tile should be along the exterior walls. Tile to have retail cost of .70 per SF.	
	
01207	E-WF.28
	Apply 12 x 12 or 12 x 24 tile over existing ceiling or furring strips. Apply tile with hidden staples or adhesive in a pattern that squares up the existing room. Any cut tile should be along the exterior walls. Tile to have retail cost of .80 per SF.	
	
01208	E-WF.28
	Install 1 x 3 furring strips, 12" o.c... ready for the installation of ceiling tile. Furring strips to be laid out so that any wall irregularities will be along both exterior walls.	
	
01211	E-WF.28
	Apply suspended ceiling with steel grid system using 24" x 48" sections. Installation to include entire "T" grid system and ceiling tile panels. Panels to be 24" x 48" and to have a retail cost per SF of .50. Ceiling grid system to be hung level and with any irregularity in ceiling dimensions to occur at outside walls.	
	
01212	E-WF.28
	Apply suspended ceiling with steel grid system using 24" x 48" sections. Installation to include entire "T" grid system and ceiling tile panels. Panels to be 24" x 48" and to have a retail cost per SF of .55. Ceiling grid system to be hung level and  with any irregularity in ceiling dimensions to occur at outside walls.	
	
01213	E-WF.28
	Apply suspended ceiling with steel grid system using 24" x 48" sections. Installation to include entire "T" grid system and ceiling tile panels. Panels to be 24" x 48" and to have a retail cost per SF of .60. Ceiling grid system to be hung level and with any irregularity in ceiling dimensions to occur at outside walls.	
	
01214	E-WF.28
	Apply suspended ceiling with steel grid system using 24" x 48" sections. Installation to include entire "T" grid system and ceiling tile panels. Panels to be 24" x 48" and to have a retail cost per SF of .65. Ceiling grid system to be hung level and  with any irregularity in ceiling dimensions to occur at outside walls.	
	
01215	E-WF.28
	Apply suspended ceiling with steel grid system using 24" x 48" sections. Installation to include entire "T" grid system and ceiling tile panels. Panels to be 24" x 48" and to have a retail cost per SF of .70. Ceiling grid system to be hung level and  with any irregularity in ceiling dimensions to occur at outside walls.	
	
01216	E-WF.28
	Apply suspended ceiling with steel grid system using 24" x 48" sections. Installation to include entire "T" grid system and ceiling tile panels. Panels to be 24" x 48" and to have a retail cost per SF of .75. Ceiling grid system to be hung level and  with any irregularity in ceiling dimensions to occur at outside walls.	
	
01217	E-WF.28
	Apply suspended ceiling with steel grid system using 24" x 48" sections. Installation to include entire "T" grid system and ceiling tile panels. Panels to be 24" x 48" and to have a retail cost per SF of .80. Ceiling grid system to be hung level and  with any irregularity in ceiling dimensions to occur at outside walls.	
	
02200	E-WF.28
	Install ceramic tile in mud. Installation to include installing metal lath over existing wood studs, then applying scratch coat with 4 1/4" x 4 1/4" ceramic tile. Installation includes cove and bullnose where required.	
	
02201	E-WF.28
	Install ceramic tile in mud. Installation to include installing metal lath over existing wood studs, then applying scratch coat with 4 1/4" x 4 1/4" ceramic tile. Installation includes cove and bullnose where required.	
	
02202	E-WF.28
	Install ceramic tile in mud. Installation to include installing metal lath over existing wood studs, then applying scratch coat with 4 1/4" x 4 1/4" ceramic tile. Installation includes cove and bullnose where required.	
	
02203	E-WF.28
	Install 4 1/4" x 4 1/4" ceramic tile over existing backer board or moisture resistant drywall. Installation to be tile set in thin set mastic and include cove and bullnose tile as needed.	
	
02204	E-WF.28
	Install 4 1/4" x 4 1/4" ceramic tile over existing backer board or moisture resistant drywall. Installation to be tile set in thin set mastic and include cove and bullnose tile as needed.	
	
02205	E-WF.28
	Install 4 1/4" x 4 1/4" ceramic tile over existing backer board or moisture resistant drywall. Installation to be tile set in thin set mastic and include cove and bullnose tile as needed.	
	
02206	E-WF.28
	Ceramic tile bathroom fixtures. Fixtures are a set to include one towel bar, toothbrush holder, paper holder and soap and grab.	
	
01002	E-WF.29
	Install 3 1/2" pine clam, ranch or colonial base. Install base with either coped or mitred joints.  All finish nails to be set, ready for spackling.	
	
01003	E-WF.29
	Install 4 1/2" pine clam, ranch or colonial base. Install base with either coped or mitred joints.  All finish nails to be set, ready for spackling.	
	
01007	E-WF.29
	Install 1 1/2" x 3/4" hardwood shoe molding. Install shoe to base to allow movement in the floor.	
	
01008	E-WF.29
	Install 1 1/2" x 3/4" pine shoe molding. Install shoe to base to allow movement in the floor.	
	
01009	E-WF.29
	Apply 3-piece base molding to consist of 11/16" x 1 1/2" top mould and a 11/16" x 3 1/2" base mould and 1 1/2" x 3/4" shoe. Molding should be applied in such a way that joints do not overlap. All nails should be set and ready for spackling.	
	
01010	E-WF.29
	Apply 3/4" bed, cove, crown or picture molding to joint between ceiling and wall. When applying ceiling moldings in multiple  applications overlap joints. All nails to be set, ready for spackling.	
	
01016	E-WF.29
	Install 3-piece crown moulding to be made up of crown and bed pieces that are 5/8" x 1 3/4" and 3/4" x 4 3/4" and 5/8" x 1 3/4". Individual molding pieces to be installed in such a way that the joints overlap and joints are either coped or mitred. Nails are to be set and ready for spackle.	
	
01017	E-WF.29
	Install 1-piece chair rail, 5/8" x 2 1/2", at a uniform horizontal height above the floor. Joints to be mitred or coped with nails to be set, ready for spackle.	
	
01018	E-WF.29
	Install 1-piece chair rail, 5/8" x 3 1/2", at a uniform horizontal height above the floor. Joints to be mitred or coped with nails to be set, ready for spackle.	
	
01019	E-WF.29
	Install 2-piece chair rail to include 2 1/2" rail with cap trim. Joints to be mitred or coped and not to overlap. Nails to be  set, ready for spackling.	
	
01020	E-WF.29
	Install 5/8" x 7/8" strips nailed to existing plaster or drywall wall to create panel effect. All joints to be mitred or coped  and nails set, ready for spackle.	
	
01021	E-WF.29
	Install 1 1/16" x 2 1/4" strips nailed to existing plaster or drywall wall to create panel effect. All joints to be mitred or coped and nails set, ready for spackle.	
	
01030	E-WF.29
	Install pre-manufactured architectural cornice mould to appear as crown and bed pieces that are in fact a single piece.  Individual molding piece to be installed in such a way that the joints overlap and joints are either coped or mitered. Nails are to be set and ready for spackle and finish.	
	
01301	E-WF.29
	Trim a 24" to 30" deep closet with #2 pine base and shoe molding, #2 hook strap, two 12" particleboard shelves and two 1 3/8" poles installed in clothes pole sockets. Installation to be ready for paint or other finish.	
	
04011	E-WF.29
	Apply 1 5/8" bed, cove, crown or picture molding to joint between ceiling and wall. When applying ceiling moldings in multiple applications overlap joints. All nails to be set, ready for spackling.	
	
04012	E-WF.29
	Apply 2 1/4" bed, cove, crown or picture molding to joint between ceiling and wall. When applying ceiling moldings in multiple applications overlap joints. All nails to be set, ready for spackling.	
	
04013	E-WF.29
	Apply 3 1/4" bed, cove, crown or picture molding to joint between ceiling and wall. When applying ceiling moldings in multiple applications overlap joints. All nails to be set, ready for spackling.	
	
04014	E-WF.29
	Apply 4 1/4" bed, cove, crown or picture molding to joint between ceiling and wall. When applying ceiling moldings in multiple applications overlap joints. All nails to be set, ready for spackling.	
	
04015	E-WF.29
	Apply 5 1/4" bed, cove, crown or picture molding to joint between ceiling and wall. When applying ceiling moldings in multiple applications overlap joints. All nails to be set, ready for spackling.	
	
04114	E-WF.29
	Install a pre-assembled economy grade fireplace mantel. Mantel to be pine or equal with plane or fluted sides. Installation to include top shelf up to 12" wide with the overall width to be up to 72". Installation to be ready for paint or other finish.	
	
04115	E-WF.29
	Install a pre-assembled medium grade fireplace mantel. Mantel to be pine or equal with plane or fluted sides. Installation to include top shelf up to 12" wide with the overall width to be up to 72". Installation to be ready for paint or other finish.	
	
04116	E-WF.29
	Install a pre-assembled premium grade fireplace mantel. Mantel to be pine or equal with plane or fluted sides. Installation to include top shelf up to 12" wide with the overall width to be up to 72". Installation to be ready for paint or other finish.	
	
04117	E-WF.29
	Install plain pine fireplace surround molding with no shelf. Surround molding to be up to 1 5/8" x 5 3/4". Installation to be ready for paint or other finish.	
	
05300	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $10 per 4' x 8' sheet.	
	
05301	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $11 per 4' x 8' sheet.	
	
05302	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $12 per 4' x 8' sheet.	
	
05303	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $13 per 4' x 8' sheet.	
	
05304	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $14 per 4' x 8' sheet.	
	
05305	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $15 per 4' x 8' sheet.	
	
05306	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $16 per 4' x 8' sheet.	
	
05307	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $17 per 4' x 8' sheet.	
	
05308	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $18 per 4' x 8' sheet.	
	
05309	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $19 per 4' x 8' sheet.	
	
05310	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $20 per 4' x 8' sheet.	
	
05311	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $25 per 4' x 8' sheet.	
	
05312	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $30 per 4' x 8' sheet.	
	
05313	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $35 per 4' x 8' sheet.	
	
05314	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $40 per 4' x 8' sheet.	
	
05315	E-WF.29
	Install prefinished 1/4" x 4' x 8' sheets of paneling. Sheets to be installed over existing wood studs, furring or drywall. Paneling to be purchased at retail for $45 per 4' x 8' sheet.	
	
05316	E-WF.29
	Install unfinished, v-joint, 3/4" thick wood paneling. Paneling to be knotty pine and in random widths up to 10" wide. Installation to include 1 x 4 base of the same material to which the paneling is butted.	
	
05317	E-WF.29
	Install unfinished, v-joint, 3/4" thick wood paneling. Paneling to be cedar and in random widths up to 10" wide. Installation to include 1 x 4 base of the same material to which the paneling is butted.	
	
05318	E-WF.29
	Install unfinished, v-joint, 3/4" thick wood paneling. Paneling to be redwood and in random widths up to 10" wide. Installation to include 1 x 4 base of the same material to which the paneling is butted.	
	
05319	E-WF.29
	Install 3/8" T & G (tongue and groove) cedar closet lining. With material to be end matched and applied over existing solid wall.	
	
05320	E-WF.29
	Install 1/4" cedar particle board closet lining. With material to be end matched and applied over existing solid wall.	
	
06305	E-WF.29
	Install main stairway that has one side open to the living area. Starting newel, birch handrail with easement and newel cap, pine balusters, oak treads and risers. Stairway to be shop built and installed on job by stair builders.	
	
06306	E-WF.29
	Install main stairway that has two sides open to the living area. Starting newel, birch handrail with easement and newel cap, pine balusters, oak treads and risers. Stairway to be shop built and installed on job by stair builders.	
	
06307	E-WF.29
	Install main stairway that has one side open to the living area. Starting newel, birch handrail with easement and newel cap, pine balusters, oak treads and risers. Stairway to be shop built and installed on job by stair builders.	
	
06308	E-WF.29
	Install main stairway that has two sides open to the living area. Starting newel, birch handrail with easement and newel cap, pine balusters, oak treads and risers. Stairway to be shop built and installed on job by stair builders.	
	
06309	E-WF.29
	Install closed main stairway. Starting newel, birch handrail with easement and newel cap, pine balusters, oak treads and risers. Stairway to be shop built and installed on job by stair builders.	
	
06310	E-WF.29
	Install straight run stairway between two walls to attic or banestringers with 1 1/8" pine treads and 3/4" pine risers. Installation to include fir handrail installed on two metal handrail brackets. Stairs to be shop built and installed on job by stair builder.	
	
06321	E-WF.29
	Install folding wood disappearing stairway up to 10-0 floor height that is 26" wide. Install in existing framed opening. Installation to be ready for paint or other finish.	
	
08100	E-WF.29
	Install exterior wood door shutters with stationary slats. Shutters to be installed without hinges and are decorative only. Installation to be ready for paint or other finish.	
	
08101	E-WF.29
	Install exterior plastic door shutters with stationary slats. Shutters to be installed without hinges and are decorative only. Installation to be ready for paint or other finish.	
	
08102	E-WF.29
	Install exterior aluminum door shutters with stationary slats. Shutters to be installed without hinges and are decorative only. Installation to be ready for paint or other finish.	
	
08103	E-WF.29
	Install exterior aluminum door shutters with stationary slats. Shutters to be installed without hinges and are decorative only. Installation to be ready for paint or other finish.	
	
08104	E-WF.29
	Install exterior wood window shutters with stationary slats. Shutters to be installed without hinges and are decorative only. Installation to be ready for paint or other finish.	
	
08105	E-WF.29
	Install exterior plastic window shutters with stationary slats. Shutters to be installed without hinges and are decorative only. Installation to be ready for paint or other finish.	
	
08106	E-WF.29
	Install exterior aluminum window shutters with stationary slats. Shutters to be installed without hinges and are decorative only. Installation to be ready for paint or other finish.	
	
08107	E-WF.29
	Install window shutters with on hinges.	
	
10302	E-WF.29
	Install additional storage shelves in closet. Installation to be #2 pine or plywood set on wood cleats with width of shelves to be 12". Installation to be ready for paint or other finish.	
	
10303	E-WF.29
	Install additional storage shelves in closet. Installation to be #2 pine or plywood set on wood cleats with width of shelves to be 16". Installation to be ready for paint or other finish.	
	
10304	E-WF.29
	Install in existing linen closet shelving that is 24" deep, 12" o.c... measured vertically. Installation to include pine base and pine shelf cleats. Shelves to be 24" o.c... vertically. Installation to be ready for paint or other finish.	
	
03020	E-WF.30
	Install wall mirror that is 1/4" thick with polished edges, attached to wall with clips or adhesive.	
	
13001	E-WF.30
	Install in framed recess, a recessed medicine cabinet with hinged plate glass mirror door. Overall size of cabinet to be 16" x 22".	
	
13003	E-WF.30
	Install in framed recess, a recessed medicine cabinet with hinged two mirror doors, overhead light. Overall size of cabinet to be 27" x 23".	
	
13004	E-WF.30
	Install surface mounted cabinet in bathroom that has two sliding glass mirror doors and overall size of 24" x 16".	
	
13005	E-WF.30
	Install surface mounted cabinet in bathroom that has two sliding glass mirror doors and overall size of 24" x 23". Cabinet installation to include an overhead 4-bulb fixture.	
	
13006	E-WF.30
	Install surface mounted cabinet in bathroom that has two sliding glass mirror doors and overall size of 28" x 23". Cabinet installation to include an overhead 4-bulb fixture.	
	
13007	E-WF.30
	Install surface mounted cabinet in bathroom that has two sliding glass mirror doors and overall size of 36" x 23". Cabinet installation to include an overhead 4-bulb fixture.	
	
13021	E-WF.30
	Install polished chrome bath accessories: Towel bar, toothbrush and glass holder, paper holder and soap dish.	
	
13022	E-WF.30
	Install chrome shower curtain rod 5' in length.	
	
14008	E-WF.30
	Install aluminum framed tub enclosure with folding plastic panel doors. Roller guides top and bottom with doors to fold to 12" up to a 66" opening with doors to be 58" high. Installation to include complete caulking around and under frame before and after installation.	
	
14009	E-WF.30
	Install an aluminum framed shower enclosure with plastic panels. Installation to be caulked around and under aluminum frame before and after installation.	
	
14010	E-WF.30
	Install aluminum framed tub enclosure with two plastic bypass panel doors 58" high up to 60" opening. Installation to include complete caulking of frame before and after installation.	
	
14012	E-WF.30
	Install aluminum framed tub enclosure with two tempered glass bypass panel doors 70" high up to 48" opening. Installation to include complete caulking of frame before and after installation.	
	
14014	E-WF.30
	Install an aluminum framed shower enclosure with two tempered glass doors for a 48" opening. Installation to be caulked around and under aluminum frame before and after installation.	
	
14015	E-WF.30
	Install an aluminum framed tub enclosure with one hinged door and one stationary panel for a 48" opening. Installation to be caulked around and under aluminum frame before and after installation.	
	
14016	E-WF.30
	Install an aluminum framed shower enclosure with one hinged door and one stationary panel for a 48" opening. Installation to be caulked around and under aluminum frame before and after installation.	
	
14017	E-WF.30
	Install a neo-angle glass shower enclosure with frame to have aluminum finish. Enclosure to have 24" side panels with a 27" door. Enclosure to be 72" high with obscure glass. Installation to be caulked around and under aluminum frame before and after enclosure is installed.	
	
14018	E-WF.30
	Install a neo-angle glass shower enclosure with frame to have brass finish. Enclosure to have 24" side panels with a 27" door. Enclosure to be 72" high with obscure glass. Installation to be caulked around and under aluminum frame before and after enclosure is installed.	
	
01000	E-WF.31
	Install red oak select grade hardwood flooring that is 3/4" x 2 1/4" on prepared subsurface. Lay tongue and groove in matched oak flooring in such a pattern that all irregularities of room dimensions are absorbed in the outside walls. Nailing to be blind in all courses except the starter course. Installation does not include sanding or finishing.	
	
01001	E-WF.31
	Install unfinished #1 common grade hardwood flooring that is 25/32" x 2 1/4" on prepared subsurface. Lay tongue and groove in matched oak flooring in such a pattern that all irregularities of room dimensions are absorbed in the outside walls. Nailing to be blind in all courses except the starter course. Installation does not include sanding or finishing.	
	
01002	E-WF.31
	Install pre-finished select grade oak flooring that is 25/32" x 2 1/4" on prepared subsurface. Lay tongue and groove in matched oak flooring in such a pattern that all irregularities of room dimensions are absorbed in the outside walls. Nailing to be blind in all courses except the starter course.	
	
01003	E-WF.31
	Install pre-finished ranch plank flooring with installation to be screwed and wood plugs installed.	
	
01005	E-WF.31
	Install 12" x 12" x 1/2" oak laminated parquet flooring set in mastic over concrete or plywood subsurface. Parquet to be tongue and groove, pre-finished clear flooring.	
	
01011	E-WF.31
	Install unfinished maple flooring that is 1" x 3" on prepared subsurface. Lay tongue and groove in matched oak flooring in such a pattern that all irregularities of room dimensions are absorbed in the outside walls. Nailing to be blind in all courses except the starter set. Installation does not include sanding or finishing.	
	
02108	E-WF.31
	Lay B-grade asphalt tile in adhesive over smooth prepared surface that is above grade.	
	
02109	E-WF.31
	Lay C-grade asphalt tile in adhesive over smooth prepared surface that is above grade.	
	
02110	E-WF.31
	Lay D-grade asphalt tile in adhesive over smooth prepared surface that is above grade.	
	
02111	E-WF.31
	Lay 9" x 9" vinyl composition tile that is 1/16" thick in adhesive over a smooth prepared subsurface.	
	
02112	E-WF.31
	Lay 9" x 9" vinyl composition tile that is 3/32" thick in adhesive over a smooth prepared subsurface.	
	
02113	E-WF.31
	Lay 9" x 9" vinyl composition tile that is 1/8" thick in adhesive over a smooth prepared subsurface.	
	
02114	E-WF.31
	Lay 12" x 12" vinyl composition tile that is 1/16" thick in adhesive over a smooth prepared subsurface.	
	
02115	E-WF.31
	Lay 12" x 12" vinyl composition tile that is 3/32" thick in adhesive over a smooth prepared subsurface.	
	
02116	E-WF.31
	Lay 12" x 12" vinyl composition tile that is 1/8" thick in adhesive or a smooth prepared subsurface.	
	
02117	E-WF.31
	Lay 9" x 9" vinyl tile that is 1/16" thick in adhesive over a smooth prepared subsurface.	
	
02118	E-WF.31
	Lay 9" x 9" vinyl tile that is 3/32" thick in adhesive over a smooth prepared subsurface.	
	
02119	E-WF.31
	Lay 9" x 9" vinyl tile that is 1/8" thick in adhesive over a smooth prepared subsurface.	
	
02120	E-WF.31
	Lay 12" x 12" vinyl tile that is 1/16" thick in adhesive over a smooth prepared subsurface.	
	
02121	E-WF.31
	Lay 12" x 12" vinyl tile that is 1/8" thick in adhesive over a smooth prepared subsurface.	
	
02122	E-WF.31
	Lay 12" x 12" vinyl tile that is premium grade in adhesive over a smooth prepared subsurface.	
	
02123	E-WF.31
	Lay economy grade resilient sheet vinyl flooring in adhesive over a smooth prepared subsurface.	
	
02124	E-WF.31
	Lay medium grade resilient sheet vinyl flooring in adhesive over a smooth prepared subsurface.	
	
02125	E-WF.31
	Lay premium grade resilient sheet vinyl flooring in adhesive over a smooth prepared subsurface.	
	
02126	E-WF.31
	Apply 2 1/2" vinyl base in adhesive. Base installation to include necessary corners.	
	
02127	E-WF.31
	Apply 4" vinyl base in adhesive. Base installation to include necessary corners.	
	
03201	E-WF.31
	Set 4 1/4" x 4 1/4", 6" x 6" or 8" x 8" ceramic floor tile in mud. Installation to include necessary cove, base or bullnose trim.	
	
03202	E-WF.31
	Set 4 1/4" x 4 1/4", 6" x 6" or 8" x 8" ceramic floor tile in mastic.  Installation to include necessary cove, base or bullnose trim.	
	
03203	E-WF.31
	Set 1/2" or 3/4" thick quarry floor tile in adhesive to smooth prepared subsurface. Tile can be 4" x 4", 6" x 6" or 8" x 8".	
	
03204	E-WF.31
	Set 1" thick paver floor tile over prepared subsurface, tile may be 4" x 4" or 6" x 6".	
	
03205	E-WF.31
	Set 3/8" thick, 12" x 12" marble floor tile on smooth prepared subsurface.	
	
04209	E-WF.31
	Install interior carpeting including padding that is of a $12 per yd. retail grade. Installation to include tack strips and necessary metal edges.	
	
04210	E-WF.31
	Install interior carpeting including padding that is of a $15 per yd. retail grade. Installation to include tack strips necessary metal edges.	
	
04211	E-WF.31
	Install interior carpeting including padding that is of a $20 per yd. retail grade. Installation to include tack strips and necessary metal edges.	
	
04212	E-WF.31
	Install interior carpeting including padding that is of a $25 per yd. retail grade. Installation to include tack strips and necessary metal edges.	
	
05100	E-WF.31
	Install 3/8" plywood under-layment as base for resilient floor. Under-layment to be nailed over existing floor ready for floor covering.	
	
05101	E-WF.31
	Install 1/2" plywood under-layment as base for resilient floor. Under-layment to be nailed over existing floor ready for floor covering.	
	
05102	E-WF.31
	Install 5/8" plywood under-layment as base for resilient floor. Under-layment to be nailed over existing floor, ready for floor covering.	
	
05103	E-WF.31
	Install 3/4" plywood under-layment as base for resilient floor. Under-layment to be nailed over existing floor ready for floor covering.	
	
05104	E-WF.31
	Install 3/8" particleboard under-layment as base for resilient floor.  Under-layment to be nailed over existing floor, ready for floor covering.	
	
05105	E-WF.31
	Install 1/2" particleboard under-layment as base for resilient floor. Under-layment to be nailed over existing floor, ready for floor covering.	
	
05106	E-WF.31
	Install 5/8" particleboard under-layment as base for resilient floor. Under-layment to be nailed over existing floor, ready for floor covering.	
	
05107	E-WF.31
	Install 3/4" particleboard under-layment as base for resilient floor. Under-layment to be nailed over existing floor, ready for floor covering.	
	
06006	E-WF.31
	Sand and finish existing new floor with a natural finish. Sanding to be a three step process followed by a three coat finish application.	
	
06007	E-WF.31
	Sand and finish existing new floor with a dark stain finish. Sanding to be a three step process followed by a three coat finish application.	
	
03200	E-WF.32
	Install 2 piece floor mounted water closet located within 5' of an existing stack and including the cost of rough " An allowance of $105 for the water closet, $20 for the seat, and $20 for the supply is allowed.	
	
03201	E-WF.32
	Install 2 piece floor wall hung water closet located within 5' of an existing stack and including the cost of rough " An allowance of $105 for the water closet, $20 for the seat, and $20 for the supply is allowed.	
	
03202	E-WF.32
	Install 1 piece floor mounted water closet located within 5' of an existing stack and including the cost of rough " An allowance of $305 for the water closet, $25 for the seat, and $20 for the supply is allowed.	
	
03205	E-WF.32
	Install floor mounted bidet within 5' of an existing stack including the cost of rough " An allowance for the bidet of $200, and $350 for brass fittings is allowed.	
	
03206	E-WF.32
	Install 5' cast iron bathtub within of 5' of an existing stack including the cost of rough " An allowance of $250 for the cast iron tub, $60 for the faucet set, and $75 for the drain assembly is allowed.	
	
03207	E-WF.32
	Install 5' steel bathtub within of 5' of an existing stack including the cost of rough " An allowance of $150 for the steel tub, $60 for the faucet set, and $75 for the drain assembly is allowed.	
	
03209	E-WF.32
	Cost of installation to a bathtub for an acrylic finish.	
	
03210	E-WF.32
	Install fiberglass whirlpool tub, 5' x 30" x 18" deep, within 5' of an existing stack including the cost of rough " Whirlpool is to have a minimum of 3 jets and includes skirting; however  the cost of electrical hookups and ceramic tile are not included. $1580 is the allowance for the whirlpool assembly.	
	
03211	E-WF.32
	Rough in and install within 5' of an existing stack a fiberglass shower stall. Fiberglass shower stall unit to be preformed and include pan and necessary plumbing hardware.	
	
03212	E-WF.32
	Rough in and install within 5' of an existing stack a fiberglass shower stall. Fiberglass shower stall unit to be preformed and include pan and necessary plumbing hardware.	
	
03213	E-WF.32
	Rough in and install within 5' of an existing stack a fiberglass shower stall. Fiberglass shower stall unit to be preformed and include pan and necessary plumbing hardware.	
	
03214	E-WF.32
	Rough in and install within 5' of an existing stack a fiberglass shower stall. Fiberglass shower stall unit to be preformed and include pan and necessary plumbing hardware.	
	
03215	E-WF.32
	Rough in and install within 5' of an existing stack a fiberglass shower stall. Fiberglass shower stall unit to be preformed and include pan and necessary plumbing hardware.	
	
03216	E-WF.32
	Rough in and install within 5' of an existing stack a fiberglass tub/shower enclosure. Fiberglass enclosure to be preformed and include necessary plumbing hardware.	
	
03217	E-WF.32
	Install 20" x 18" wall hung lavatory within 5' of existing stack including the costs of rough " Installation to include the  lavatory, faucet, trap assembly. An allowance of $80 for lavatory, $50 for faucet set, $30 for trap assembly is allowed.	
	
03218	E-WF.32
	Install 17" x 19" vitreous china lavatory bowl within 5' of existing stack including the costs of rough " Installation to include the  lavatory, faucet, trap assembly. An allowance of $80 for lavatory, $50 for faucet set, $30 for trap assembly is allowed.	
	
03219	E-WF.32
	Install pedestal sink within 5' of an existing stack including the cost of rough " An allowance of $220 for the pedestal sink, $50 for the faucet set, and $30 for the trap assembly is allowed.	
	
03220	E-WF.32
	Install pedestal sink within 5' of an existing stack including the cost of rough " An allowance of $220 for the pedestal sink, $50 for the faucet set, and $30 for the trap assembly is allowed.	
	
03300	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 24" deep. Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03301	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 24" deep. Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03302	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 30" deep.  Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03303	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 30" deep.  Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03304	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 36" deep.  Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03305	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 36" deep.  Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03306	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 42" wide. Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03307	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 42" deep.  Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03308	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 48" wide.  Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03309	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 48" deep.  Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03310	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 60" wide.  Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03311	E-WF.32
	Install prefinished vanity base cabinet, 30" x 21" and 60" deep.  Installation to be located within 5" of an existing stack and includes the cost of rough " An allowance for the vanity.	
	
03312	E-WF.32
	Install plastic laminate vanity top 22" or 25" in depth.  Installation to include 4" back splash. Installation to be located within 5" of an existing stack.  Assembly is allowed.	
	
03313	E-WF.32
	Install plastic laminate vanity top 22" or 25" in depth.  Installation to include 4" back splash. Installation to be located within 5" of an existing stack.	
	
03314	E-WF.32
	Install vanity top in prefinished vanity base cabinet, 21" x 24"with imitation marble top including bowl. Installation to include 4" back splash. Installation to be located within 5" of an existing stack and includes the cost of rough in .
	
03315	E-WF.32
	Install vanity top in prefinished vanity base cabinet, 31" x 22" with imitation marble top including bowl. Installation to include 4" back splash. Installation to be located within 5" of an existing stack and includes the cost of rough in .
	
03316	E-WF.32
	Install vanity top in prefinished vanity base cabinet, 37" x 22"with imitation marble top including bowl. Installation to include 4" back splash. Installation to be located within 5" of an existing stack and includes the cost of rough in .
	
03317	E-WF.32
	Install vanity top in prefinished vanity base cabinet, 49" x 22"with imitation marble top including bowl. Installation to include 4" back splash. Installation to be located within 5" of an existing stack and includes the cost of rough in .
	
03318	E-WF.32
	Install vanity top in prefinished vanity base cabinet, 61" x 22"with imitation marble top including bowl. Installation to include 4" back splash. Installation to be located within 5" of an existing stack and includes the cost of rough in .
	
03319	E-WF.32
	Install 16" x 19" porcelain vanity lavatory bowl within 5' of existing stack including the costs of rough " Installation to include the  lavatory, faucet, trap assembly. An allowance of $80 for lavatory, $50 for faucet set, $30 for trap assembly is allowed.	
	
03320	E-WF.32
	Install 16" x 19" enameled steel vanity lavatory bowl within 5' of existing stack including the costs of rough " Installation to include the  lavatory, faucet, trap assembly. An allowance of$80 for lavatory, $50 for faucet set, $30 for trap assembly is allowed.	
	
03321	E-WF.32
	Install 16" x 19" vitreous china vanity lavatory bowl within 5' of existing stack including the costs of rough " Installation to include the  lavatory, faucet, trap assembly. An allowance of$80 for lavatory, $50 for faucet set, $30 for trap assembly is allowed.	
	
04100	E-WF.32
	Rough in and install cast iron kitchen single sink, including faucet and spray with 2 strainers. Installation to include all labor for plumbing and electrical work that is required. Extension of drain and water pipes as required.	
	
04101	E-WF.32
	Rough in and install cast iron kitchen double sink, including faucet and spray with 2 strainers. Installation to include all labor for plumbing and electrical work that is required. Extension of drain and water pipes as required. 	
	
04102	E-WF.32
	Rough in and install stainless steel kitchen single sink, including faucet and spray with 2 strainers. Sink size of 24" x 21". Installation to include all labor for plumbing and electrical work that is required. Extension of drain and water pipes as required.	
	
04103	E-WF.32
	Rough in and install stainless steel kitchen double sink, including faucet and spray with 2 strainers. Installation to include all labor for plumbing and electrical work that is required. Extension of drain and water pipes as required.	
	
04104	E-WF.32
	Rough in and install stainless steel kitchen triple sink, including faucet and spray with 2 strainers. Installation to include all labor for plumbing and electrical work that is required. Extension of drain and water pipes as required.	
	
04105	E-WF.32
	Install instant hot water device next to existing sink. Installation to include labor and material necessary for both the electrical and plumbing hookups.	
	
04106	E-WF.32
	Install in existing sink a new 1/3 hp garbage disposer to include electrical rough in .
	
04107	E-WF.32
	Install in existing sink a new 1/2 hp garbage disposer to include electrical rough in .
	
04108	E-WF.32
	Install new medium grade dishwasher next to existing sink. Installation to include all necessary electrical and plumbing rough in .
	
04109	E-WF.32
	Install new premium grade dishwasher next to existing sink. Installation to include all necessary electrical and plumbing rough in .
	
06110	E-WF.32
	Install new polypropylene 20 gallon laundry sink, including rubber stopper, raised soap dish and drain assembly with faucet.	
	
01013	E-WF.34
	Install 3-Way Switch set in existing circuit. Installation to include mounting the box and labor to make the installation of the switch.	
	
01015	E-WF.34
	Install 12" x 12" recessed lighting fixture in new work. Installation to include fixture, outlet box and switch to be installed on existing circuit.	
	
01016	E-WF.34
	Install 12" fluorescent kitchen fixture under existing kitchen cabinet. Fixture to include switch. Installation to include labor and material necessary to hook fixture up to existing circuit.	
	
01017	E-WF.34
	Install 2 outside spotlights on eaves of house at first floor location. Installation to include interior wall mounted switch on existing circuit.	
	
01018	E-WF.34
	Install 2 outside spotlights on eaves of house at second floor location. Installation to include interior wall mounted switch on existing circuit.	
	
01020	E-WF.34
	Install outside fixture over door or at the side of door. Installation does not include the cost of fixture. Installation to include interior wall mounted switch installed on existing circuit.	
	
03019	E-WF.34
	Install a fixture. Installation to include fixture and wall mounted switch and necessary boxes. Labor and material for electrical connections to existing circuit is included; however, the fixture is additional.	
	
04014	E-WF.34
	Install fluorescent bath fixture over existing medicine cabinet. Fixture to be one tube and one plug, installation includes outlet and switch as well as fixture.	
	
04100	E-WF.34
	Install bathroom exhaust fan. Installation to include necessary box and switches necessary to install fan. Fan and box are included in this installation.	
	
04101	E-WF.34
	Supply and install 1000 watt combination bathroom fan and heater. Installation to be on existing circuit and includes necessary wiring for wall mounted switch.	
	
04102	E-WF.34
	Supply and install 1000 watt combination bathroom fan, heater and light. Installation to be on existing circuit and includes necessary wiring for wall mounted switch.	
	
04103	E-WF.34
	Supply and install ceiling or wall mounted bathroom exhaust fan.  Installation to be on existing circuit.	
	
04104	E-WF.34
	Supply and install 30" ductless range hood. Installation to include labor and material necessary to install hood on existing electrical circuit.	
	
04105	E-WF.34
	Supply and install 36" ductless range hood. Installation to include labor and material necessary to install hood on existing electrical circuit.	
	
04106	E-WF.34
	Supply and install 42" ductless range hood. Installation to include labor and material necessary to install hood on existing electrical circuit.	
	
04107	E-WF.34
	Supply and install 30" range hood. Installation to include ducting to nearest exterior wall. Installation to include electrical hookup on existing circuit. Installation does not include duct vent or any necessary wall or ceiling repairs.	
	
04108	E-WF.34
	Supply and install 36" range hood. Installation to include ducting to nearest exterior wall. Installation to include electrical hookup on existing circuit. Installation does not include duct vent or any necessary wall or ceiling repairs.	
	
04109	E-WF.34
	Supply and install 42" range hood. Installation to include ducting to nearest exterior wall. Installation to include electrical hookup on existing circuit. Installation does not include duct vent or any necessary wall or ceiling repairs.	
	
04118	E-WF.36
	Install a pine, pre-assembled china corner case of economy grade. Overall height to 7-4 with overall width to 2-6. Installation to be ready for paint or other finish.	
	
04119	E-WF.36
	Install a pine, pre-assembled china corner case of medium grade. Overall height to 7-4 with overall width to 2-6. Installation to be ready for paint or other finish.	
	
04120	E-WF.36
	Install a pine, pre-assembled china corner case of premium grade. Overall height to 7-4 with overall width to 2-6. Installation to be ready for paint or other finish.	
	
04300	E-WF.36
	Trim a 24" to 30" deep closet with #2 pine base and shoe molding, #2 hook strap, 12" particleboard shelf and 1 3/8" pole installed in clothes pole socket. Installation to be ready for paint or other finish.	
	
02101	E-WF.37
	Paint prime and one coat with brush over wood, plywood, asbestos or composition siding. Application to include all necessary   clean-up and protection of items not to be painted.	
	
02102	E-WF.37
	Paint prime and two coats with brush over wood, plywood, asbestos or composition siding. Application to include all necessary clean-up and protection of items not to be painted.	
	
02104	E-WF.37
	Paint prime and one coat with roller over wood, plywood, asbestos or composition siding. Application to include all necessary clean-up and protection of items not to be painted.	
	
02105	E-WF.37
	Paint prime and two coats with roller over wood, plywood, asbestos or composition siding. Application to include all necessary clean-up and protection of items not to be painted.	
	
02107	E-WF.37
	Paint prime and one coat with spray gun over wood, plywood, asbestos or composition siding. Application to include all necessary clean-up and protection of items not to be painted.	
	
02108	E-WF.37
	Paint prime and two coats with spray gun over wood, plywood, asbestos or composition siding. Application to include all necessary clean-up and protection of items not to be painted.	
	
02109	E-WF.37
	Stain one coat with brush over wood, plywood, asbestos or composition siding. Application to include all necessary clean-up and protection of items not to be stained.	
	
02110	E-WF.37
	Stain two coats with brush over wood, plywood, asbestos or composition siding. Application to include all necessary clean-up and protection of items not to be stained.	
	
02117	E-WF.37
	Paint wood shingles or rough siding with brush, prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
02118	E-WF.37
	Paint wood shingles or rough siding with brush, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
02120	E-WF.37
	Paint wood shingles or rough siding with spray gun, prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
02121	E-WF.37
	Paint wood shingles or rough siding with spray gun, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
02122	E-WF.37
	Stain wood shingles or rough siding with brush, one coat. Application to include necessary clean-up and protection of items not to be stained.	
	
02123	E-WF.37
	Stain wood shingles or rough siding with brush, two coats. Application to include necessary clean-up and protection of items not to be stained.	
	
02124	E-WF.37
	Stain wood shingles or rough siding with spray gun, one coat. Application to include necessary clean-up and protection of items not to be stained.	
	
02125	E-WF.37
	Stain wood shingles or rough siding with spray gun, two coats. Application to include necessary clean-up and protection of items not to be stained.	
	
02127	E-WF.37
	Paint smooth brick or stucco with roller, prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
02128	E-WF.37
	Paint smooth brick or stucco with roller, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
02130	E-WF.37
	Paint smooth brick or stucco with spray gun, prime and one coat. Application to include necessary clean-up and protection of   items not to be painted.	
	
02131	E-WF.37
	Paint smooth brick or stucco with spray gun, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
02133	E-WF.37
	Paint porous brick or stucco with roller, prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
02134	E-WF.37
	Paint porous brick or stucco with roller, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
02136	E-WF.37
	Paint porous brick or stucco with spray gun, prime and one coat. Application to include necessary clean-up and protection of   items not to be painted.	
	
02137	E-WF.37
	Paint porous brick or stucco with spray gun, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
03525	E-WF.37
	Paint one side of a flush or panel door including casing and one side of jamb with brush. Application to be prime and one coat  with necessary clean-up and protection of items not to be painted.	
	
03526	E-WF.37
	Paint one side of a flush or panel door including casing and one side of jamb with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03528	E-WF.37
	Paint one side of a flush or panel door including casing and one side of jamb with roller. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03529	E-WF.37
	Paint one side of a flush or panel door including casing and one side of jamb with roller. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03530	E-WF.37
	Stain and/or clear finish one side of a flush or panel door including casing and one side of jamb with brush. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
03531	E-WF.37
	Stain and/or clear finish one side of a flush or panel door including casing and one side of jamb with brush. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
03532	E-WF.37
	Stain and/or clear finish one side of a flush or panel door including casing and one side of jamb with brush. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
03534	E-WF.37
	Paint both sides of louver door including casing and jamb with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03535	E-WF.37
	Paint both sides of louver door including casing and jamb with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03536	E-WF.37
	Stain and/or clear finish both sides of louver door including casing and jamb with brush. Application to be one coat with necessary clean-up and protection of items not to be painted.	
	
03537	E-WF.37
	Stain and/or clear finish both sides of louver door including casing and jamb with brush. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
03538	E-WF.37
	Stain and/or clear finish both sides of louver door including casing and jamb with brush. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
03540	E-WF.37
	Paint both sides of bifold door unit up to 5-0 wide including casing and jamb with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03541	E-WF.37
	Paint both sides of bifold door unit up to 5-0 wide including casing and jamb with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03542	E-WF.37
	Stain and/or clear finish both sides of bifold door unit up to 5-0 wide including casing and jamb with brush. Application to be one coat with necessary clean-up and protection of items not to be painted.	
	
03543	E-WF.37
	Stain and/or clear finish both sides of bifold door unit up to 5-0 wide including casing and jamb with brush. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
03544	E-WF.37
	Stain and/or clear finish both sides of bifold door unit up to 5-0 wide including casing and jamb with brush. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
03602	E-WF.37
	Paint one side only of a wood or metal window including all trim. Window dimension from 1-8 to 3-4.  Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03604	E-WF.37
	Paint one side only of a wood or metal window including all trim. Window dimension from 1-8 to 3-0. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03605	E-WF.37
	Paint one side only of a wood or metal window including all trim. Window dimension from 1-8 to 3-0. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03606	E-WF.37
	Paint one side only of a wood or metal window including all trim. Window dimension from 1-8 to 3-4.  Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03607	E-WF.37
	Paint one side only of a wood or metal window including all trim, 12-16 lights. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03608	E-WF.37
	Paint one side only of a wood or metal window including all trim, 4 lights. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03609	E-WF.37
	Paint one side only of a wood or metal window including all trim, 12-16 lights. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03610	E-WF.37
	Paint one side only of a wood or metal window including all trim, 12-16 lights. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03614	E-WF.37
	Stain and/or clear finish one side only of a wood or metal window including all trim. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
03615	E-WF.37
	Stain and/or clear finish one side only of a wood or metal window including all trim.  Window dimension from 1-8 to 3-0. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
03616	E-WF.37
	Stain and/or clear finish one side only of a wood or metal window including all trim. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
03617	E-WF.37
	Stain and/or clear finish one side only of a wood or metal window including all trim.  Window dimension from 1-8 to 3-0. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
03618	E-WF.37
	Stain and/or clear finish one side only of a wood or metal window including all trim, 1-2 lights. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
03619	E-WF.37
	Stain and/or clear finish one side only of a wood or metal window including all trim, 12-16 lights. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
03620	E-WF.37
	Stain and/or clear finish one side only of a wood or metal window including all trim, 1-2 lights. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
03621	E-WF.37
	Stain and/or clear finish one side only of a wood or metal window including all trim, 12-16 lights. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
03624	E-WF.37
	Additional required for work on ladder or scaffolding.	
	
03625	E-WF.37
	Paint divided light grilles for each window installed. Use one coat of paint.	
	
03626	E-WF.37
	Paint divided light grilles for each window installed. Use two coats of paint.	
	
03701	E-WF.37
	Paint smooth finish plaster or drywall wall with roller. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03702	E-WF.37
	Paint smooth finish plaster or drywall wall with roller. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03704	E-WF.37
	Paint smooth finish plaster or drywall wall with spray gun. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03705	E-WF.37
	Paint smooth finish plaster or drywall wall with spray gun. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03707	E-WF.37
	Paint wood paneled walls with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03708	E-WF.37
	Paint wood paneled walls with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03710	E-WF.37
	Paint wood paneled walls with roller. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03711	E-WF.37
	Paint wood paneled walls with roller. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03712	E-WF.37
	Stain and/or clear finish wood paneled walls with roller. Application to be one coat with necessary clean-up and protection of items not to be painted.	
	
03713	E-WF.37
	Stain and/or clear finish wood paneled walls with roller. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
03714	E-WF.37
	Stain and/or clear finish wood paneled walls with roller. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
03725	E-WF.37
	Paint smooth finish plaster or drywall ceiling with roller. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03726	E-WF.37
	Paint smooth finish plaster or drywall ceiling with roller. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03728	E-WF.37
	Paint smooth finish plaster or drywall ceiling with spray gun. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03729	E-WF.37
	Paint smooth finish plaster or drywall ceiling with spray gun. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03731	E-WF.37
	Paint textured finish plaster or drywall ceiling with roller. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03732	E-WF.37
	Paint textured finish plaster or drywall ceiling with roller. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03734	E-WF.37
	Paint textured finish plaster or drywall ceiling with spray gun. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
03735	E-WF.37
	Paint textured finish plaster or drywall ceiling with spray gun. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03738	E-WF.37
	Paint wood Tongue and Groove ceiling with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
03739	E-WF.37
	Paint wood Tongue and Groove ceiling with roller. Application to be one coat on painted surface with necessary clean-up and protection of items not to be painted.	
	
03826	E-WF.37
	Paint stairway and trim with brush, two coats, cost per riser. Application to include necessary clean-up and protection of items not to be painted.	
	
03827	E-WF.37
	Paint stairway and trim with brush, prime and one coat, stairway 7 to 8 risers.  Application to include necessary clean-up and protection of items not to be painted.	
	
03828	E-WF.37
	Paint stairway and trim with brush, prime and one coat, stairway 14 to 16 risers. Application to include necessary clean-up and protection of items not to be painted.	
	
04201	E-WF.37
	Paint exterior molding and trim with brush, prime and one coat. Application to include necessary clean-up and protection of   items not to be painted.	
	
04202	E-WF.37
	Paint exterior molding and trim with brush, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
04204	E-WF.37
	Paint fascia up to 12" wide with brush, including one face and edge. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04205	E-WF.37
	Paint fascia up to 12" wide with brush, including one face and edge. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04207	E-WF.37
	Paint soffit up to 12" wide with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04208	E-WF.37
	Paint soffit up to 12" wide with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04210	E-WF.37
	Paint soffit up to 12" wide with roller. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04211	E-WF.37
	Paint soffit up to 12" wide with roller. Application to be prime and two coats with necessary clean-up and protection of items  not to be painted.	
	
04213	E-WF.37
	Paint soffit up to 12" wide with spray gun. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04214	E-WF.37
	Paint soffit up to 12" wide with spray gun. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04216	E-WF.37
	In open eaves with brush, all sides of rafters, interior of fascia and the underside of roof sheathing is to be painted. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04217	E-WF.37
	In open eaves with brush, all sides of rafters, interior of fascia and the underside of roof sheathing is to be painted. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04219	E-WF.37
	In open eaves with spray gun, all sides of rafters, interior of fascia and the underside of roof sheathing is to be painted. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04220	E-WF.37
	In open eaves with spray gun, all sides of rafters, interior of fascia and the underside of roof sheathing is to be painted. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04401	E-WF.37
	Paint metal gutters and/or downspouts with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04402	E-WF.37
	Paint metal gutters and/or downspouts with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04404	E-WF.37
	Paint wood gutter, 4" x 5" with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04405	E-WF.37
	Paint wood gutter, 4" x 5" with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04406	E-WF.37
	Paint wood lattice work all sides with brush, two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
04407	E-WF.37
	Paint wood lattice work all sides with brush, two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
04408	E-WF.37
	Paint wood lattice work all sides with spray gun, one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
04409	E-WF.37
	Paint wood lattice work all sides with spray gun, two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
04410	E-WF.37
	Paint wood columns and pilasters with brush, one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
04411	E-WF.37
	Paint wood columns and pilasters with brush, two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
04412	E-WF.37
	Paint wood columns and pilasters with spray gun, one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
04413	E-WF.37
	Paint wood columns and pilasters with spray gun, two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
04415	E-WF.37
	Paint wood or metal flush entrance door all sides, including jamb and casing with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04416	E-WF.37
	Paint wood or metal flush entrance door all sides, including jamb and casing with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04418	E-WF.37
	Paint wood or metal flush entrance door on all sides, including jamb and casing with roller. Application to be prime and one  coat with necessary clean-up and protection of items not to be painted.	
	
04419	E-WF.37
	Paint wood or metal flush entrance door on all sides, including jamb and casing with roller. Application to be prime and two  coats with necessary clean-up and protection of items not to be painted.	
	
04420	E-WF.37
	Stain and/or clear finish wood or metal flush entrance door on all sides, including jamb and casing with brush. Application to be one coat with necessary clean-up and protection of items not to be painted.	
	
04421	E-WF.37
	Stain and/or clear finish wood or metal flush entrance door on all sides, including jamb and casing with brush. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
04422	E-WF.37
	Stain and/or clear finish wood or metal flush entrance door on all sides, including jamb and casing with brush. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
04424	E-WF.37
	Paint wood or metal 2-6 panel entrance door, on all sides, including jamb and casing with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04425	E-WF.37
	Paint wood or metal 2-6 panel entrance door, on all sides, including jamb and casing with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04426	E-WF.37
	Stain and/or clear finish wood or metal 2-6 panel entrance door, on all sides, including jamb and casing with brush. Application to be one coat with necessary clean-up and protection of items not to be painted.	
	
04427	E-WF.37
	Stain and/or clear finish wood or metal 2-6 panel entrance door, on all sides, including jamb and casing with brush. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
04428	E-WF.37
	Stain and/or clear finish wood or metal 2-6 panel entrance door, one side only, including jamb and casing with brush. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
04429	E-WF.37
	Paint 2-6 light wood door, one side only, including jamb and casing with brush. Application to be one coat on painted surface with necessary clean-up and protection of items not to be painted.	
	
04430	E-WF.37
	Paint 2-6 light wood door, on all sides, including jamb and casing with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04431	E-WF.37
	Paint 2-6 light wood door, on all sides, including jamb and casing with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04432	E-WF.37
	Stain and/or clear finish 2-6 light wood door, on all sides, including jamb and casing with brush. Application to be one coat with necessary clean-up and protection of items not to be painted.	
	
04433	E-WF.37
	Stain and/or clear finish 2-6 light wood door, on all sides, including jamb and casing with brush. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
04434	E-WF.37
	Stain and/or clear finish 2-6 light wood door, on all sides, including jamb and casing with brush. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
04436	E-WF.37
	Paint 9-15 light French door, on all sides, including jamb and casing with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04437	E-WF.37
	Paint 9-15 light French door, on all sides, including jamb and casing with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04438	E-WF.37
	Stain and/or clear finish 9-15 light French door, on all sides, including jamb and casing with brush. Application to be one coat with necessary clean-up and protection of items not to be painted.	
	
04439	E-WF.37
	Stain and/or clear finish 9-15 light French door, on all sides , including jamb and casing with brush. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
04440	E-WF.37
	Stain and/or clear finish 9-15 light French door, on all sides , including jamb and casing with brush. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
04441	E-WF.37
	Paint a single wood Colonial entrance door with brush. Application to be one coat on painted surface with necessary clean-up and protection of items not to be painted.	
	
04443	E-WF.37
	Paint a single wood Colonial entrance door with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04445	E-WF.37
	Paint a single wood Colonial entrance door with two sidelights with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04446	E-WF.37
	Paint a single wood Colonial entrance door with two sidelights with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04501	E-WF.37
	Paint gliding patio door on all sides, including exterior jamb and casing. Paint with brush, two panels, prime and one coat.  Application to include necessary clean-up and protection of items not to be painted.	
	
04502	E-WF.37
	Paint gliding patio door, on all sides, including exterior jamb and casing. Paint with brush, two panels, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
04507	E-WF.37
	Paint gliding patio door on all sides, including exterior jamb and casing. Paint with brush, three panels, prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
04508	E-WF.37
	Paint gliding patio door on all sides, including exterior jamb and casing. Paint with brush, three panels, prime and two coats.  Application to include necessary clean-up and protection of items not to be painted.	
	
04513	E-WF.37
	Paint wood garage door on both sides, including jamb and casing. Paint 9-0 x 7-0 door with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04514	E-WF.37
	Paint wood garage door on both sides, including jamb and casing. Paint 9-0 x 7-0 door with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04516	E-WF.37
	Paint wood garage door on both sides, including jamb and casing. Paint 9-0 x 7-0 door with spray gun. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04517	E-WF.37
	Paint wood garage door on both sides, including jamb and casing. Paint 9-0 x 7-0 door with spray gun. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04519	E-WF.37
	Paint wood garage door on both sides, including jamb and casing. Paint 16-0 x 7-0 door with brush. Application to be prime and  one coat with necessary clean-up and protection of items not to be painted.	
	
04520	E-WF.37
	Paint wood garage door on both sides, including jamb and casing. Paint 16-0 x 7-0 door with brush. Application to be prime and  two coats with necessary clean-up and protection of items not to be painted.	
	
04522	E-WF.37
	Paint wood garage door on both sides, including jamb and casing. Paint 16-0 x 7-0 door with spray gun. Application to be prime  and one coat with necessary clean-up and protection of items not to be painted.	
	
04523	E-WF.37
	Paint wood garage door on both sides, including jamb and casing. Paint 16-0 x 7-0 door with spray gun. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04716	E-WF.37
	Paint base or ceiling molding, chair rail, door or window trim up to 6", with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04717	E-WF.37
	Paint base or ceiling molding, chair rail, door or window trim up to 6", with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04718	E-WF.37
	Stain and/or clear finish base or ceiling molding, chair rail, door or window trim up to 6", with brush. Application to be one coat with necessary clean-up and protection of items not to be painted.	
	
04719	E-WF.37
	Stain and/or clear finish base or ceiling molding, chair rail, door or window trim up to 6", with brush. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
04720	E-WF.37
	Stain and/or clear finish base or ceiling molding, chair rail, door or window trim up to 6", with brush. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
04801	E-WF.37
	Paint cased opening including door jambs and two sides of casing with brush. Opening to be 3-0. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04802	E-WF.37
	Paint cased opening including door jambs and two sides of casing with brush. Opening to be 3-0. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04804	E-WF.37
	Paint cased opening including door jambs and two sides of casing with brush. Opening to be 6-0. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04805	E-WF.37
	Paint cased opening including door jambs and two sides of casing with brush. Opening to be 6-0. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04806	E-WF.37
	Stain and/or clear finish cased opening including door jambs and two sides of casing with brush. Opening to be 3-0. Application to be one coat with necessary clean-up and protection of items not to be painted.	
	
04807	E-WF.37
	Stain and/or clear finish cased opening including door jambs and two sides of casing with brush. Opening to be 3-0. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
04808	E-WF.37
	Stain and/or clear finish cased opening including door jambs and two sides of casing with brush. Opening to be 3-0. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
04809	E-WF.37
	Stain and/or clear finish cased opening including door jambs and two sides of casing with brush. Opening to be 6-0. Application to be one coat with necessary clean-up and protection of items not to be painted.	
	
04810	E-WF.37
	Stain and/or clear finish cased opening including door jambs and two sides of casing with brush. Opening to be 6-0. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
04811	E-WF.37
	Stain and/or clear finish cased opening including door jambs and two sides of casing with brush. Opening to be 6-0. Application to be three coats with necessary clean-up and protection of items not to be painted.	
	
04815	E-WF.37
	Paint open shelves, with no backing or vertical supports. Shelves to be painted top, bottom and edges with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04816	E-WF.37
	Paint open shelves, with no backing or vertical supports. Shelves to be painted top, bottom and edges with brush. Application to be prime and two coats with necessary clean-up and protection of items not to be painted.	
	
04817	E-WF.37
	Stain and/or clear finish open shelves, with no backing or vertical supports. Shelves to be stained top, bottom and edges with brush. Application to be one coat with necessary clean-up and protection of items not to be painted.	
	
04818	E-WF.37
	Stain and/or clear finish open shelves, with no backing or vertical supports. Shelves to be stained top, bottom and edges with brush. Application to be two coats with necessary clean-up and protection of items not to be painted.	
	
04819	E-WF.37
	Stain and/or clear finish open shelves, with no backing or vertical supports. Shelves to be stained top, bottom and edges with brush. Application to be three coats with necessary clean-up and protection of items not to be painted	
	
04820	E-WF.37
	Paint bookcase and all shelve sides with brush. Application to be primer and one coat with necessary clean-up and protection of items not to be painted.	
	
04821	E-WF.37
	Paint bookcase and all shelve sides with brush. Application to be primer and one coat with necessary clean-up and protection of items not to be painted.	
	
04822	E-WF.37
	Stain and/or clear finish bookcase or cabinet shelving 12" deep with brush. Application to be two coat with necessary clean-up and protection of items not to be painted.	
	
04823	E-WF.37
	Stain and/or clear finish bookcase or cabinet shelving 12" deep with brush. Application to be two coat with necessary clean-up and protection of items not to be painted.	
	
04824	E-WF.37
	Paint closet shelves, with no backing or vertical supports. Shelves to be painted top, bottom and edges with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
04825	E-WF.37
	Paint closet shelves, with no backing or vertical supports. Shelves to be painted top, bottom and edges with brush. Application to be prime and one coat with necessary clean-up and protection of items not to be painted.	
	
05222	E-WF.37
	Paint wood deck or porch floor on the top side with brush. Application to be prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05223	E-WF.37
	Paint wood deck or porch floor on the top side with brush. Application to be prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05225	E-WF.37
	Paint wood deck or porch floor on the top side with roller. Application to be prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05226	E-WF.37
	Paint wood deck or porch floor on the top side with roller. Application to be prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05228	E-WF.37
	Paint wood deck or porch floor on the top side with spray gun. Application to be prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05229	E-WF.37
	Paint wood deck or porch floor on the top side with spray gun. Application to be prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05230	E-WF.37
	Stain and/or clear finish wood deck or porch floor on the top side with brush. Application to be one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05231	E-WF.37
	Stain and/or clear finish wood deck or porch floor on the top side with brush. Application to be two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05232	E-WF.37
	Stain and/or clear finish wood deck or porch floor on the top side with brush. Application to be 3 coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05233	E-WF.37
	Stain and/or clear finish wood deck or porch floor on the top side with roller. Application to be one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05234	E-WF.37
	Stain and/or clear finish wood deck or porch floor on the top side with roller. Application to be two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05235	E-WF.37
	Stain and/or clear finish wood deck or porch floor on the top side with roller. Application to be 3 coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05236	E-WF.37
	Stain and/or clear finish wood deck or porch floor on the top side with spray gun. Application to be one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05237	E-WF.37
	Stain and/or clear finish wood deck or porch floor on the top side with spray gun. Application to be two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05238	E-WF.37
	Stain and/or clear finish wood deck or porch floor on the top side with spray gun. Application to be 3 coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05240	E-WF.37
	Paint wood porch ceiling with brush, prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05241	E-WF.37
	Paint wood porch ceiling with brush, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05243	E-WF.37
	Paint wood porch ceiling with roller, prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05244	E-WF.37
	Paint wood porch ceiling with roller, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05246	E-WF.37
	Paint wood porch ceiling with spray gun, prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05247	E-WF.37
	Paint wood porch ceiling with spray gun, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05300	E-WF.37
	Paint porch or deck railing with brush, one coat primer and one coat paint. Application to include necessary clean-up and protection of items not to be painted.	
	
05301	E-WF.37
	Paint porch or deck railing with brush, two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05302	E-WF.37
	Paint porch or deck railing with spraygun, one coat primer and one coat paint. Application to include necessary clean-up and protection of items not to be painted.	
	
05303	E-WF.37
	Paint porch or deck railing with spray gun, two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05304	E-WF.37
	Stain and/or clear finish porch or deck railing with brush, one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05305	E-WF.37
	Stain and/or clear finish porch or deck railing with brush, two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05306	E-WF.37
	Stain and/or clear finish porch or deck railing with brush, three coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05307	E-WF.37
	Stain and/or clear finish porch or deck railing with spray gun, one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05308	E-WF.37
	Stain and/or clear finish porch or deck railing with spray gun, two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05309	E-WF.37
	Stain and/or clear finish porch or deck railing with spray gun, three coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05311	E-WF.37
	Paint wood steps including all surfaces of steps and stringers with brush, prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05312	E-WF.37
	Paint wood steps including all surfaces of steps and stringers with brush, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05314	E-WF.37
	Paint wood steps including all surfaces of steps and stringers with spray gun, prime and one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05315	E-WF.37
	Paint wood steps including all surfaces of steps and stringers with spray gun, prime and two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05316	E-WF.37
	Stain and/or clear finish wood steps including all surfaces of steps and stringers with brush, one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05317	E-WF.37
	Stain and/or clear finish wood steps including all surfaces of steps and stringers with brush, two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05318	E-WF.37
	Stain and/or clear finish wood steps including all surfaces of steps and stringers with brush, three coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05319	E-WF.37
	Stain and/or clear finish wood steps including all surfaces of steps and stringers with spray gun, one coat. Application to include necessary clean-up and protection of items not to be painted.	
	
05320	E-WF.37
	Stain and/or clear finish wood steps including all surfaces of steps and stringers with spray gun, two coats. Application to include necessary clean-up and protection of items not to be painted.	
	
05321	E-WF.37
	Stain and/or clear finish wood steps including all surfaces of steps and stringers with spray gun, three coats. Application to include necessary clean-up and protection of items not to be painted.	
	
08900	E-WF.37
	Apply wallpaper as required to walls and/or ceiling up to 8' above floor. Wallpaper to be applied on prepared surface and have a retail cost of $11 per roll.	
	
08901	E-WF.37
	Apply wallpaper as required to walls and/or ceiling up to 8' above floor. Wallpaper to be applied on prepared surface and have a retail cost of $14 per roll.	
	
08902	E-WF.37
	Apply wallpaper as required to walls and/or ceiling up to 8' above floor. Wallpaper to be applied on prepared surface and have a retail cost of $17 per roll.	
	
08903	E-WF.37
	Apply wallpaper as required to walls and/or ceiling up to 8' above floor. Wallpaper to be applied on prepared surface and have a retail cost of $20 per roll.	
	
08904	E-WF.37
	Apply wallpaper as required to walls and/or ceiling up to 8' above floor. Wallpaper to be applied on prepared surface and have a retail cost of $25 per roll.	
	
08905	E-WF.37
	Apply wallpaper as required to walls and/or ceiling up to 8' above floor. Wallpaper to be applied on prepared surface and have a retail cost of $30 per roll.	
	
08906	E-WF.37
	Apply light duty vinyl wallpaper to walls and/or ceilings, with ceilings to be 8' above floor.	
	
08907	E-WF.37
	Apply medium duty vinyl wallpaper to walls and/or ceilings, with ceilings to be 8' above floor.	
	
08908	E-WF.37
	Apply heavy duty vinyl wallpaper to walls and/or ceilings, with ceilings to be 8' above floor.	
	
08909	E-WF.37
	Apply economy grade trimmed grass cloth wallpaper to walls and/or ceilings, with ceilings to be 8' above floor.	
	
08910	E-WF.37
	Apply medium grade trimmed grass cloth wallpaper to walls and/or ceilings, with ceilings to be 8' above floor.	
	
08911	E-WF.37
	Apply premium grade trimmed grass cloth wallpaper to walls and/or ceilings, with ceilings to be 8' above floor.	
	
08912	E-WF.37
	Apply premium grade trimmed grass cloth wallpaper to walls and/or ceilings, with ceilings to be 8' above floor.	
	
03000	E-WF.38
	Clean-up of demolition work to include the removal of debris, loading masonry, plaster, lumber and other tear-out material. Load truck by hand from the building and haul to a dumping site within five miles. Dumping fees not included.	
	
03001	E-WF.38
	Clean up trim and finish rubbish and broom clean site.	
	
03012	E-WF.38
	Clean-up of demolition work to include the removal of debris, loading masonry, plaster, lumber and other tear-out material. Load truck by chute from the building and haul to a dumping site within five miles. Dumping fees not included.	
	
03014	E-WF.38
	Clean-up deck to include removal of scrap lumber and tear-out debris. Clean-up to include hauling up to five miles but does not include dumping fees.	
	
04016	E-WF.38
	Maid service to take site cleaning from broom clean to complete cleaning of interior area that has been remodeling. Including windows inside and out, but does not include carpet or upholstery cleaning.	
	
04017	E-WF.38
	Maid service as above, the cost per square foot.	
	
04018	E-WF.38
	Maid service with additional work due to particularly difficult conditions the cost per square foot.	
	
04008	E-WF.39
	Install unfinished fir flooring that is 1" x 4" on prepared subsurface. Lay tongue and groove in matched oak flooring in such a pattern that all irregularities of room dimensions are absorbed in the outside walls. Nailing to be blind in all courses except the starter set. Installation does not include sanding or finishing.	
	
04009	E-WF.39
	Install unfinished pine flooring that is 1" x 4" on prepared subsurface. Lay tongue and groove in matched oak flooring in such a pattern that all irregularities of room dimensions are absorbed in the outside walls. Nailing to be blind in all courses except the starter set. Installation does not include sanding or finishing.	
	
04010	E-WF.39
	Install unfinished pine flooring that is 1" x 4" on prepared subsurface. Lay tongue and groove in matched oak flooring in such a pattern that all irregularities of room dimensions are absorbed in the outside walls. Nailing to be blind in all courses except the starter set. Installation does not include sanding or finishing.	
	
04050	E-WF.39
	Apply 5/8" x 4" planks to bottom of porch ceiling joists. Install fir beaded ceiling with center beaded on one side and center V-d on the other side. Includes ceiling cove moldings at wall intersections.	
	
04051	E-WF.39
	Apply 1 x 6 Redwood with V joint to bottom of porch ceiling joists. Installation to include ceiling cove moldings at wall intersections.	
	
04052	E-WF.39
	Apply 1 x 6 Knotty Pine with V joint to bottom of porch ceiling joists. Installation includes ceiling cove moldings at wall intersections.	
	
04053	E-WF.39
	Install 1x/4" fir porch flooring over existing porch floor joists. To be installed with galvanized nails.	
	
04054	E-WF.39
	Install trim over porch headers. Trim to be #2 Pine/Fir. Soffit to be 6" wide with two 12" fascias. All nails to be galvanized.	
	
04055	E-WF.39
	Install 4 x 4 posts to support porch.  Posts to be 8 foot in length.	
	
04056	E-WF.39
	Install 5 x 5 posts to support porch.  Posts to be 8 foot in length.	
	
04200	E-WF.39
	Install solid wood posts on existing footings up to 8' in length that are 4 x 4 pressure treated lumber. All deck framing will be installed with galvanized nails, hangers and other metal accessories.	
	
04201	E-WF.39
	Install solid wood posts on existing footings up to 8' in length that are 4 x 4 redwood lumber. All deck framing will be installed with galvanized nails, hangers and other metal accessories.	
	
04202	E-WF.39
	Install solid wood posts on existing footings up to 8' in length that are 6 x 6 pressure treated lumber. All deck framing will be installed with galvanized nails, hangers and other metal accessories.	
	
04205	E-WF.39
	Install solid or built-up wood beam or header on existing support. Beam to be 4 x 8 pressure treated lumber. All nails, hangers and other metal accessories to be galvanized.	
	
04206	E-WF.39
	Install solid or built-up wood beam or header on existing support. Beam to be 6 x 8 pressure treated lumber. All nails, hangers and other metal accessories to be galvanized.	
	
04207	E-WF.39
	Install solid or built-up wood beam or header on existing support. Beam to be 4 x 10 pressure treated lumber. All nails, hangers and other metal accessories to be galvanized.	
	
04208	E-WF.39
	Install solid or built-up wood beam or header on existing support. Beam to be 6 x 10 pressure treated lumber. All nails, hangers and other metal accessories to be galvanized.	
	
04210	E-WF.39
	Install solid or built-up wood beam or header on existing support. Beam to be 4 x 8 construction grade redwood lumber. All nails, hangers and other metal accessories to be galvanized.	
	
04211	E-WF.39
	Install solid or built-up wood beam or header on existing support. Beam to be 6 x 8 construction grade redwood lumber. All nails, hangers and other metal accessories to be galvanized.	
	
04212	E-WF.39
	Install solid or built-up wood beam or header on existing support. Beam to be 4 x 10 construction grade redwood lumber. All nails, hangers and other metal accessories to be galvanized.	
	
04213	E-WF.39
	Install solid or built-up wood beam or header on existing support. Beam to be 6 x 10 construction grade redwood lumber. All nails, hangers and other metal accessories to be galvanized.	
	
04214	E-WF.39
	Install header joist against building with 2 x 8 pressure treated lumber. Joist installed 16" OC. All perimeter joists to be doubled up. All nails and joist hangers to be galvanized.	
	
04215	E-WF.39
	Install header joist against building with 2 x 10 pressure treated lumber. Joist installed 24" OC. All perimeter joists to be doubled up. All nails and joist hangers to be galvanized.	
	
04220	E-WF.39
	Install header joist against building with 2 x 8 construction grade Redwood lumber. Joist installed 16" OC. All perimeter joists to be doubled up. All nails and joist hangers to be galvanized.	
	
04223	E-WF.39
	Install header joist against building with 2 x 8 construction grade Redwood lumber. Joist installed 24" OC. All perimeter joists to be doubled up. All nails and joist hangers to be galvanized.	
	
04300	E-WF.39
	Apply 2 x 6 pressure treated decking lumber over deck joists with 1/8" space between each course of lumber. All joints to be supported.	
	
04301	E-WF.39
	Apply 2 x 6 Construction Grade Redwood decking lumber over deck joists with 1/8" space between each course of lumber. All joints to be supported.	
	
04304	E-WF.39
	Install deck railing constructed of pressure treated lumber up to 3'6" high with 4 x 4 end and intermediate posts. Posts to be installed 6' OC with beveled 2 x 6 top rail and 2 x 4 middle and bottom rails. This design does not include pickets.	
	
04305	E-WF.39
	Install deck railing constructed of Construction Grade Redwood lumber up to 3'6" high with 4 x 4 end and intermediate posts. Posts to be installed 6' OC with beveled 2 x 6 top rail and 2 x 4 middle and bottom rails. This design does not include pickets.	
	
04306	E-WF.39
	Install deck railing constructed of Pressure Treated lumber up to 3'6" high with 4 x 4 end and intermediate posts. Posts to be installed 6' OC with beveled 2 x 4 top rail and 2 x 4 middle and bottom rails. Install 2 x 2 pickets 6" OC.	
	
04307	E-WF.39
	Install deck railing constructed of Construction Grade Redwood lumber up to 3'6" high with 4 x 4 end and intermediate posts. Posts to be installed 6' OC with beveled 2 x 4 top rail and 2 x 4 middle and bottom rails. Install 2 x 2 pickets 6" OC.	
	
04308	E-WF.39
	Install, using Pressure Treated lumber, three 2 x 6 rails fastened to 4 x 4 posts as required. Install 18" wide seat 18" above deck to be located below the 2 x 6 rails.	
	
04309	E-WF.39
	Install, using Construction Grade Redwood lumber, three 2 x 6 rails fastened to 4 x 4 posts as required. Install 18" wide seat 18" above deck to be located below the 2 x 6 rails.	
	
04310	E-WF.39
	Construct steps of Pressure Treated lumber up to 4 feet wide to two 2 x 12 stringers. Treads to be two 2 x 6 with open risers. Stringers to rest upon concrete or masonry, tread set at ground grade.	
	
04311	E-WF.39
	Construct steps of Construction Grade Redwood up to 4 feet wide to two 2 x 12 stringers. Treads to be two 2 x 6 with open risers. Stringers to rest upon concrete or masonry, tread set at ground grade.	
	
09201	E-WF.40
	Spread topsoil by wheelbarrow after dirt is dumped on premises in piles at a cost not to exceed $10 per cubic yard 6" deep.	
	
09204	E-WF.40
	Bluegrass sod, sodding by nursery personnel, 1 1/2" deep. Nursery to supply labor and material.	
	
10202	E-WF.40
	Rake out topsoil and spread seed by hand.	
	
10203	E-WF.40
	Rake out topsoil and spread seed by hand.	
	
